;****************************************************************************************************************
; File:     BDLDefaults.txt
; 
; Purpose:  Provides default labels and help IDs by BDL Command/Keyword for use
;           by BDL Object Creation mechanism.
;
; Format:   BDL Command, BDL Command Type, BDL Keyword, "Control Label",
;           Item Help ID, Topic Help ID, (currently unused additional help ID),
;           Misc Flag (decimal precision for numeric parameters & max nuber of 
;           characters for strings), Status Bar Message
;
;           Formatting Notes:    Max Label Length = 51 characters
; Bogus chars: ’
;****************************************************************************************************************

SCHEDULE,          1, TYPE,                                                    "Schedule Type", 31540, 32001, 0,  2, ""
SCHEDULE,          1, GROUP,                                                                "",     0, 32001, 0,  2, ""
SCHEDULE,          1, MONTH,                                                       "End Month", 31798, 32001, 0,  2, ""
SCHEDULE,          1, DAY,                                                           "End Day", 31799, 32001, 0,  2, ""
SCHEDULE,          1, WEEK-SCHEDULES,                                          "Week Schedule", 31797, 32001, 0,  2, ""
SCHEDULE,          2, TYPE,                                                    "Schedule Type", 31540, 32001, 0,  2, ""
SCHEDULE,          2, GROUP,                                                                "",     0, 32001, 0,  2, ""
SCHEDULE,          2, MONTH,                                                       "End Month", 31798, 32001, 0,  2, ""
SCHEDULE,          2, DAY,                                                           "End Day", 31799, 32001, 0,  2, ""
SCHEDULE,          2, WEEK-SCHEDULES,                                          "Week Schedule", 31797, 32001, 0,  2, ""
SCHEDULE,          3, TYPE,                                                    "Schedule Type", 31540, 32001, 0,  2, ""
SCHEDULE,          3, GROUP,                                                                "",     0, 32001, 0,  2, ""
SCHEDULE,          3, MONTH,                                                       "End Month", 31798, 32001, 0,  2, ""
SCHEDULE,          3, DAY,                                                           "End Day", 31799, 32001, 0,  2, ""
SCHEDULE,          3, WEEK-SCHEDULES,                                          "Week Schedule", 31797, 32001, 0,  2, ""
SCHEDULE,          4, TYPE,                                                    "Schedule Type", 31540, 32001, 0,  2, ""
SCHEDULE,          4, GROUP,                                                                "",     0, 32001, 0,  2, ""
SCHEDULE,          4, MONTH,                                                       "End Month", 31798, 32001, 0,  2, ""
SCHEDULE,          4, DAY,                                                           "End Day", 31799, 32001, 0,  2, ""
SCHEDULE,          4, WEEK-SCHEDULES,                                          "Week Schedule", 31797, 32001, 0,  2, ""
SCHEDULE,          5, TYPE,                                                    "Schedule Type", 31540, 32001, 0,  2, ""
SCHEDULE,          5, GROUP,                                                                "",     0, 32001, 0,  2, ""
SCHEDULE,          5, MONTH,                                                       "End Month", 31798, 32001, 0,  2, ""
SCHEDULE,          5, DAY,                                                           "End Day", 31799, 32001, 0,  2, ""
SCHEDULE,          5, WEEK-SCHEDULES,                                          "Week Schedule", 31797, 32001, 0,  2, ""
SCHEDULE,          6, TYPE,                                                    "Schedule Type", 31540, 32001, 0,  2, ""
SCHEDULE,          6, GROUP,                                                                "",     0, 32001, 0,  2, ""
SCHEDULE,          6, MONTH,                                                       "End Month", 31798, 32001, 0,  2, ""
SCHEDULE,          6, DAY,                                                           "End Day", 31799, 32001, 0,  2, ""
SCHEDULE,          6, WEEK-SCHEDULES,                                          "Week Schedule", 31797, 32001, 0,  2, ""
SCHEDULE,          7, TYPE,                                                    "Schedule Type", 31540, 32001, 0,  2, ""
SCHEDULE,          7, GROUP,                                                                "",     0, 32001, 0,  2, ""
SCHEDULE,          7, MONTH,                                                       "End Month", 31798, 32001, 0,  2, ""
SCHEDULE,          7, DAY,                                                           "End Day", 31799, 32001, 0,  2, ""
SCHEDULE,          7, WEEK-SCHEDULES,                                          "Week Schedule", 31797, 32001, 0,  2, ""
SCHEDULE,          8, TYPE,                                                    "Schedule Type", 31540, 32001, 0,  2, ""
SCHEDULE,          8, GROUP,                                                                "",     0, 32001, 0,  2, ""
SCHEDULE,          8, MONTH,                                                       "End Month", 31798, 32001, 0,  2, ""
SCHEDULE,          8, DAY,                                                           "End Day", 31799, 32001, 0,  2, ""
SCHEDULE,          8, WEEK-SCHEDULES,                                          "Week Schedule", 31797, 32001, 0,  2, ""
SCHEDULE,          9, TYPE,                                                    "Schedule Type", 31540, 32001, 0,  2, ""
SCHEDULE,          9, GROUP,                                                                "",     0, 32001, 0,  2, ""
SCHEDULE,          9, MONTH,                                                       "End Month", 31798, 32001, 0,  2, ""
SCHEDULE,          9, DAY,                                                           "End Day", 31799, 32001, 0,  2, ""
SCHEDULE,          9, WEEK-SCHEDULES,                                          "Week Schedule", 31797, 32001, 0,  2, ""
SCHEDULE,         10, TYPE,                                                    "Schedule Type", 31540, 32001, 0,  2, ""
SCHEDULE,         10, GROUP,                                                                "",     0, 32001, 0,  2, ""
SCHEDULE,         10, MONTH,                                                       "End Month", 31798, 32001, 0,  2, ""
SCHEDULE,         10, DAY,                                                           "End Day", 31799, 32001, 0,  2, ""
SCHEDULE,         10, WEEK-SCHEDULES,                                          "Week Schedule", 31797, 32001, 0,  2, ""
SCHEDULE,         11, TYPE,                                                    "Schedule Type", 31540, 32001, 0,  2, ""
SCHEDULE,         11, GROUP,                                                                "",     0, 32001, 0,  2, ""
SCHEDULE,         11, MONTH,                                                       "End Month", 31798, 32001, 0,  2, ""
SCHEDULE,         11, DAY,                                                           "End Day", 31799, 32001, 0,  2, ""
SCHEDULE,         11, WEEK-SCHEDULES,                                          "Week Schedule", 31797, 32001, 0,  2, ""
SCHEDULE,         12, TYPE,                                                    "Schedule Type", 31540, 32001, 0,  2, ""
SCHEDULE,         12, GROUP,                                                                "",     0, 32001, 0,  2, ""
SCHEDULE,         12, MONTH,                                                       "End Month", 31798, 32001, 0,  2, ""
SCHEDULE,         12, DAY,                                                           "End Day", 31799, 32001, 0,  2, ""
SCHEDULE,         12, WEEK-SCHEDULES,                                          "Week Schedule", 31797, 32001, 0,  2, ""
WEEK-SCHEDULE,     1, TYPE,                                               "Week Schedule Type", 31540, 32002, 0,  2, ""
WEEK-SCHEDULE,     1, DAY-SCHEDULES,   "Day Schedules 1) Weekdays/Design 2) Weekends/Holidays",  1838, 32002, 0,  2, ""
WEEK-SCHEDULE,     2, TYPE,                                               "Week Schedule Type", 31540, 32002, 0,  2, ""
WEEK-SCHEDULE,     2, DAY-SCHEDULES,   "Day Schedules 1) Weekdays/Design 2) Weekends/Holidays",  1838, 32002, 0,  2, ""
WEEK-SCHEDULE,     3, TYPE,                                               "Week Schedule Type", 31540, 32002, 0,  2, ""
WEEK-SCHEDULE,     3, DAY-SCHEDULES,   "Day Schedules 1) Weekdays/Design 2) Weekends/Holidays",  1838, 32002, 0,  2, ""
WEEK-SCHEDULE,     4, TYPE,                                               "Week Schedule Type", 31540, 32002, 0,  2, ""
WEEK-SCHEDULE,     4, DAY-SCHEDULES,   "Day Schedules 1) Weekdays/Design 2) Weekends/Holidays",  1838, 32002, 0,  2, ""
WEEK-SCHEDULE,     5, TYPE,                                               "Week Schedule Type", 31540, 32002, 0,  2, ""
WEEK-SCHEDULE,     5, DAY-SCHEDULES,   "Day Schedules 1) Weekdays/Design 2) Weekends/Holidays",  1838, 32002, 0,  2, ""
WEEK-SCHEDULE,     6, TYPE,                                               "Week Schedule Type", 31540, 32002, 0,  2, ""
WEEK-SCHEDULE,     6, DAY-SCHEDULES,   "Day Schedules 1) Weekdays/Design 2) Weekends/Holidays",  1838, 32002, 0,  2, ""
WEEK-SCHEDULE,     7, TYPE,                                               "Week Schedule Type", 31540, 32002, 0,  2, ""
WEEK-SCHEDULE,     7, DAY-SCHEDULES,   "Day Schedules 1) Weekdays/Design 2) Weekends/Holidays",  1838, 32002, 0,  2, ""
WEEK-SCHEDULE,     8, TYPE,                                               "Week Schedule Type", 31540, 32002, 0,  2, ""
WEEK-SCHEDULE,     8, DAY-SCHEDULES,   "Day Schedules 1) Weekdays/Design 2) Weekends/Holidays",  1838, 32002, 0,  2, ""
WEEK-SCHEDULE,     9, TYPE,                                               "Week Schedule Type", 31540, 32002, 0,  2, ""
WEEK-SCHEDULE,     9, DAY-SCHEDULES,   "Day Schedules 1) Weekdays/Design 2) Weekends/Holidays",  1838, 32002, 0,  2, ""
WEEK-SCHEDULE,    10, TYPE,                                               "Week Schedule Type", 31540, 32002, 0,  2, ""
WEEK-SCHEDULE,    10, DAY-SCHEDULES,   "Day Schedules 1) Weekdays/Design 2) Weekends/Holidays",  1838, 32002, 0,  2, ""
WEEK-SCHEDULE,    11, TYPE,                                               "Week Schedule Type", 31540, 32002, 0,  2, ""
WEEK-SCHEDULE,    11, DAY-SCHEDULES,   "Day Schedules 1) Weekdays/Design 2) Weekends/Holidays",  1838, 32002, 0,  2, ""
WEEK-SCHEDULE,    12, TYPE,                                               "Week Schedule Type", 31540, 32002, 0,  2, ""
WEEK-SCHEDULE,    12, DAY-SCHEDULES,   "Day Schedules 1) Weekdays/Design 2) Weekends/Holidays",  1838, 32002, 0,  2, ""
DAY-SCHEDULE,      1, TYPE,                                                "Day Schedule Type", 31540, 32003, 0,  2, "The type of day schedule (must be the same as parent week and annual schedules)"
DAY-SCHEDULE,      1, VALUES,                "Value for Midnight-1AM (default for entire day)", 31570, 32003, 0,  2, ""
DAY-SCHEDULE,      1, SCALE,                                                                "",     0, 32003, 0,  2, ""
DAY-SCHEDULE,      1, BIAS,                                                                 "",     0, 32003, 0,  2, ""
DAY-SCHEDULE,      2, TYPE,                                                "Day Schedule Type", 31540, 32003, 0,  2, "The type of day schedule (must be the same as parent week and annual schedules)"
DAY-SCHEDULE,      2, VALUES,                "Value for Midnight-1AM (default for entire day)", 31570, 32003, 0,  2, ""
DAY-SCHEDULE,      2, SCALE,                                                                "",     0, 32003, 0,  2, ""
DAY-SCHEDULE,      2, BIAS,                                                                 "",     0, 32003, 0,  2, ""
DAY-SCHEDULE,      3, TYPE,                                                "Day Schedule Type", 31540, 32003, 0,  2, "The type of day schedule (must be the same as parent week and annual schedules)"
DAY-SCHEDULE,      3, VALUES,                "Value for Midnight-1AM (default for entire day)", 31570, 32003, 0,  2, ""
DAY-SCHEDULE,      3, SCALE,                                                                "",     0, 32003, 0,  2, ""
DAY-SCHEDULE,      3, BIAS,                                                                 "",     0, 32003, 0,  2, ""
DAY-SCHEDULE,      4, TYPE,                                                "Day Schedule Type", 31540, 32003, 0,  2, "The type of day schedule (must be the same as parent week and annual schedules)"
DAY-SCHEDULE,      4, VALUES,                "Value for Midnight-1AM (default for entire day)", 31570, 32003, 0,  2, ""
DAY-SCHEDULE,      4, SCALE,                                                                "",     0, 32003, 0,  2, ""
DAY-SCHEDULE,      4, BIAS,                                                                 "",     0, 32003, 0,  2, ""
DAY-SCHEDULE,      5, TYPE,                                                "Day Schedule Type", 31540, 32003, 0,  2, "The type of day schedule (must be the same as parent week and annual schedules)"
DAY-SCHEDULE,      5, VALUES,                "Value for Midnight-1AM (default for entire day)", 31570, 32003, 0,  2, ""
DAY-SCHEDULE,      5, SCALE,                                                                "",     0, 32003, 0,  2, ""
DAY-SCHEDULE,      5, BIAS,                                                                 "",     0, 32003, 0,  2, ""
DAY-SCHEDULE,      6, TYPE,                                                "Day Schedule Type", 31540, 32003, 0,  2, "The type of day schedule (must be the same as parent week and annual schedules)"
DAY-SCHEDULE,      6, VALUES,                "Value for Midnight-1AM (default for entire day)", 31570, 32003, 0,  2, ""
DAY-SCHEDULE,      6, SCALE,                                                                "",     0, 32003, 0,  2, ""
DAY-SCHEDULE,      6, BIAS,                                                                 "",     0, 32003, 0,  2, ""
DAY-SCHEDULE,      7, TYPE,                                                "Day Schedule Type", 31540, 32003, 0,  2, "The type of day schedule (must be the same as parent week and annual schedules)"
DAY-SCHEDULE,      7, VALUES,                "Value for Midnight-1AM (default for entire day)", 31570, 32003, 0,  2, ""
DAY-SCHEDULE,      7, SCALE,                                                                "",     0, 32003, 0,  2, ""
DAY-SCHEDULE,      7, BIAS,                                                                 "",     0, 32003, 0,  2, ""
DAY-SCHEDULE,      8, TYPE,                                                "Day Schedule Type", 31540, 32003, 0,  2, "The type of day schedule (must be the same as parent week and annual schedules)"
DAY-SCHEDULE,      8, VALUES,                "Value for Midnight-1AM (default for entire day)", 31570, 32003, 0,  2, ""
DAY-SCHEDULE,      8, SCALE,                                                                "",     0, 32003, 0,  2, ""
DAY-SCHEDULE,      8, BIAS,                                                                 "",     0, 32003, 0,  2, ""
DAY-SCHEDULE,      9, TYPE,                                                "Day Schedule Type", 31540, 32003, 0,  2, "The type of day schedule (must be the same as parent week and annual schedules)"
DAY-SCHEDULE,      9, VALUES,                "Value for Midnight-1AM (default for entire day)", 31570, 32003, 0,  2, ""
DAY-SCHEDULE,      9, SCALE,                                                                "",     0, 32003, 0,  2, ""
DAY-SCHEDULE,      9, BIAS,                                                                 "",     0, 32003, 0,  2, ""
DAY-SCHEDULE,     10, TYPE,                                                "Day Schedule Type", 31540, 32003, 0,  2, "The type of day schedule (must be the same as parent week and annual schedules)"
DAY-SCHEDULE,     10, VALUES,                "Value for Midnight-1AM (default for entire day)", 31570, 32003, 0,  2, ""
DAY-SCHEDULE,     10, SCALE,                                                                "",     0, 32003, 0,  2, ""
DAY-SCHEDULE,     10, BIAS,                                                                 "",     0, 32003, 0,  2, ""
DAY-SCHEDULE,     11, TYPE,                                                "Day Schedule Type", 31540, 32003, 0,  2, "The type of day schedule (must be the same as parent week and annual schedules)"
DAY-SCHEDULE,     11, OUTSIDE-HI,                           "Outdoor DryBulb High Temperature", 31541, 32003, 0,  2, "The outside drybulb air temp that corresponds to the lower supply air set-point temperature"
DAY-SCHEDULE,     11, OUTSIDE-LO,                            "Outdoor DryBulb Low Temperature", 31541, 32003, 0,  2, "The outside drybulb air temp that corresponds to the upper supply air set-point temperature"
DAY-SCHEDULE,     11, SUPPLY-HI,                        "Equipment Temperature at Outdoor Low", 31544, 32003, 0,  2, "The upper supply air set-point temp that corresponds to the Outside Drybulb Temp Low"
DAY-SCHEDULE,     11, SUPPLY-LO,                       "Equipment Temperature at Outdoor High", 31544, 32003, 0,  2, "The lower supply air set-point temp that corresponds to the Outside Drybulb Temp High"
DAY-SCHEDULE,     11, DAY-HOURS,                                                   "DAY-HOURS", 31545, 32003, 0,  2, "First and last hour of the day for which the Primary reset parameters are used"
DAY-SCHEDULE,     11, OUTSIDE-HI2,                                               "OUTSIDE-HI2", 31541, 32003, 0,  2, "The outside drybulb air temp that corresponds to the lower supply air set-point temperature"
DAY-SCHEDULE,     11, OUTSIDE-LO2,                                               "OUTSIDE-LO2", 31541, 32003, 0,  2, "The outside drybulb air temp that corresponds to the upper supply air set-point temperature"
DAY-SCHEDULE,     11, SUPPLY-HI2,                                                 "SUPPLY-HI2", 31544, 32003, 0,  2, "The upper supply air set-point temp that corresponds to the Outside Drybulb Temp Low"
DAY-SCHEDULE,     11, SUPPLY-LO2,                                                 "SUPPLY-LO2", 31544, 32003, 0,  2, "The lower supply air set-point temp that corresponds to the Outside Drybulb Temp High"
DAY-SCHEDULE,     12, TYPE,                                                "Day Schedule Type", 31540, 32003, 0,  2, "The type of day schedule (must be the same as parent week and annual schedules)"
DAY-SCHEDULE,     12, OUTSIDE-HI,                              "Outdoor DryBulb High Setpoint", 31541, 32003, 0,  2, "The outside drybulb air temp that corresponds to the lower supply air set-point temperature"
DAY-SCHEDULE,     12, OUTSIDE-LO,                               "Outdoor DryBulb Low Setpoint", 31541, 32003, 0,  2, "The outside drybulb air temp that corresponds to the upper supply air set-point temperature"
DAY-SCHEDULE,     12, SUPPLY-HI,                  "Equipment Fractional Output at Outdoor Low", 31544, 32003, 0,  2, "The upper supply air set-point temp that corresponds to the Outside Drybulb Temp Low"
DAY-SCHEDULE,     12, SUPPLY-LO,                 "Equipment Fractional Output at Outdoor High", 31544, 32003, 0,  2, "The lower supply air set-point temp that corresponds to the Outside Drybulb Temp High"
DAY-SCHEDULE,     12, DAY-HOURS,                                                   "DAY-HOURS", 31545, 32003, 0,  2, "First and last hour of the day for which the Primary reset parameters are used"
DAY-SCHEDULE,     12, OUTSIDE-HI2,                                               "OUTSIDE-HI2", 31541, 32003, 0,  2, "The outside drybulb air temp that corresponds to the lower supply air set-point temperature"
DAY-SCHEDULE,     12, OUTSIDE-LO2,                                               "OUTSIDE-LO2", 31541, 32003, 0,  2, "The outside drybulb air temp that corresponds to the upper supply air set-point temperature"
DAY-SCHEDULE,     12, SUPPLY-HI2,                                                 "SUPPLY-HI2", 31544, 32003, 0,  2, "The upper supply air set-point temp that corresponds to the Outside Drybulb Temp Low"
DAY-SCHEDULE,     12, SUPPLY-LO2,                                                 "SUPPLY-LO2", 31544, 32003, 0,  2, "The lower supply air set-point temp that corresponds to the Outside Drybulb Temp High"
SITE-PARAMETERS,   0, LATITUDE,                                                     "Latitude", 12504,   758, 0,  2, "Building site latitude - northern hemishpere is positive"
SITE-PARAMETERS,   0, LONGITUDE,                                                   "Longitude", 12505,   758, 0,  2, "Building site longitude - degrees from the prime meridian, west (+) or east (-)"
SITE-PARAMETERS,   0, TIME-ZONE,                                                   "Time Zone", 12506, 32004, 0,  0, "Building site time zone - number of time zones west (+) or east (-) of the prime meridian"
SITE-PARAMETERS,   0, ALTITUDE,                                                     "Altitude", 12535,   788, 0,  0, "Building site altitude above mean sea level, used to adjust air quantities"
SITE-PARAMETERS,   0, DAYLIGHT-SAVINGS,                                                     "", 12534, 32004, 0,  0, "Is daylight savings observed? (Yes/No)"
SITE-PARAMETERS,   0, GROUND-T,                                                             "",   811, 32004, 0,  2, "Mean monthly ground temperature"
SITE-PARAMETERS,   0, CLEARNESS-NUMBER,                                                     "", 63059, 32004, 0,  2, "Empirical constant used in ASHRAE clear sky calculation (atmospheric transmissivity)"
SITE-PARAMETERS,   0, ATM-MOISTURE,                                                         "", 63060,   758, 0,  2, "Number of inches of precipitable moisture in the atmosphere (monthly averages)"
SITE-PARAMETERS,   0, ATM-TURBIDITY,                                                        "", 63061, 32004, 0,  2, "A measure of the amount of aerosols or particulates in the atmosphere (monthly averages)"
SITE-PARAMETERS,   0, SHIELDING-COEF,                                  "Shielding Coefficient", 12536,   773, 0,  0, "In the S-G infiltration method, modifies the wind speed to account for local obstructions"
SITE-PARAMETERS,   0, TERRAIN-PAR1,                                      "Terrain Parameter 1", 12537,   773, 0,  0, "Building site terrain parameter; used to convert wind speed from weather station conditions"
SITE-PARAMETERS,   0, TERRAIN-PAR2,                                      "Terrain Parameter 2", 12538,   773, 0,  0, "Building site terrain parameter; used to convert wind speed from weather station conditions"
SITE-PARAMETERS,   0, WS-TERRAIN-PAR1,                                 "Weather Station Par 1", 12539,   773, 0,  0, "Weather station terrain parameter; used to convert wind speed from weather station conditions."
SITE-PARAMETERS,   0, WS-TERRAIN-PAR2,                                 "Weather Station Par 2", 12540,   773, 0,  0, "Weather station terrain parameter; used to convert wind speed from weather station conditions."
SITE-PARAMETERS,   0, WS-HEIGHT,                                      "Weather Station Height", 12541,   773, 0,  0, "Height above ground at which wind speed data were recorded"
SITE-PARAMETERS,   0, WS-HEIGHT-LIST,                                                       "", 11504,   773, 0,  2, "Height above ground at which wind speed data were recorded (monthly values)"
BUILDING-SHADE,    0, TRANSMITTANCE,                                           "Transmittance", 12560, 32005, 0,  0, "Fraction of the incident (direct) solar radiation that passes through the Building Shade"
BUILDING-SHADE,    0, SHADE-SCHEDULE,                                               "Schedule",   679,   679, 0,  0, "Fraction Schedule: transmittance of direct (beam) solar radiation for the Building Shade"
BUILDING-SHADE,    0, SHADE-VIS-REFL,                                    "Visible Reflectance", 12561,  3006, 0,  0, "Visible light reflectance of the side of the Building Shade from which its outward normal points"
BUILDING-SHADE,    0, SHADE-GND-REFL,                                     "Ground Reflectance", 12562, 32005, 0,  0, "The visible light reflectance of the ground near the Building Shade"
BUILDING-SHADE,    0, X,                                                                   "X", 19080,   788, 0,  1, "X coordinate for the shade origin (relative to the Building coordinate system)"
BUILDING-SHADE,    0, Y,                                                                   "Y", 19081,   788, 0,  1, "Y coordinate for the shade origin (relative to the Building coordinate system)"
BUILDING-SHADE,    0, Z,                                                                   "Z", 19082,   788, 0,  1, "Z coordinate for the shade origin (relative to the Building coordinate system)"
BUILDING-SHADE,    0, HEIGHT,                                                         "Height", 19083, 32005, 0,  1, "Height of the shade (measured parallel to the Building z-axis)."
BUILDING-SHADE,    0, WIDTH,                                                           "Width", 19084, 32005, 0,  1, "Width of the shade (measured parallel to the Building x-axis)."
BUILDING-SHADE,    0, AZIMUTH,                                                       "Azimuth", 19085,   788, 0,  1, "Azimuth of surface outward normal relative to Biulding Y-axis (positive = clockwise rotation)"
BUILDING-SHADE,    0, TILT,                                                             "Tilt", 19087, 32005, 0,  2, "Tilt of the surface outward normal, relative to the Building Z-axis (+ for clockwise rotation)"
BUILDING-SHADE,    0, SHADE-DIF-REFL,                                                       "",     0, 32005, 0,  0, ""
BUILDING-SHADE,    0, SHADE-SPEC-REFL,                                                      "",     0, 32005, 0,  0, ""
BUILDING-SHADE,    0, SHADE-REFL-ROUGH,                                                     "",     0, 32005, 0,  0, ""
CONSTRUCTION,      0, TYPE,                                                             "Type", 14469, 32006, 0,  0, "Whether you define all of the Layers (& Materials) in the wall, or just its overall parameters"
CONSTRUCTION,      0, ABSORPTANCE,                                               "Absorptance", 12093, 32006, 0,  3, "Fraction of incident solar radiation absorbed by the exterior finish of this construction"
CONSTRUCTION,      0, ROUGHNESS,                                                   "Roughness", 12092, 32006, 0,  0, "Roughness of the exterior finish of this construction (1=roughest,  6=smoothest)"
CONSTRUCTION,      0, WALL-PARAMETERS,                                                      "",     0,   753, 0,  2, ""
CONSTRUCTION,      0, U-VALUE,                                               "Overall U-Value", 12091, 32006, 0,  3, "Overall thermal conductance of this construction (less exterior film resistance)"
CONSTRUCTION,      0, LAYERS,                                                         "Layers", 19017, 32006, 0,  0, "Name of the construction of this wall (alternative to U-Value)"
CONSTRUCTION,      0, PICTURE,                                                              "",     0, 32006, 0,  2, ""
CONSTRUCTION,      0, DRAWING,                                                              "",     0, 32006, 0,  2, ""
GLASS-TYPE,        0, TYPE,                                                             "Type", 14280, 32007, 0,  0, "The type of layer (Glass, Gap or Blind)"
GLASS-TYPE,        0, GLASS-TYPE-CODE,                                       "Glass Type Code", 13131,   760, 0, 32, "Glass type code selected from library for this glass type"
GLASS-TYPE,        0, SHADING-COEF,                                      "Shading Coefficient", 13132,   759, 0,  2, "Amount of solar radiation that the window transmits (relative to standard glass)"
GLASS-TYPE,        0, GLASS-CONDUCT,                                       "Glass Conductance", 13133, 32007, 0,  2, "Glass thermal conductance (gls only or gls+frame, less ext. film res.)"
GLASS-TYPE,        0, VIS-TRANS,                                       "Visible Transmittance", 13146,  3006, 0,  2, "Fraction of visible daylight that is transmitted through the glass (at normal incidence)"
GLASS-TYPE,        0, OUTSIDE-EMISS,                                      "Outside Emissivity", 13135, 32007, 0,  2, "Infrared (IR) emissivity of the exterior finish of this glass type"
GLASS-TYPE,        0, PICTURE,                                                              "",     0, 32007, 0,  2, ""
GLASS-TYPE,        0, DRAWING,                                                              "",     0, 32007, 0,  2, ""
SPACE,             0, X,                                                                   "X", 19000,   756, 0,  2, "X coordinate for the space origin (relative to the Building coordinate system)"
SPACE,             0, Y,                                                                   "Y", 19001,   756, 0,  2, "Y coordinate for the space origin (relative to the Building coordinate system)"
SPACE,             0, Z,                                                                   "Z", 19002,   756, 0,  2, "Z coordinate for the space origin (relative to the Building coordinate system)"
SPACE,             0, AZIMUTH,                                                       "Azimuth", 19003,   756, 0,  2, "Azimuth of Space Y-axis relative to Biulding Y-axis (positive = clockwise rotation)"
SPACE,             0, HEIGHT,                                                   "Space Height", 19016, 32008, 0,  2, "Height of space: used only, and required, if the space is defined with either Shape or Polygon"
SPACE,             0, AREA,                                                       "Space Area", 12004, 32008, 0,  1, "Floor area of this space (before multiplication by Multiplier or Floor Multiplier)"
SPACE,             0, VOLUME,                                                   "Space Volume", 12005, 32008, 0,  1, "Air volume of this space (before multiplication by Multiplier or Floor Multiplier)"
SPACE,             0, MULTIPLIER,                                           "Space Multiplier", 12002,   769, 0,  0, "Number of identical spaces (includes heat transfer through interior surfaces, if any)"
SPACE,             0, SHAPE,                                  "Space Shape Description Method", 19004,   755, 0,  0, "An alternative, simplified method to specify space geometry (Shape) in plan view"
SPACE,             0, WIDTH,                                                     "Space Width", 19006, 32008, 0,  2, "If SHAPE is used,  this is the depth of the space (measured parallel to the Space y-axis)."
SPACE,             0, DEPTH,                                                     "Space Depth", 19005, 32008, 0,  2, "Applies (& required) only if the space is defined via Shape"
SPACE,             0, SPACE-CONDITIONS,                                                     "", 10029, 32008, 0,  2, ""
SPACE,             0, FLOOR-WEIGHT,                                             "Floor Weight", 12031,   799, 0,  0, "Total weight of interior furnishings and surrounding surfaces of a space per unit floor area"
SPACE,             0, FURNITURE-TYPE,                                         "Furniture Type", 12033,   799, 0,  0, "Furniture type (Light is approx 40 lb/cubic ft; Heavy is approx 80 lb/cubic ft)"
SPACE,             0, FURN-FRACTION,             "Fraction of Floor Area Covered by Furniture", 12034,   799, 0,  2, "The fraction of floor area covered by furniture"
SPACE,             0, WEIGHTING-FACTOR,                                     "Weighting Factor", 12032,   799, 0,  0, "Name of user-calculated weighting factors to be stored in or recalled from the library"
SPACE,             0, ZONE-TYPE,                                                   "Zone Type", 12263, 32008, 0,  0, "Type of zone (i.e., conditioned, unconditioned, plenum)"
SPACE,             0, TEMPERATURE,                                    "Loads Calc Temperature", 12022,   752, 0,  1, "Annual average space T: normally set this to midpoint of Heating & Cooling Design T's"
SPACE,             0, PEOPLE-SCHEDULE,                                    "Occupancy Schedule", 12067, 32008, 0,  0, "Name of the schedule that governs occupancy in the selected space"
SPACE,             0, LIGHTING-SCHEDUL,                                    "Lighting Schedule", 62013, 32084, 0,  0, "A fractional schedule that adjusts the lighting subsystem's power consumption each hour"
SPACE,             0, TASK-LIGHT-SCH,                                 "Task Lighting Schedule", 13581, 32008, 0,  2, "Schedule of operation for all the task lights in the space (schedule type should be Fraction)"
SPACE,             0, EQUIP-SCHEDULE,                                     "Equipment Schedule", 12070, 32008, 0,  0, "Name of schedule that controls the equipment energy use in the selected zone"
SPACE,             0, SOURCE-SCHEDULE,                                       "Source Schedule",   726,   726, 0,  0, "Schedule that controls the source energy use in the selected space"
SPACE,             0, INF-SCHEDULE,                                    "Infiltration Schedule", 12037, 32008, 0,  0, "A Fraction Schedule that modifies the rate of air infiltration into the space"
SPACE,             0, LIGHTING-TYPE,                                                        "", 62014, 32084, 0,  0, "Defines distribution of heat from lights; to return air, radiative/convective fractions, etc."
SPACE,             0, SOURCE-TYPE,                                               "Source Type",   725,   725, 0,  0, "Type of source energy use in the selected space"
SPACE,             0, SOURCE-POWER,                                             "Source Power",   724,   724, 0,  2, "Total source input power for the selected space"
SPACE,             0, SOURCE-BTU/HR,                                      "Source Input Power",   724,   724, 0,  2, "Total source input power for the selected space"
SPACE,             0, INF-METHOD,                                        "Infiltration Method", 12036, 32008, 0,  0, "The method PowerDOE uses to calculate the rate of outside air infiltration into the space"
SPACE,             0, AIR-CHANGES/HR,                                       "Air Changes/Hour", 12038, 32008, 0,  1, "Number of air changes per hour due to infiltration into the zone, at a wind speed of 10 mph"
SPACE,             0, INF-FLOW/AREA,                                       "Infiltration Flow", 12039, 32008, 0,  2, "Outside air infiltration rate into the space per unit floor Area"
SPACE,             0, INF-CFM/SQFT,                                        "Infiltration Flow", 12039, 32008, 0,  2, "Outside air infiltration rate into the space per unit floor Area"
SPACE,             0, NEUTRAL-ZONE-HT,                                   "Neutral Zone Height", 12040,   773, 0,  2, "Vertical distance between each zone and the neutral pressure level of the building"
SPACE,             0, PEOPLE-HG-LAT,                                 "People Latent Heat Gain", 12068, 32008, 0,  0, "Latent heat gain per occupant in the selected space"
SPACE,             0, PEOPLE-HG-SENS,                              "People Sensible Heat Gain", 12069, 32008, 0,  0, "Sensible heat gain per occupant in the selected space"
SPACE,             0, LIGHTING-KW,                                    "Lighting System Power ", 62015, 32084, 0,  2, "Maximum amount of power consumed by the overhead lighting subsystem"
SPACE,             0, LIGHT-TO-SPACE,                    "Fraction of Light Heat (This Space)", 13573,   772, 0,  2, "Fraction of the lighting power consumption that appears in the space as heat"
SPACE,             0, TASK-LIGHTING-KW,                                                "Power", 13580, 32084, 0,  2, "Maximum energy consumption of task lighting"
SPACE,             0, EQUIPMENT-KW,                             "Equipment Total Input Power ", 12072, 32008, 0,  2, "Total equipment input power for the selected space (an alternative to Input Power Density)"
SPACE,             0, EQUIP-LATENT,                          "Equipment Power Latent Portion ", 12073, 32008, 0,  2, "Fraction of Equipment Power Input released to the space as latent heat"
SPACE,             0, EQUIP-SENSIBLE,                      "Equipment Power Sensible Portion ",   727,   722, 0,  2, "Fraction of Equipment Power Input released to the space as sensible heat"
SPACE,             0, SOURCE-LATENT,                                           "Source Latent",   723, 32008, 0,  2, "Fraction of source power input in the selected space that is sensible"
SPACE,             0, SOURCE-SENSIBLE,                                       "Source Sensible",   722, 32008, 0,  2, "Fraction of source power input in the selected space that is sensible"
SPACE,             0, NUMBER-OF-PEOPLE,                                     "Number of People", 12064, 32008, 0,  0, "Maximum number of people in the space"
SPACE,             0, PEOPLE-HEAT-GAIN,                                      "Total Heat Gain", 12066, 32008, 0,  0, "Total (sensible plus latent) heat gain per occupant in the selected space"
SPACE,             0, RES-INF-CST,                  "Resid. Infiltration Constant Coefficient",   674,   674, 0,  2, "Used to calculate outside air infiltration into the space (based on wind speed & temperature)"
SPACE,             0, RES-INF-WND,                "Resid. Infiltration Wind Speed Coefficient",   672,   672, 0,  2, "Used to calculate outside air infiltration into the space (based on wind speed & temperature)"
SPACE,             0, RES-INF-TEMP,              "Resid. Infiltration Temperature Coefficient",   673,   673, 0,  2, "Used to calculate outside air infiltration into the space (based on wind speed & temperature)"
SPACE,             0, RES-INF-COEF,                          "Resid. Infiltration Coefficient", 12044, 32008, 0,  1, "Used to calculate outside air infiltration into the space (based on wind speed & temperature)"
SPACE,             0, LIGHTING-W/AREA,                               "Lighting Power Density ", 12028, 32084, 0,  2, "Max power consumption of main overhead lights in zone, per square foot of floor area"
SPACE,             0, TASK-LT-W/AREA,                                          "Power Density", 13579, 32084, 0,  2, "Maximum energy consumption of task lighting, per square feet of space floor area"
SPACE,             0, EQUIPMENT-W/AREA,                                 "Input Power Density ", 12071, 32008, 0,  1, "Equipment input power density for the selected space (an alternative to Input Power)"
SPACE,             0, FURN-WEIGHT,                                       "Weight of Furniture", 12035,   799, 0,  0, "The weight of the furniture per unit floor area"
SPACE,             0, DAYLIGHTING,                                               "Daylighting", 12048,  3006, 0,  0, "Whether Daylighting is used to offset lighting power consumption in this zone"
SPACE,             0, LIGHT-REF-POINT1,  "X,Y (1,2) Location of Sensor for 1st Lighting Zone ", 13821,  3006, 0,  2, "The desired illuminance level for the first Daylit zone in the space is calculated at this point"
SPACE,             0, LIGHT-REF-POINT2,  "X,Y (1,2) Location of Sensor for 2nd Lighting Zone ", 13837,  3006, 0,  2, "Desired illuminance level for the second Daylit zone in the space is calculated at this point"
SPACE,             0, ZONE-FRACTION1,            "Fraction of SPACE Area of 1st Lighting Zone", 12049,  3006, 0,  2, "Fraction of floor area in the selected space controlled by Lighting Reference Point 1"
SPACE,             0, ZONE-FRACTION2,            "Fraction of SPACE Area of 2nd Lighting Zone", 12050,  3006, 0,  2, "Fraction of floor area in the selected space controlled by Lighting Reference Point 2"
SPACE,             0, LIGHT-SET-POINT1,           "Controller Set Point for 1st Lighting Zone", 12051,  3006, 0,  0, "Desired lighting level at Lighting Ref Point 1 (that Daylighting controls attempt to maintain)"
SPACE,             0, LIGHT-SET-POINT2,           "Controller Set Point for 2nd Lighting Zone", 12052,  3006, 0,  0, "Desired lighting level at Lighting Ref Point 2 (that Daylighting controls attempt to maintain)"
SPACE,             0, LIGHT-CTRL-TYPE1,      "Lighting  Controller Type for 1st Lighting Zone", 12053,  3006, 0,  0, "Lighting controller type for lights in Zone Fraction 1"
SPACE,             0, LIGHT-CTRL-TYPE2,      "Lighting  Controller Type for 2nd Lighting Zone", 12054,  3006, 0,  0, "Lighting controller type for lights in Zone Fraction 2"
SPACE,             0, VIEW-AZIMUTH,                                                         "", 63035,   762, 0,  2, "Direction of the occupant's view (in horizontal plane) in which the daylight glare is calculated"
SPACE,             0, MAX-GLARE,                                               "Maximum Glare", 12055,   762, 0,  0, "Maximum tolerable glare before glare control shading devices are deployed"
SPACE,             0, MIN-POWER-FRAC,                                 "Minimum Power Fraction", 12056,  3006, 0,  2, "The minimum input power required by a continuous dimming lighting controller"
SPACE,             0, MIN-LIGHT-FRAC,                                 "Minimum Light Fraction", 12057,  3006, 0,  2, "The minimum light output achieved by a continuous dimming lighting controller"
SPACE,             0, LIGHT-CTRL-STEPS,                                  "Light Control Steps", 12058,  3006, 0,  0, "The number of steps in a stepped lighting control system (excluding the off state)"
SPACE,             0, LIGHT-OUT-FP,                                                         "",     0, 32008, 0,  2, ""
SPACE,             0, LIGHT-CTRL-PROB,                             "Light Control Probability", 12060,  3006, 0,  2, "Probability of manually switched lights being correctly switched in response to daylight levels"
SPACE,             0, DAYLIGHT-REP-SCH,                          "Daylighting Report Schedule", 12061,  3006, 0,  0, "An On-Off Schedule that indicates which hours are included in the daylighting reports"
SPACE,             0, HOR-LEAK-FRAC,                                   "Horizontal Leak Ratio", 12045,   773, 0,  2, "Fraction of the total leakage area that is in the ceiling"
SPACE,             0, NEUTRAL-LEVEL,                                           "Neutral Level", 12046,   773, 0,  2, "Fraction of zone height at which the indoor air pressure equals the outdoor air pressure"
SPACE,             0, FRAC-LEAK-AREA,                            "Leak Fraction of Floor Area", 12047,   773, 0,  2, "Total leakage area (expressed as a fraction of the floor area of the space)"
SPACE,             0, LIGHT-TO-OTHER,                "Fraction of Light Heat (Adjusted Space)", 13574,   772, 0,  2, "Fraction of the lighting power consumption that appears in an adjacent space as heat"
SPACE,             0, LIGHT-TO-RETURN,                   "Fraction of Light Heat (Return Air)", 13575,   772, 0,  2, "Fraction of lighting power consumption that appears in the return air stream space as heat"
SPACE,             0, LIGHT-HEAT-TO,                       "Adjacent Space Light Heat Goes To", 13578,   772, 0,  0, "An adjacent space that receives the Fraction of Light Heat to Adjacent Space"
SPACE,             0, LIGHT-RAD-FRAC,                       "Lighting System Radiant Fraction", 13576,   771, 0,  2, "The fraction of heat (from lights) in the space that is radiative (the remainder is convective)"
SPACE,             0, LUM-SPACE-DIV,                                                        "", 13582, 32008, 0,  2, "The space is divided into this number identical rooms for the lighting calculations"
SPACE,             0, FLOOR-MULTIPLIER,                                                     "", 12422,   769, 0,  2, "Number of floors in the facility that are identical, and served by the same HVAC system"
SPACE,             0, SUNSPACE,                                                     "Sunspace", 12021,   753, 0,  0, "Sunspaces allow more detailed calculations of heat transfer with other spaces"
SPACE,             0, AREA/PERSON,                                               "Area/Person", 12065, 32008, 0,  0, "Maximum occupancy density (expressed as area per person in the selected space)"
SPACE,             0, FUNCTION,                                                             "",     0, 32008, 0,  2, ""
SPACE,             0, DAYL-ILLUM-FN,                                                        "",     0,  3006, 0,  2, ""
SPACE,             0, DAYL-LTCTRL-FN,                                                       "",     0,  3006, 0,  2, ""
SPACE,             0, EXTERIOR-WALLS,                                                       "",     0, 32008, 0,  2, ""
SPACE,             0, ROOFS,                                                                "",     0, 32008, 0,  2, ""
SPACE,             0, TROMBE-WALL-NV,                                                       "",     0, 32008, 0,  2, ""
SPACE,             0, TROMBE-WALL-V,                                                        "",     0, 32008, 0,  2, ""
SPACE,             0, INTERIOR-WALLS,                                                       "",     0, 32008, 0,  2, ""
SPACE,             0, UNDERGROUND-WALL,                                                     "",     0, 32008, 0,  2, ""
SPACE,             0, UNDERGROUND-FLOO,                                                     "",     0, 32008, 0,  2, ""
SPACE,             0, POLYGON,                            "Polygon that Describes Space Shape", 19020, 31030, 0,  0, "Name of the Polygon that defines the space's floor geometry"
SPACE,             0, LIGHTING-SYSTEM,                                "Space Lighting System ", 13584, 32084, 0,  2, ""
SPACE,             0, NO-OF-LUMINAIRES,             "Number of Luminaires in Lighting System ", 62019, 32008, 0,  2, "No. of luminaires in the lighting subsystem, of the type defined by the chosen Lighting System"
SPACE,             0, CEIL-TO-LUM-DIS,                                                      "", 62017, 32008, 0,  2, "Distance from the ceiling to the center plane of the luminaires"
SPACE,             0, WORKPLANE-HEIGHT,                                                     "",  1517, 32084, 0,  2, "Distance from the floor to the workplane; PowerDOE calculates the Illuminance at this height"
SPACE,             0, ELEC-ILLUMINANCE,            "Illuminance Desired from Lighting System ",  3005, 32008, 0,  2, "Desired average illuminance from each of the lighting subsystems"
SPACE,             0, LTG-SPEC-METHOD,                                                      "", 19041, 32084, 0,  2, "Power Defn=simplified;Luminaire Count=Lighting Systems;Illuminance=light level desired"
SPACE,             0, LOCATION,                         "Location of Space on Floor Perimeter", 19155, 32008, 0,  2, "Location of the space in the parent floor's polygon or Box"
SPACE,             0, *DISP-LIGHT-KW,                                      "Overhead Lighting", 62015, 32008, 0,  2, ""
SPACE,             0, *DISP-LIGHT-W/AR,                                                     "",     0, 32008, 0,  2, ""
SPACE,             0, *DISP-EQUIP-KW,                                              "Equipment", 12072, 32008, 0,  2, ""
SPACE,             0, *DISP-EQUIP-W/AR,                                                     "",     0, 32008, 0,  2, ""
SPACE,             0, *DISP-TASK-KW,                                                        "",     0, 32008, 0,  2, ""
SPACE,             0, *DISP-TASK-W/AR,                                                      "",     0, 32008, 0,  2, ""
EXTERIOR-WALL,     0, CONSTRUCTION,                                             "Construction",  2502, 32010, 0,  0, "The construction (Layers) of the surface"
EXTERIOR-WALL,     0, GND-REFLECTANCE,                                    "Ground Reflectance", 12085, 32010, 0,  3, "Fraction of solar radiation ('seen' by this exterior surface) that is reflected by the ground plane"
EXTERIOR-WALL,     0, SKY-FORM-FACTOR,                                                      "", 63054, 32010, 0,  2, "Fraction of the hemisphere facing the surface that is open sky"
EXTERIOR-WALL,     0, GND-FORM-FACTOR,                                                      "", 63055, 32010, 0,  2, "Fraction of the hemisphere facing the surface that is the 'ground'"
EXTERIOR-WALL,     0, INF-COEF,                                     "Infiltration Coefficient", 12080, 32010, 0,  1, "Infiltration flow coefficient for this exterior surface (used with the infiltration Crack Method)"
EXTERIOR-WALL,     0, DEG-FROM-NORTH,               "Wall AZIMUTH clock-wise from true north ",     0, 32010, 0,  2, ""
EXTERIOR-WALL,     0, OUTSIDE-EMISS,                                      "Outside Emissivity", 12081, 32010, 0,  0, "Infrared (IR) emissivity of the exterior finish of this surface"
EXTERIOR-WALL,     0, INSIDE-SOL-ABS,                               "Inside Solar Absorptance", 12082,   753, 0,  3, "Fraction of incident total solar radiation the inside absorbs (see Inside Solar Fraction)"
EXTERIOR-WALL,     0, SOLAR-FRACTION,                                  "Inside Solar Fraction", 12083, 32010, 0,  3, "The fraction of solar radiation entering this space incident on the interior of this surface"
EXTERIOR-WALL,     0, SHADING-DIVISION,                          "Number of Shading Divisions", 12088, 32010, 0,  0, "Number of 'vertical' segmentations used in shading calculations for this exterior surface"
EXTERIOR-WALL,     0, MULTIPLIER,                                                 "Multiplier", 12001,   769, 0,  0, "Number of identical surfaces in this space"
EXTERIOR-WALL,     0, INSIDE-VIS-REFL,                            "Inside Visible Reflectance", 12084,  3006, 0,  3, "Fraction of the incident visible light reflected by the interior finish of this surface"
EXTERIOR-WALL,     0, X,                                                                   "X", 19008,   755, 0,  1, "X coordinate for the surface origin (relative to this Space coordinate system)"
EXTERIOR-WALL,     0, Y,                                                                   "Y", 19009,   755, 0,  1, "Y coordinate for the surface origin (relative to this Space coordinate system)"
EXTERIOR-WALL,     0, Z,                                                                   "Z", 19010,   755, 0,  1, "Z coordinate for the surface origin (relative to this Space coordinate system)"
EXTERIOR-WALL,     0, HEIGHT,                                                         "Height", 19013, 32010, 0,  1, "Dimension of the surface parallel to the Surface Y-axis"
EXTERIOR-WALL,     0, WIDTH,                                                           "Width", 19014, 32010, 0,  1, "Width of the surface (measured parallel to the Surface x-axis)."
EXTERIOR-WALL,     0, AZIMUTH,                                                            "Az", 19011,   755, 0,  1, "Azimuth of surface outward normal relative to Space Y-axis (positive = clockwise rotation)"
EXTERIOR-WALL,     0, TILT,                                                             "Tilt", 19012, 32010, 0,  1, "Tilt of the surface outward normal, relative to the Space Z-axis (+ for clockwise rotation)"
EXTERIOR-WALL,     0, LOCATION,                                                     "Location", 19015,   755, 0,  0, "Positions this surface in the space (applies only if space is defined with Shape or Polygon)"
EXTERIOR-WALL,     0, SURFACE-TYPE,                                                         "", 63036, 32010, 0,  2, "Whether this is a ceiling, roof, floor or wall"
EXTERIOR-WALL,     0, POLYGON,                                                              "",   694, 31030, 0,  2, "Name of the Polygon that defines the wall's geometry"
EXTERIOR-WALL,     0, SHADING-SURFACE,                                       "Shading Surface", 12090,   777, 0,  0, "YES causes this exterior surface to also act as a Building Shade."
EXTERIOR-WALL,     0, EW-DIF-REFL,                                                          "", 63038, 32010, 0,  2, ""
EXTERIOR-WALL,     0, EW-SPEC-REFL,                                                         "", 63039, 32010, 0,  2, ""
EXTERIOR-WALL,     0, EW-REFL-ROUGH,                                                        "", 63053, 32010, 0,  2, ""
EXTERIOR-WALL,     0, GROUND-DIF-REFL,                                                      "", 63041, 32010, 0,  2, ""
EXTERIOR-WALL,     0, GROUND-SPEC-REFL,                                                     "", 63042, 32010, 0,  2, ""
EXTERIOR-WALL,     0, GROUND-REFL-ROUG,                                                     "", 63043, 32010, 0,  2, ""
EXTERIOR-WALL,     0, FUNCTION,                                                             "",     0, 32010, 0,  2, ""
EXTERIOR-WALL,     0, WINDOWS,                                                              "",     0, 32010, 0,  2, ""
EXTERIOR-WALL,     0, DOORS,                                                                "",     0, 32010, 0,  2, ""
WINDOW,            0, GLASS-TYPE,                                                 "Glass Type", 19019,   760, 0,  0, "Select a glass type for the window"
WINDOW,            0, SHADING-SCHEDULE,                                     "Shading Schedule", 12099,   762, 0,  0, "Schedule containing hourly multipliers applied to the solar transmission of this window"
WINDOW,            0, CONDUCT-SCHEDULE,                                 "Conductance Schedule", 12112,   762, 0,  0, "Schedule containing hourly multipliers for glass conductance properties for this window"
WINDOW,            0, SHADING-DIVISION,                          "Number of Shading Divisions", 12100, 32012, 0,  2, "Number of 'vertical' segmentations used in shading calculations for this window"
WINDOW,            0, SKY-FORM-FACTOR,                                                      "", 63054, 32012, 0,  2, "Fraction of the hemisphere facing the surface that is open sky"
WINDOW,            0, GND-FORM-FACTOR,                                                      "", 63055, 32012, 0,  2, "Fraction of the hemisphere facing the surface that is the 'ground'"
WINDOW,            0, INF-COEF,                                     "Infiltration Coefficient", 12114, 32012, 0,  1, "Infiltration flow coefficient for this window (used with the infiltration Crack Method)"
WINDOW,            0, WIN-SPEC-METHOD,                           "Window Specification Method", 12381, 32012, 0,  2, "Glass Type Input = from library; Window Layers Input = custom defined using Layers"
WINDOW,            0, FRAME-WIDTH,                                               "Frame Width", 19026,   775, 0,  1, "Width of window frame (assumed equal for all four sides of the window)"
WINDOW,            0, MULTIPLIER,                                                 "Multiplier", 12011,   769, 0,  0, "Number of identical windows on this surface"
WINDOW,            0, CONVERGENCE-TOL,                                                      "", 13136, 32012, 0,  0, "Initiates detailed window conductance calculations (extremely slow computation)"
WINDOW,            0, X,                                                                   "X", 19022,   788, 0,  1, "X coordinate for the window origin (relative to this Surface coordinate system)"
WINDOW,            0, Y,                                                                   "Y", 19023,   788, 0,  1, "Y coordinate for the window origin (relative to this Surface coordinate system)"
WINDOW,            0, HEIGHT,                                                         "Height", 19024, 32012, 0,  1, "Dimension of the window parallel to the Surface Y-axis"
WINDOW,            0, WIDTH,                                                           "Width", 19025, 32012, 0,  1, "Width of the window (measured parallel to the Surface x-axis)."
WINDOW,            0, SETBACK,                                                       "Setback", 19027,   776, 0,  0, "The distance that the window is recessed into the wall (shading effects only)"
WINDOW,            0, WIN-SHADE-TYPE,                                                       "", 63048, 32012, 0,  2, "Type of shading device - for total solar gain and/or glare control; requires a Shading Schedule"
WINDOW,            0, MAX-SOLAR-SCH,                                  "Maximum Solar Schedule", 12103,   762, 0,  0, "Schedule of maximum tolerable direct solar gain values (e.g., simulates closed blinds)"
WINDOW,            0, VIS-TRANS-SCH,                          "Visible Transmittance Schedule", 12106,  3006, 0,  0, "Schedule of hourly multipliers applied to the visible transmission of this window"
WINDOW,            0, CONDUCT-TMIN-SCH,             "Conductance Minimum Temperature Schedule", 12113,   762, 0,  0, "Schedule of minimum ambient temperatures (used to simulate movable insulation)"
WINDOW,            0, SUN-CTRL-PROB,                                 "Sun Control Probability", 12107,   762, 0,  3, "Probability that an open shade will be closed when direct solar gain exceeds Maximum Glare"
WINDOW,            0, GLARE-CTRL-PROB,                             "Glare Control Probability", 12108,   762, 0,  0, "Probability that a shade is re-opened when (beam & diffuse) solar gain decreases sufficiently"
WINDOW,            0, INSIDE-VIS-REFL,                            "Inside Visible Reflectance", 12109,  3006, 0,  3, "Fraction of the incident visible light reflected by the interior surface of this window"
WINDOW,            0, DAY-X-DIVISION,                                    "Daylight X Division", 12110,  3006, 0,  0, "Number of 'vertical' segmentations used in direct daylight calculations for this window"
WINDOW,            0, DAY-Y-DIVISION,                                    "Daylight Y Division", 12111,  3006, 0,  0, "Number of 'horizontal' segmentations used in direct daylight calculations for this window"
WINDOW,            0, OPEN-SHADE-SCH,                                    "Open Shade Schedule", 12104,   762, 0,  0, "Probability that a shade is re-opened when (beam & diffuse) solar gain decreases sufficiently"
WINDOW,            0, SOL-TRANS-SCH,                            "Solar Transmittance Schedule", 12105,   753, 0,  0, "Schedule containing hourly solar transmission properties of shades (sunspaces only)"
WINDOW,            0, GLASS-TYPE-SW,                       "Glass Type When  in Switched Mode", 12115,   774, 0,  0, "For switchable glazings,  name of the glass type for the fully switched state"
WINDOW,            0, SWITCH-CONTROL,                                         "Switch Control", 12116,   774, 0,  0, "For switchable glazings,  specifies how the switching is controlled"
WINDOW,            0, SWITCH-SET-LO,            "Switch Lo Setting (point of 100% main glass)", 12117,   774, 0,  1, "Lower set point value for the selected window Switch Control variable"
WINDOW,            0, SWITCH-SET-HI,       "Switch Hi Setting (point of 100% alternate glass)", 12118,   774, 0,  1, "Upper set point value for the selected window Switch Control variable"
WINDOW,            0, SWITCH-SCH,      "Schedule of Control Variable for Glass Type Switching", 12119,   774, 0,  0, "Schedule that specifies when glass switching is allowed"
WINDOW,            0, OVERHANG-A,                                                 "Overhang A", 12217, 32033, 0,  0, "Distance overhang extends beyond the LEFT edge of the window"
WINDOW,            0, OVERHANG-B,                                                 "Overhang B", 12218, 32033, 0,  0, "Distance between the top of the window and the bottom of the overhang"
WINDOW,            0, OVERHANG-W,                                                 "Overhang W", 12220, 32033, 0,  0, "Width of the overhang (measured parallel to the Window X-axis)"
WINDOW,            0, OVERHANG-D,                                                 "Overhang D", 12219, 32033, 0,  0, "Depth of the overhang (the dimension of both of the projecting edges)"
WINDOW,            0, OVERHANG-ANGLE,                                         "Overhang Angle", 12221, 32033, 0,  0, "Angle of the overhang relative to the window plane (e.g., <90° tilts 'down',  >90° tilts 'up')"
WINDOW,            0, LEFT-FIN-A,                                                 "Left Fin A", 12213, 32033, 0,  0, "Distance between the left edge of the window and the edge of the left fin"
WINDOW,            0, LEFT-FIN-B,                                                 "Left Fin B", 12214, 32033, 0,  0, "Distance between left fin top edge and window top edge, (-) fin extends above window"
WINDOW,            0, LEFT-FIN-H,                                                 "Left Fin H", 12216, 32033, 0,  0, "Height of the left fin (measured parallel to the Window Y-axis)"
WINDOW,            0, LEFT-FIN-D,                                                 "Left Fin D", 12215, 32033, 0,  0, "Depth of the left fin (the dimension of either of the projecting edges)"
WINDOW,            0, RIGHT-FIN-A,                                               "Right Fin A", 12222, 32033, 0,  0, "Distance between the right edge of the window and the edge of the right fin"
WINDOW,            0, RIGHT-FIN-B,                                               "Right Fin B", 12223, 32033, 0,  0, "Distance between right fin top edge and window top edge, (-) fin extends above window"
WINDOW,            0, RIGHT-FIN-H,                                               "Right Fin H", 12225, 32033, 0,  0, "Height of the right fin (measured parallel to the Window Y-axis)"
WINDOW,            0, RIGHT-FIN-D,                                               "Right Fin D", 12224, 32033, 0,  0, "Depth of the right fin (the dimension of both of the projecting edges)"
WINDOW,            0, WI-SH-DIF-REFL,                                                       "", 63051, 32012, 0,  2, ""
WINDOW,            0, WI-SH-SPEC-REFL,                                                      "", 63052, 32012, 0,  2, ""
WINDOW,            0, WI-SH-REFL-ROUGH,                                                     "", 63053, 32012, 0,  2, ""
WINDOW,            0, FRAME-CONDUCT,                                                        "", 13137,   775, 0,  2, "Thermal conductance of the frame ( including the inside air film, excluding the outside airfilm)"
WINDOW,            0, SPACER-TYPE,                                                          "", 13139,   761, 0,  2, "The type of spacer that separates the glass layers (in multi-pane windows)"
WINDOW,            0, FRAME-ABS,                                                            "", 13138,   775, 0,  2, "Fraction of total incident solar radiation absorbed by the outside surface of the frame"
WINDOW,            0, FUNCTION,                                                             "",     0, 32012, 0,  2, ""
WINDOW,            0, WINDOW-SPEC-FN,                                                       "",     0, 32012, 0,  2, ""
WINDOW,            0, WINDOW-LAYERS,                                    "Select Window Layer ", 61032, 32012, 0,  2, "Window layers are specified from outside to inside"
WINDOW,            0, SLAT-SCHEDULE,                      "Schedule For Control of Slat Angle",   764, 32092, 0,  2, "Adjusts slat coverage between the Minimum Slat Coverage and Maximum Slat Coverage"
WINDOW,            0, SLAT-TRIGG-SCH,  "Schedule: Threshold Value for Slat Control Variable",   763, 32092, 0,  2, "If Room Temp or Solar Intensity > this, slats are closed (see Slat Adjustment Type)"
WINDOW,            0, SLAT-ADJ-TYPE,                                                        "",   765, 32092, 0,  2, "Indicates how the Slat Angle is adjusted (if a blind is present)"
WINDOW,            0, BLIND-SCHEDULE,                 "Schedule For Control of Blind Coverage",   767, 32092, 0,  2, "Adjusts blind coverage between the Minimum Blind Coverage and Maximum Blind Coverage"
WINDOW,            0, BLIND-TRIGG-SCH, "Schedule: Threshold Value for Blind Deployment Variable",   766, 32092, 0,  2, "If Room Temp or Solar Intensity > this, blinds are closed (see Blind Adjustment Type)"
WINDOW,            0, BLIND-ADJ-TYPE,                                                       "",   768, 32092, 0,  2, "None=fixed;Sched=Blind Sch;Solar Intensity=Blind Trig Sch;Room T=if T> Blind Trig Sch"
WINDOW,            0, TUBE-DIAMETER,                                          "Tube Diameter:",     0, 32012, 0,  2, "Diameter of tube"
INTERIOR-WALL,     0, NEXT-TO,                                           "Space On Other Side", 63044,   771, 0,  2, "Name of space on other side of wall (for heat tranfer)"
INTERIOR-WALL,     0, AREA,                                                             "Area", 12166, 32013, 0,  1, "Area of this interior surface (an alternative to entering Height and Width)"
INTERIOR-WALL,     0, CONSTRUCTION,                                             "Construction", 12522, 32013, 0,  0, "Assign interior wall construction."
INTERIOR-WALL,     0, CONVECT-FILM-RES,                                                     "",     0, 32013, 0,  2, "(Not yet defined)"
INTERIOR-WALL,     0, INSIDE-SOL-ABS,                               "Inside Solar Absorptance", 12142,   753, 0,  3, "The fraction of incident total solar radiation absorbed at the interior finish of this surface"
INTERIOR-WALL,     0, SOLAR-FRACTION,                                  "Inside Solar Fraction", 12144, 32013, 0,  3, "The fraction of solar radiation entering this space incident on the interior of this surface"
INTERIOR-WALL,     0, INT-WALL-TYPE,                                   "Interior Surface Type", 12165, 32013, 0,  0, "Type of interior wall"
INTERIOR-WALL,     0, X,                                                                   "X", 19065,   755, 0,  2, "X coordinate for the surface origin (relative to this Space coordinate system)"
INTERIOR-WALL,     0, Y,                                                                   "Y", 19066,   755, 0,  2, "Y coordinate for the surface origin (relative to this Space coordinate system)"
INTERIOR-WALL,     0, Z,                                                                   "Z", 19067,   755, 0,  2, "Z coordinate for the surface origin (relative to this Space coordinate system)"
INTERIOR-WALL,     0, HEIGHT,                                                         "Height", 19071, 32013, 0,  2, "Dimension of the surface parallel to the Surface Y-axis"
INTERIOR-WALL,     0, WIDTH,                                                           "Width", 19072, 32013, 0,  2, "Width of the surface (measured parallel to the Surface x-axis)."
INTERIOR-WALL,     0, AZIMUTH,                                                       "Azimuth", 19068,   755, 0,  2, "Azimuth of surface outward normal relative to Space Y-axis (positive = clockwise rotation)"
INTERIOR-WALL,     0, TILT,                                                             "Tilt", 19069,   755, 0,  2, "Tilt of the surface outward normal,  relative to the Space Z-axis (+ for clockwise rotation)"
INTERIOR-WALL,     0, LOCATION,                                                     "Location", 19070,   755, 0, 21, "Positions this surface in the space (applies only if space is defined with Shape or Polygon)"
INTERIOR-WALL,     0, SURFACE-TYPE,                                                         "", 63036, 32013, 0,  2, ""
INTERIOR-WALL,     0, POLYGON,                                                              "",   694, 31030, 0,  2, "Name of the Polygon that defines the wall's geometry"
INTERIOR-WALL,     0, INSIDE-VIS-REFL,                            "Inside Visible Reflectance", 12143,  3006, 0,  3, "Fraction of the incident visible light reflected by the interior finish of this surface"
INTERIOR-WALL,     0, WINDOWS,                                                              "",     0, 32013, 0,  2, ""
UNDERGROUND-WALL,  0, AREA,                                                             "Area", 12161, 32014, 0,  1, "Area of this underground surface (an alternative to entering Height and Width)"
UNDERGROUND-WALL,  0, CONSTRUCTION,                                             "Construction", 12736, 32014, 0,  0, "The construction (Layers) of the surface"
UNDERGROUND-WALL,  0, CONVECT-FILM-RES,                           "Convective Film Resistance", 12124, 32014, 0,  2, "(Not yet defined)"
UNDERGROUND-WALL,  0, INSIDE-SOL-ABS,                               "Inside Solar Absorptance", 12146,   753, 0,  3, "The fraction of incident total solar radiation absorbed at the interior finish of this surface"
UNDERGROUND-WALL,  0, SOLAR-FRACTION,                                  "Inside Solar Fraction", 12148, 32014, 0,  0, "The fraction of solar radiation entering this space incident on the interior of this surface"
UNDERGROUND-WALL,  0, MULTIPLIER,                                                 "Multiplier", 12160,   769, 0,  0, "Number of identical surfaces in this space"
UNDERGROUND-WALL,  0, U-EFFECTIVE,                                                          "", 12162, 32014, 0,  0, "Effective u-value (used with custom weighting factors to estimate perimeter conduction)"
UNDERGROUND-WALL,  0, X,                                                                   "X", 19051,   755, 0,  2, "X coordinate for the surface origin (relative to this Space coordinate system)"
UNDERGROUND-WALL,  0, Y,                                                                   "Y", 19052,   755, 0,  2, "Y coordinate for the surface origin (relative to this Space coordinate system)"
UNDERGROUND-WALL,  0, Z,                                                                   "Z", 19053,   755, 0,  2, "Z coordinate for the surface origin (relative to this Space coordinate system)"
UNDERGROUND-WALL,  0, HEIGHT,                                                         "Height", 19057, 32014, 0,  2, "Dimension of the surface parallel to the Surface Y-axis (before applying a Tilt)"
UNDERGROUND-WALL,  0, WIDTH,                                                           "Width", 19058, 32014, 0,  2, "Width of the surface (measured parallel to the Surface x-axis)."
UNDERGROUND-WALL,  0, AZIMUTH,                                                       "Azimuth", 19054,   755, 0,  2, "Azimuth of outward normal relative to Space Y-axis; before applying Tilt (positive = clockwise)"
UNDERGROUND-WALL,  0, TILT,                                                             "Tilt", 19055,   755, 0,  2, "Tilt of the surface outward normal,  relative to the Space Z-axis (+ for clockwise rotation)"
UNDERGROUND-WALL,  0, LOCATION,                                                     "Location", 19056,   755, 0,  0, "Positions this surface in the space (applies only if space is defined with Shape or Polygon)"
UNDERGROUND-WALL,  0, SURFACE-TYPE,                                                         "", 63036, 32014, 0,  2, ""
UNDERGROUND-WALL,  0, POLYGON,                                                              "",   694, 31030, 0,  2, "Name of the Polygon that defines the wall's geometry"
UNDERGROUND-WALL,  0, INSIDE-VIS-REFL,                            "Inside Visible Reflectance", 12147,  3006, 0,  3, "Fraction of the incident visible light reflected by the interior finish of this surface"
UNDERGROUND-WALL,  0, FUNCTION,                                                             "",     0, 32014, 0,  2, ""
DESIGN-DAY,        0, TYPE,                                                  "Design Day Type",  1514, 32017, 0,  0, "The type of Design Day: Heating or Cooling"
DESIGN-DAY,        0, DRYBULB-HIGH,                                             "Drybulb High", 12737, 32017, 0,  0, "Maximum outside air drybulb temperature during the Design Day"
DESIGN-DAY,        0, DRYBULB-RANGE,                                           "Drybulb Range", 12738, 32017, 0,  0, "Maximum swing in outside air drybulb temperatures during the Design Day"
DESIGN-DAY,        0, WETBULB-AT-HIGH,                                       "Wetbulb at High",  1516, 32017, 0,  0, "The outside air wetbulb temperature that corresponds to the Drybulb High temperature"
DESIGN-DAY,        0, HOUR-HIGH,                                                   "Hour High", 12739, 32017, 0,  0, "The hour during which the maximum outside air drybulb temperature (Drybulb High) occurs"
DESIGN-DAY,        0, HOUR-LOW,                                                     "Hour Low", 12740, 32017, 0,  0, "The hour during which the minimum outside air drybulb temperature (Drybulb Low) occurs"
DESIGN-DAY,        0, WIND-SPEED,                                                 "Wind Speed", 12745, 32017, 0,  0, "The local wind speed during the whole Design Day (expressed in knots)"
DESIGN-DAY,        0, WIND-DIR,                                               "Wind Direction", 12746, 32017, 0,  0, "The direction that the wind comes from during the whole Design Day"
DESIGN-DAY,        0, CLOUD-AMOUNT,                                             "Cloud Amount", 12747, 32017, 0,  0, "Amount of cloud cover during the whole Design Day (on a scale of one to ten)"
DESIGN-DAY,        0, MONTH,                                                           "Month",  1513, 32017, 0,  0, "The Month during which PowerDOE performs the Design Day calculation"
DESIGN-DAY,        0, DAY,                                                               "Day",  1512, 32017, 0,  0, "The Day during which PowerDOE performs the Design Day calculation"
DESIGN-DAY,        0, GROUND-T,                                           "Ground Temperature",   812, 32017, 0,  0, "Local ground temperature during the whole Design Day"
DESIGN-DAY,        0, CLIMATE,                                                       "Climate",  1511, 32017, 0,  0, "Type of climate at the site (used by PowerDOE in the new cloud cover model)"
DESIGN-DAY,        0, VISIBILITY,                                                 "Visibility",  1515, 32017, 0,  0, "The type of visibility at the site (used by PowerDOE in the new cloud cover model)"
DESIGN-DAY,        0, NUMBER-OF-DAYS,                                                       "",     0, 32017, 0,  0, "Number of days to simulate these conditions, starting at above MONTH/DAY"
LOADS-REPORT,      0, VERIFICATION,                                                         "",     0, 32018, 0,  2, ""
LOADS-REPORT,      0, SUMMARY,                                                              "",     0, 32018, 0,  2, ""
LOADS-REPORT,      0, DUMP-OPTIONS,                                                         "",     0, 32018, 0,  2, ""
LOADS-REPORT,      0, REPORT-FREQUENCY,                                                     "",     0, 32018, 0,  2, ""
LOADS-REPORT,      0, HOURLY-DATA-SAVE,                                                     "",     0, 32018, 0,  2, ""
LAYERS,            0, INSIDE-FILM-RES,                        "Inside Film Resistance (R-val)", 12132, 32019, 0,  3, "The combined convective and radiative air film resistance for the inside wall surface"
LAYERS,            0, MATERIAL,                                                    "Material ", 13124, 32019, 0,  0, ""
LAYERS,            0, THICKNESS,                                                            "", 13125, 32019, 0,  2, ""
LAYERS,            0, PICTURE,                                                              "",     0, 32019, 0,  2, ""
LAYERS,            0, DRAWING,                                                              "",     0, 32019, 0,  2, ""
MATERIAL,          0, TYPE,                                                    "Material Type", 14470, 32020, 0,  0, "Whether you specify merely the thermal Resistance of the material, or all of its properties"
MATERIAL,          0, THICKNESS,                                                   "Thickness", 13125, 32020, 0,  3, "Thickness of the material"
MATERIAL,          0, CONDUCTIVITY,                                             "Conductivity", 13126, 32020, 0,  4, "Thermal conductivity of the material"
MATERIAL,          0, DENSITY,                                                       "Density", 13127, 32020, 0,  2, "Density of the material"
MATERIAL,          0, SPECIFIC-HEAT,                                           "Specific Heat", 13128, 32020, 0,  3, "Specific heat capacity of the material"
MATERIAL,          0, RESISTANCE,                                                 "Resistance", 13129, 32020, 0,  3, "Thermal resistance of the material"
REPORT-BLOCK,      0, VARIABLE-TYPE,                                           "Variable Type", 12752, 32021, 0,  0, ""
REPORT-BLOCK,      0, VARIABLE-LIST,                                           "Variable List", 12753, 32021, 0,  0, ""
HOURLY-REPORT,     0, OPTION,                                                               "",     0, 32022, 0,  2, ""
HOURLY-REPORT,     0, DIVIDE,                                                               "",     0, 32022, 0,  2, ""
HOURLY-REPORT,     0, AXIS-ASSIGN,                                                          "",     0, 32022, 0,  2, ""
HOURLY-REPORT,     0, AXIS-MAX,                                                             "",     0, 32022, 0,  2, ""
HOURLY-REPORT,     0, AXIS-MIN,                                                             "",     0, 32022, 0,  2, ""
HOURLY-REPORT,     0, AXIS-TITLES,                                                          "",     0, 32022, 0,  2, ""
HOURLY-REPORT,     0, REPORT-SCHEDULE,                                       "Report Schedule", 12752, 32022, 0,  0, ""
HOURLY-REPORT,     0, REPORT-BLOCK,                                       "First Report Block", 12753, 32022, 0,  0, ""
TITLE,             0, LINE-1,                                                               "",     0, 32023, 0,  2, ""
TITLE,             0, LINE-2,                                                               "",     0, 32023, 0,  2, ""
TITLE,             0, LINE-3,                                                               "",     0, 32023, 0,  2, ""
TITLE,             0, LINE-4,                                                               "",     0, 32023, 0,  2, ""
TITLE,             0, LINE-5,                                                               "",     0, 32023, 0,  2, ""
RUN-PERIOD,        0, BEGIN-MONTH,                                            "Starting Month", 13007, 32024, 0,  0, "Beginning month of the simulation"
RUN-PERIOD,        0, BEGIN-DAY,                                                "Starting Day", 13009, 32024, 0,  0, "Beginning day of the simulation"
RUN-PERIOD,        0, BEGIN-YEAR,                                              "Starting Year", 13011, 32024, 0,  0, "Beginning year of the simulation"
RUN-PERIOD,        0, END-MONTH,                                                "Ending Month", 13008, 32024, 0,  0, "Last month of the simulation"
RUN-PERIOD,        0, END-DAY,                                                    "Ending Day", 13010, 32024, 0,  0, "Last day of the simulation"
RUN-PERIOD,        0, END-YEAR,                                                  "Ending Year", 13012, 32024, 0,  0, "Last year of the simulation"
DOOR,              0, CONSTRUCTION,                                             "Construction",  3020, 32033, 0,  0, "The construction (Layers) of the door"
DOOR,              0, SHADING-DIVISION,                          "Number of Shading Divisions", 12120, 32033, 0,  0, "Number of 'vertical' segmentations used in shading calculations for this door"	
DOOR,              0, SKY-FORM-FACTOR,                                                      "", 63054, 32033, 0,  2, "Fraction of the hemisphere facing the surface that is open sky"
DOOR,              0, GND-FORM-FACTOR,                                                      "", 63055, 32033, 0,  2, "Fraction of the hemisphere facing the surface that is the 'ground'"
DOOR,              0, INF-COEF,                                     "Infiltration Coefficient", 12123, 32033, 0,  1, "Infiltration flow coefficient for this door (used with the infiltration Crack Method)"
DOOR,              0, CONVECT-FILM-RES,                           "Convective Film Resistance", 12124, 32033, 0,  1, "(Not yet defined)"
DOOR,              0, INSIDE-ABSORP,                                      "Inside Absorptance", 12125, 32033, 0,  3, "Fraction of incident total solar radiation absorbed at the interior finish of this surface"
DOOR,              0, MULTIPLIER,                                                 "Multiplier", 12152,   769, 0,  0, "Number of identical doors on this surface"
DOOR,              0, INSIDE-VIS-REFL,                            "Inside Visible Reflectance", 12126,  3006, 0,  3, "Fraction of the incident visible light reflected by the interior finish of this door"
DOOR,              0, X,                                                                   "X", 19034,   788, 0,  2, "X coordinate for the door origin (relative to this Surface coordinate system)"
DOOR,              0, Y,                                                                   "Y", 19035,   788, 0,  2, "Y coordinate for the door origin (relative to this Surface coordinate system)"
DOOR,              0, HEIGHT,                                                         "Height", 19036, 32033, 0,  2, "Dimension of the door parallel to the Surface Y-axis"
DOOR,              0, WIDTH,                                                           "Width", 19037, 32033, 0,  2, "Width of the door (measured parallel to the Surface x-axis)."
DOOR,              0, SETBACK,                                                       "Setback", 19038,   776, 0,  0, "The distance that the door is recessed into the wall (shading effects only)"
DOOR,              0, OVERHANG-A,                                                 "Overhang A", 12230, 32033, 0,  0, "Distance overhang extends beyond the LEFT edge of the door, (-) for no extension"
DOOR,              0, OVERHANG-B,                                                 "Overhang B", 12231, 32033, 0,  0, "Distance between the top of the door and the bottom of the overhang"
DOOR,              0, OVERHANG-W,                                                 "Overhang W", 12233, 32033, 0,  0, "Width of the overhang (measured parallel to the Door X-axis)"
DOOR,              0, OVERHANG-D,                                                 "Overhang D", 12232, 32033, 0,  0, "Depth of the overhang (the dimension of both of the projecting edges)"
DOOR,              0, OVERHANG-ANGLE,                                         "Overhang Angle", 12234, 32033, 0,  1, "Angle of the overhang relative to the door plane (e.g.,  <90° tilts 'down', >90° tilts 'up')"
DOOR,              0, LEFT-FIN-A,                                                 "Left Fin A", 12226, 32033, 0,  0, "Distance between the left edge of the door and the edge of the left fin"
DOOR,              0, LEFT-FIN-B,                                                 "Left Fin B", 12227, 32033, 0,  0, "Distance between left fin top edge and door top edge,  (-) fin extends above door"
DOOR,              0, LEFT-FIN-H,                                                 "Left Fin H", 12229, 32033, 0,  0, "Height of the left fin (measured parallel to the door Y-axis)"
DOOR,              0, LEFT-FIN-D,                                                 "Left Fin D", 12228, 32033, 0,  0, "Depth of the left fin (the dimension of either of the projecting edges)"
DOOR,              0, RIGHT-FIN-A,                                               "Right Fin A", 12235, 32033, 0,  0, "Distance between the right edge of the door and the edge of the right fin"
DOOR,              0, RIGHT-FIN-B,                                               "Right Fin B", 12236, 32033, 0,  0, "Distance between right fin top edge and door top edge, (-) fin extends above door"
DOOR,              0, RIGHT-FIN-H,                                               "Right Fin H", 12238, 32033, 0,  0, "Height of the right fin (measured parallel to the door Y-axis)"
DOOR,              0, RIGHT-FIN-D,                                               "Right Fin D", 12237, 32033, 0,  0, "Depth of the right fin (the dimension of both of the projecting edges)"
DOOR,              0, DR-SH-DIF-REFL,                                                       "", 63056, 32033, 0,  2, ""
DOOR,              0, DR-SH-SPEC-REFL,                                                      "", 63057, 32033, 0,  2, ""
DOOR,              0, DR-SH-REFL-ROUGH,                                                     "", 63058, 32033, 0,  2, ""
DOOR,              0, FUNCTION,                                                             "",     0, 32033, 0,  2, ""
WEIGHTING-FACTOR,  0, FACTOR-LIST,                                                          "",   727, 32034, 0,  2, ""
WALL-PARAMETERS,   0, EMISSIVITY,                                                           "",     0,   753, 0,  2, ""
WALL-PARAMETERS,   0, CHANNEL-WIDTH,                                                        "",     0,   753, 0,  2, ""
WALL-PARAMETERS,   0, LOWER-VENT-AREA,                                                      "",     0,   753, 0,  2, ""
WALL-PARAMETERS,   0, UPPER-VENT-AREA,                                                      "",     0,   753, 0,  2, ""
WALL-PARAMETERS,   0, VERT-VENT-SEP,                                                        "",     0,   753, 0,  2, ""
WALL-PARAMETERS,   0, AIR-FLOW-TYPE,                                                        "",     0,   753, 0,  2, ""
WALL-PARAMETERS,   0, AIR-FLOW-RATE,                                                        "",     0,   753, 0,  2, ""
WALL-PARAMETERS,   0, AIR-FLOW-CFM,                                                         "",     0,   753, 0,  2, ""
WALL-PARAMETERS,   0, AIR-FLOW-CTRL-DT,                                                     "",     0,   753, 0,  2, ""
WALL-PARAMETERS,   0, FAN-KW/FLOW,                                                          "",     0,   753, 0,  2, ""
WALL-PARAMETERS,   0, FAN-KW,                                                               "",     0,   753, 0,  2, ""
WALL-PARAMETERS,   0, DOORWAY-H,                                                            "",     0,   753, 0,  2, ""
WALL-PARAMETERS,   0, DOORWAY-W,                                                            "",     0,   753, 0,  2, ""
FIXED-SHADE,       0, TRANSMITTANCE,                                           "Transmittance", 12801, 32005, 0,  0, "Fraction of the incident (direct) solar radiation that passes through the Fixed Shade"
FIXED-SHADE,       0, SHADE-SCHEDULE,                                         "Shade Schedule", 19094, 32005, 0,  0, "Fraction Schedule: transmittance of direct (beam) solar radiation for the Fixed Shade"
FIXED-SHADE,       0, SHADE-VIS-REFL,                                    "Visible Reflectance", 12802,  3006, 0,  0, "Visible reflectance of the side of the Fixed Shade from which the outward normal points"
FIXED-SHADE,       0, SHADE-GND-REFL,                                     "Ground Reflectance", 12803, 32005, 0,  0, "The visible light reflectance of the ground near the Fixed Shade"
FIXED-SHADE,       0, X-REF,                                                               "X", 19088,   788, 0,  1, "X coordinate for the shade origin (relative to the Site coordinate system)"
FIXED-SHADE,       0, Y-REF,                                                               "Y", 19089,   788, 0,  1, "Y coordinate for the shade origin (relative to the Site coordinate system)"
FIXED-SHADE,       0, Z-REF,                                                               "Z", 19090,   788, 0,  1, "Z coordinate for the shade origin (relative to the Site coordinate system)"
FIXED-SHADE,       0, HEIGHT,                                                         "Height", 19091, 32005, 0,  1, "Height of the shade (measured parallel to the Site z-axis)."
FIXED-SHADE,       0, WIDTH,                                                           "Width", 19092, 32005, 0,  1, "Width of the shade (measured parallel to the Site x-axis)."
FIXED-SHADE,       0, AZIMUTH,                                                       "Azimuth", 19093,   788, 0,  1, "Azimuth of surface outward normal relative to Site Y-axis (positive = clockwise rotation)"
FIXED-SHADE,       0, TILT,                                                             "Tilt", 19095, 32005, 0,  1, "Tilt of the surface outward normal, relative to the Site Z-axis (+ for clockwise rotation)"
FIXED-SHADE,       0, SHADE-DIF-REFL,                                                       "",     0, 32005, 0,  0, ""
FIXED-SHADE,       0, SHADE-SPEC-REFL,                                                      "",     0, 32005, 0,  0, ""
FIXED-SHADE,       0, SHADE-REFL-ROUGH,                                                     "",     0, 32005, 0,  0, ""
HOLIDAYS,          0, TYPE,                                                     "Holiday Type", 14534, 12543, 0,  2, "Whether the official US Holidays are used, or none, or a custom set of Holidays"
HOLIDAYS,          0, MONTHS,                                                          "Month",   691, 12543, 0,  2, "The month number of each custom Holiday"
HOLIDAYS,          0, DAYS,                                                              "Day",   685, 12543, 0,  2, "The day number of each custom Holiday"
POLYGON,           0, V1,                                                     "Vertex 1 (X,Y)", 61000, 31030, 0,  2, ""
POLYGON,           0, V2,                                                     "Vertex 2 (X,Y)", 61001, 31030, 0,  2, ""
POLYGON,           0, V3,                                                     "Vertex 3 (X,Y)", 61002, 31030, 0,  2, ""
POLYGON,           0, V4,                                                     "Vertex 4 (X,Y)", 61003, 31030, 0,  2, ""
POLYGON,           0, V5,                                                     "Vertex 5 (X,Y)", 61004, 31030, 0,  2, ""
POLYGON,           0, V6,                                                     "Vertex 6 (X,Y)", 61005, 31030, 0,  2, ""
POLYGON,           0, V7,                                                     "Vertex 7 (X,Y)", 61006, 31030, 0,  2, ""
POLYGON,           0, V8,                                                     "Vertex 8 (X,Y)", 61007, 31030, 0,  2, ""
POLYGON,           0, V9,                                                     "Vertex 9 (X,Y)", 61008, 31030, 0,  2, ""
POLYGON,           0, V10,                                                   "Vertex 10 (X,Y)", 61009, 31030, 0,  2, ""
POLYGON,           0, V11,                                                   "Vertex 11 (X,Y)", 61010, 31030, 0,  2, ""
POLYGON,           0, V12,                                                   "Vertex 12 (X,Y)", 61011, 31030, 0,  2, ""
POLYGON,           0, V13,                                                   "Vertex 13 (X,Y)", 61011, 31030, 0,  2, ""
POLYGON,           0, V14,                                                   "Vertex 14 (X,Y)", 61011, 31030, 0,  2, ""
POLYGON,           0, V15,                                                   "Vertex 15 (X,Y)", 61011, 31030, 0,  2, ""
POLYGON,           0, V16,                                                   "Vertex 16 (X,Y)", 61011, 31030, 0,  2, ""
POLYGON,           0, V17,                                                   "Vertex 17 (X,Y)", 61011, 31030, 0,  2, ""
POLYGON,           0, V18,                                                   "Vertex 18 (X,Y)", 61011, 31030, 0,  2, ""
POLYGON,           0, V19,                                                   "Vertex 19 (X,Y)", 61011, 31030, 0,  2, ""
POLYGON,           0, V20,                                                   "Vertex 20 (X,Y)", 61011, 31030, 0,  2, ""
POLYGON,           0, V21,                                                   "Vertex 21 (X,Y)", 61011, 31030, 0,  2, ""
POLYGON,           0, V22,                                                   "Vertex 22 (X,Y)", 61011, 31030, 0,  2, ""
POLYGON,           0, V23,                                                   "Vertex 23 (X,Y)", 61011, 31030, 0,  2, ""
POLYGON,           0, V24,                                                   "Vertex 24 (X,Y)", 61011, 31030, 0,  2, ""
POLYGON,           0, V25,                                                   "Vertex 25 (X,Y)", 61011, 31030, 0,  2, ""
POLYGON,           0, V26,                                                   "Vertex 26 (X,Y)", 61011, 31030, 0,  2, ""
POLYGON,           0, V27,                                                   "Vertex 27 (X,Y)", 61011, 31030, 0,  2, ""
POLYGON,           0, V28,                                                   "Vertex 28 (X,Y)", 61011, 31030, 0,  2, ""
POLYGON,           0, V29,                                                   "Vertex 29 (X,Y)", 61011, 31030, 0,  2, ""
POLYGON,           0, V30,                                                   "Vertex 30 (X,Y)", 61011, 31030, 0,  2, ""
FLOOR,             0, MULTIPLIER,                                                           "", 12422,   769, 0,  2, "Number of floors in the facility that are identical, and served by the same HVAC system"
FLOOR,             0, X,                                                                   "X",  1002,   788, 0,  2, "X coordinate for the floor origin (relative to the Building coordinate system)"
FLOOR,             0, Y,                                                                   "Y", 19048,   788, 0,  2, "Y coordinate for the floor origin (relative to the Building coordinate system)"
FLOOR,             0, Z,                                                                   "Z", 19049,   788, 0,  2, "Z coordinate for the floor origin (relative to the Building coordinate system)"
FLOOR,             0, AZIMUTH,                                                       "Azimuth", 19059,   788, 0,  2, "Azimuth of outward normal relative to Space Y-axis; before applying Tilt (positive = clockwise)"
FLOOR,             0, SPACES,                                                               "",     0,  1510, 0,  2, ""
FLOOR,             0, POLYGON,                            "Polygon that Describes Floor Shape", 19060,  1510, 0,  2, "Name of the Polygon that defines the floor's geometry"
FLOOR,             0, SHAPE,                                  "Method to Describe Floor Shape", 19166,     0, 0,  2, "Specifies whether the geometry of floor is defined as a Box, using a Polygon, or No Shape"
FLOOR,             0, FLOOR-HEIGHT,                                  "Floor to Floor Distance", 19168,     0, 0,  2, "Average height of the floor (used to calculate the Volume of the floor)"
FLOOR,             0, AREA,                                                       "Floor Area", 12279,     0, 0,  2, "The gross Floor area of the floor"
FLOOR,             0, VOLUME,                                                   "Floor Volume", 12280,     0, 0,  2, "The total volume of the floor"
FLOOR,             0, WIDTH,                                                     "Floor Width", 19170,     0, 0,  2, "The average width of the floor (used to calculate the Area of the floor)"
FLOOR,             0, DEPTH,                                                     "Floor Depth", 19169,     0, 0,  2, "The depth of the floor (used to calculate the floor area)"
FLOOR,             0, SPACE-HEIGHT,                                "Height of Spaces on Floor", 19167,     0, 0,  2, "The default (average) Height of all spaces on the floor"
BUILD-PARAMETERS,  0, AZIMUTH,                                                       "Azimuth", 12542,   757, 0,  0, "Azimuth relative to true north (positive for clockwise rotation)"
BUILD-PARAMETERS,  0, HOLIDAYS,                                                     "Holidays", 12543, 32042, 0,  0, "Whether Holidays follow different schedules than days of the week (Mondays, Tuesdays, etc.)"
BUILD-PARAMETERS,  0, GROSS-AREA,                                                 "Gross Area", 12544, 32042, 0,  0, "Total building gross area (equals or exceeds sum of areas for conditioned spaces)"
BUILD-PARAMETERS,  0, HEAT-PEAK-PERIOD,                                     "Heat Peak Period", 12545, 32042, 0,  0, "Starting hour of daily time interval used to calculate Design Day heating peak loads"
BUILD-PARAMETERS,  0, COOL-PEAK-PERIOD,                                     "Cool Peak Period", 12547, 32042, 0,  0, "Starting hour of daily time interval used to calculate Design Day cooling peak loads"
BUILD-PARAMETERS,  0, X-REF,                                                     "X-Reference", 12549,   757, 0,  0, "X coordinate for the building origin (relative to the Reference coordinate system)"
BUILD-PARAMETERS,  0, Y-REF,                                                     "Y-Reference", 12550,   757, 0,  0, "Y coordinate for the building origin (relative to the Reference coordinate system)"
BUILD-PARAMETERS,  0, FUNCTION,                                                             "",     0, 32042, 0,  0, ""
BUILD-PARAMETERS,  0, DAYL-FUNCTION,                                                        "",     0, 32042, 0,  0, ""
BUILD-PARAMETERS,  0, SOLAR-REFL-CALC,                                                      "", 62004, 32042, 0,  0, "Whether PowerDOE calculates detailed solar reflections from adjacent components"
GLASS-TYPE-CODE,   0, DESCRIPTION,                                                          "", 13141, 32047, 0, 64, "Description of selected glass type code"
GLASS-TYPE-CODE,   0, NLAYER,                                                               "", 13142, 32047, 0,  0, "Number of panes of glass in the window"
GLASS-TYPE-CODE,   0, GAPS-THICK,                                                           "", 61023, 32047, 0,  2, ""
GLASS-TYPE-CODE,   0, GAPS-COND,                                                            "", 61024, 32047, 0,  2, ""
GLASS-TYPE-CODE,   0, GAPS-DCOND,                                                           "", 61025, 32047, 0,  2, ""
GLASS-TYPE-CODE,   0, GAPS-VISC,                                                            "", 61026, 32047, 0,  2, ""
GLASS-TYPE-CODE,   0, GAPS-DVISC,                                                           "", 61027, 32047, 0,  2, ""
GLASS-TYPE-CODE,   0, GAPS-DENS,                                                            "", 61028, 32047, 0,  2, ""
GLASS-TYPE-CODE,   0, GAPS-DDENS,                                                           "", 61029, 32047, 0,  2, ""
GLASS-TYPE-CODE,   0, GAPS-PR,                                                              "", 61030, 32047, 0,  2, ""
GLASS-TYPE-CODE,   0, GAPS-DPR,                                                             "", 61031, 32047, 0,  2, ""
GLASS-TYPE-CODE,   0, TSOL,                                                                 "", 13145, 32047, 0,  3, "Solar transmittance of the selected glass type code"
GLASS-TYPE-CODE,   0, TVIS,                                                                 "", 13146, 32047, 0,  3, "visible transmittance defined for selected glass type code"
GLASS-TYPE-CODE,   0, ABS-1,                                                                "", 61034, 32047, 0,  2, ""
GLASS-TYPE-CODE,   0, ABS-2,                                                                "", 61035, 32047, 0,  2, ""
GLASS-TYPE-CODE,   0, ABS-3,                                                                "", 61036, 32047, 0,  2, ""
GLASS-TYPE-CODE,   0, ABS-4,                                                                "", 61037, 32047, 0,  2, ""
GLASS-TYPE-CODE,   0, ABS-5,                                                                "", 61038, 32047, 0,  2, ""
GLASS-TYPE-CODE,   0, RBSOL-HEMI,                        "Solar Reflectance (from the inside)", 12907, 32047, 0,  3, ""
GLASS-TYPE-CODE,   0, RBVIS-HEMI,                      "Visible Reflectance (from the inside)", 12908, 32047, 0,  3, ""
GLASS-TYPE-CODE,   0, SHDCOF,                                                               "", 13132, 32047, 0,  2, ""
GLASS-TYPE-CODE,   0, PANES-TIR,                                                            "", 61018, 32047, 0,  2, ""
GLASS-TYPE-CODE,   0, PANES-EMIS-F,                                                         "", 61019, 32047, 0,  2, ""
GLASS-TYPE-CODE,   0, PANES-EMIS-B,                                                         "", 61020, 32047, 0,  2, ""
GLASS-TYPE-CODE,   0, PANES-THICK,                                                          "", 61017, 32047, 0,  2, ""
GLASS-TYPE-CODE,   0, PANES-COND,                                                           "", 61021, 32047, 0,  2, ""
GLASS-TYPE-CODE,   0, FILMS-COND,                                                           "",     0, 32047, 0,  2, ""
GLASS-TYPE-CODE,   0, U-CENTER,                                                             "", 13143,   759, 0,  2, "The center of glass U-value of the selected glass type code"
GLASS-TYPE-CODE,   0, GAPS-FILL,                                                            "", 61022, 32047, 0,  2, ""
GLASS-TYPE-CODE,   0, PANES-ID,                                                             "", 61016, 32047, 0,  2, ""
GLASS-TYPE-CODE,   0, PICTURE,                                                              "",     0, 32047, 0,  0, ""
GLASS-TYPE-CODE,   0, DRAWING,                                                              "",     0, 32047, 0,  0, ""
SYSTEM,            0, TYPE,                                                             "Type", 19064, 32048, 0,  0, "Type of HVAC unit (determines defaults & applicability of all other Air HVAC parameters)"
SYSTEM,            0, SYSTEM-CONTROL,                                                       "",     0, 32048, 0,  2, ""
SYSTEM,            0, SYSTEM-AIR,                                                           "",     0, 32048, 0,  2, ""
SYSTEM,            0, SYSTEM-FANS,                                                          "",     0, 32048, 0,  2, ""
SYSTEM,            0, SYSTEM-TERMINAL,                                                      "",     0, 32048, 0,  2, ""
SYSTEM,            0, SYSTEM-FLUID,                                                         "",     0, 32048, 0,  2, ""
SYSTEM,            0, SYSTEM-EQUIPMENT,                                                     "",     0, 32048, 0,  2, ""
SYSTEM,            0, *COST,                                                            "Cost", 13156, 32048, 0,  0, ""
SYSTEM,            0, HEAT-SOURCE,                                               "Heat Source", 13489, 32048, 0,  0, "The source of heat for the main heating coils (in the central air distribution system)"
SYSTEM,            0, ZONE-HEAT-SOURCE,                                     "Zone Heat Source", 13389, 32048, 0,  0, "Heat source for the zonal (reheat) coils for all zones in the system"
SYSTEM,            0, PREHEAT-SOURCE,                                         "Preheat Source", 12604, 32048, 0,  0, "The source of heat the preheat coils in the central air distribution system"
SYSTEM,            0, BASEBOARD-SOURCE,                                     "Baseboard Source", 13488, 32048, 0,  0, "The source of heat for the baseboard heaters (for all zones in the system)"
SYSTEM,            0, VARIABLE-T,                                                           "",     0, 32048, 0,  2, ""
SYSTEM,            0, SIZING-RATIO,                                             "Sizing Ratio", 13087, 32048, 0,  2, "Use to deliberately oversize or undersize all of the equipment in the system"
SYSTEM,            0, HEAT-SIZING-RATI,                                    "Heat Sizing Ratio", 13479, 32048, 0,  2, "Used to deliberately oversize or undersize heating coil capacity when autosizing"
SYSTEM,            0, COOL-SIZING-RATI,                                    "Cool Sizing Ratio", 13466, 32048, 0,  2, "Used to deliberately oversize or undersize the cooling coil capacity"
SYSTEM,            0, RETURN-AIR-PATH,                                       "Return Air Path", 13084, 32048, 0,  0, "The route that the return air takes on its way back to the central (system) air handling unit"
SYSTEM,            0, HUMIDIFIER-TYPE,                                       "Humidifier Type", 13159, 32048, 0,  0, "The heat source for humidification in the central air distribution system"
SYSTEM,            0, FUNCTION,                                                             "",     0, 32048, 0,  2, ""
SYSTEM,            0, RETURN-UA,                                              "Return Duct UA", 13100, 32048, 0,  2, "Overall thermal conductivity of the return ductwork"
SYSTEM,            0, HTREC-DW-HEATER,                          "DHW Heater for Heat Recovery", 13529,   696, 0,  0, "Name of the DHW Heater that receives the superheat from the air conditioner"
SYSTEM,            0, DDS-TYPE,                                               "Dual Duct Type", 13097, 32048, 0,  0, "The type of dual-duct system (Single or Dual Fan)"
SYSTEM,            0, MAX-SUPPLY-T,                               "Maximum Supply Temperature", 12269, 32048, 0,  1, "Max temperature for air entering the zones (the highest allowable diffuser air temperature)"
SYSTEM,            0, HEAT-SET-T,                                                 "Heat Set T", 13482, 32048, 0,  1, "Maximum allowable temperature setpoint of the central heating coil"
SYSTEM,            0, HEATING-SCHEDULE,                                     "Heating Schedule", 13485, 32048, 0,  0, "Whether mechanical heating is allowed"
SYSTEM,            0, HEAT-RESET-SCH,                                    "Heat Reset Schedule", 13381, 32048, 0,  0, "A Reset Temp Schedule that defines the heating supply air temp as a fct of outside air temp"
SYSTEM,            0, HEAT-SET-SCH,                                        "Heat Set Schedule", 13378, 32048, 0,  0, "Temperature of the heating supply air temperature (used only if Heating Control = Scheduled)"
SYSTEM,            0, HEAT-CONTROL,                                             "Heat Control", 13486, 32048, 0,  0, "Strategy used to control supply air temperature leaving the systems central heating coil"
SYSTEM,            0, MIN-SUPPLY-T,                               "Minimum Supply Temperature", 12278, 32048, 0,  1, "Minimum temperature of air entering zones (lowest allowable diffuser air temperature)"
SYSTEM,            0, COOL-SET-T,                                       "Cool Set Temperature", 13470, 32048, 0,  1, "The (constant) cooling supply air temperature; used when Cooling Control = Constant"
SYSTEM,            0, COOLING-SCHEDULE,                                     "Cooling Schedule", 13473, 32048, 0,  0, "Whether mechanical cooling is allowed (not incl. natural ventilation or Night Cycle Control)"
SYSTEM,            0, COOL-RESET-SCH,                                    "Cool Reset Schedule", 13220, 32048, 0,  0, "A Reset Temp Schedule that defines the cooling supply air temp as a fct of outside air temp"
SYSTEM,            0, COOL-SET-SCH,                                        "Cool Set Schedule", 13216, 32048, 0,  2, "The temperature of cooling air supply temperature; used when Cooling Control = Scheduled"
SYSTEM,            0, COOL-CONTROL,                                             "Cool Control", 13474, 32048, 0,  0, "Strategy used to control supply air temperature leaving the systems central cooling coil"
SYSTEM,            0, MAX-HUMIDITY,                                         "Maximum Humidity", 13471, 32048, 0,  1, "Highest allowable relative humidity in the return air (from all zones served by the system)"
SYSTEM,            0, MIN-HUMIDITY,                                         "Minimum Humidity", 13484, 32048, 0,  1, "Lowest allowable relative humidity in the return air (from all zones served by the system)"
SYSTEM,            0, BASEBOARD-SCH,                                      "Baseboard Schedule", 12701, 32048, 0,  0, "A Reset Temp Schedule that defines baseboard heat output as fct of outside air temperature "
SYSTEM,            0, ECONO-LIMIT-T,                                                        "", 13448, 32048, 0,  2, "If outside air temp is above this value economizer dampers close to their minimum setting"
SYSTEM,            0, DRYBULB-LIMIT,                                         "Maximum Drybulb", 13448, 32048, 0,  1, "If outside air temp is above this value economizer dampers close to their minimum setting"
SYSTEM,            0, ENTHALPY-LIMIT,                                       "Maximum Enthalpy", 13449, 32048, 0,  1, "Outside air enthalpy above which economizer's outside air damper returns to its min position"
SYSTEM,            0, ECONO-LOCKOUT,                                      "Economizer Lockout", 13454, 32048, 0,  0, "Whether the compressor is allowed to turn on when the economizer is open"
SYSTEM,            0, PREHEAT-T,                                         "Preheat Temperature", 13490, 32048, 0,  1, "Minimum temperature of the air leaving the preheat coil"
SYSTEM,            0, ECONO-LOW-LIMIT,                                  "Economizer Low Limit", 13455, 32048, 0,  1, "Outdoor air (drybulb) temp below which outside dampers are returned to their min position "
SYSTEM,            0, DESC-CTRL-MODE,                                 "Desiccant Control Mode", 13152, 32048, 0,  2, "The control mode of the add-on (integrated) desiccant unit"
SYSTEM,            0, DESC-DEW-SET,                               "Desiccant Exiting Dewpoint", 13153, 32048, 0,  1, "Dewpoint temperature setpoint of air exiting the desiccant unit"
SYSTEM,            0, WS-ECONO,                                        "Water-Side Economizer", 13269, 32048, 0,  0, "Whether or not there is a water side economizer"
SYSTEM,            0, WS-ECONO-MIN-DT,                                       "CW Coil Delta T", 13264, 32048, 0,  1, "Minimum delta T between condenser water loop and entering air"
SYSTEM,            0, RESET-PRIORITY,                                         "Reset Priority", 13219, 32048, 0,  0, "Priority by which supply-air temperature is reset (for Cool Ctrl=warmest or Heat Ctrl=coldest)"
SYSTEM,            0, COOL-MAX-RESET-T,                    "Maximum Cooling Reset Temperature", 13221, 32048, 0,  1, "Maximum temperature that the supply air can be reset to (during cooling)"
SYSTEM,            0, HEAT-MIN-RESET-T,                    "Minimum Heating Reset Temperature", 13383, 32048, 0,  1, "Minimum temperature that the supply air temperature can be reset to during heating"
SYSTEM,            0, NIGHT-CYCLE-FANS,                                     "Night Cycle Fans", 12933, 32048, 0,  0, "Whether one or both supply fans can operate during Night Cycle Control operation"
SYSTEM,            0, SUPPLY-FLOW,                                         "Supply Design cfm", 13424, 32048, 0,  0, "Design air flow rate of the system's supply air fan (in standard cfm)"
SYSTEM,            0, SUPPLY-CFM,                                                 "Supply cfm", 12298, 32048, 0,  0, "Design air flow rate of the system's supply air fan (in standard cfm)"
SYSTEM,            0, RETURN-FLOW,                                         "Return Design cfm", 13426, 32048, 0,  0, "Design air flow rate of the system's return air fan (in standard cfm)"
SYSTEM,            0, RETURN-CFM,                                                 "Return cfm", 12297, 32048, 0,  0, "Design air flow rate of the system's return air fan (in standard cfm)"
SYSTEM,            0, MIN-OUTSIDE-AIR,                                   "Minimum Outside Air", 13088, 32048, 0,  2, "Minimum outside air flow rate (as a fraction of the maximum supply air flow rate)"
SYSTEM,            0, MIN-AIR-SCH,                              "Minimum Outside Air Schedule", 13446, 32048, 0,  0, "The ratio of minimum outside air flow to Supply Air Flow for each hour"
SYSTEM,            0, OA-CONTROL,                                        "Outside Air Control", 13093, 32048, 0,  0, "Type of outside air/economizer control strategy"
; SAC 10/28/01 - Removed certain keywords
; SYSTEM,            0, RECOV-EFF,                             "Recovery Sensible Effectiveness", 13452, 32048, 0,  2, "Design sensible eff. of heat recovery system (at 10°F delta T and design min outside air)"
; SAC 1/16/03 - Added new ERV-related keyword
SYSTEM,            0, RECOVER-EXHAUST,                                      "Recover Exhaust?",     0, 32048, 0,  0, "presence of an energy recovery ventilator"
SYSTEM,            0, *RATED-FLOW,                                         "Cooling Rated cfm", 12916, 32048, 0,  0, "Nominal capacity of system central supply fan; use if different than system design airflow rate"
SYSTEM,            0, *RATED-CFM,                                                           "", 12916, 32048, 0,  2, "Nominal capacity of system central supply fan; use if different than system design airflow rate"
SYSTEM,            0, DUCT-AIR-LOSS,                                           "Duct Air Loss", 13099, 32048, 0,  2, "Fraction of the supply air that is lost from the ductwork (to the Duct Zone)"
SYSTEM,            0, DUCT-DT,                                                  "Duct Delta T", 13101, 32048, 0,  2, "Temp decrease in the hot ducts (and increase in cold ducts) due to heat loss through ducts"
SYSTEM,            0, MAX-OA-FRACTION,                          "Maximum Outside Air Fraction", 13456, 32048, 0,  2, "Max outside air flow rate when the economizer is operating (as a fraction of the supply air)"
SYSTEM,            0, VENT-METHOD,                                               "Ventilation", 13450, 32048, 0,  0, "When windows open: Air Change=Constant vent ;S-G=Ventilation is function of wind speed"
SYSTEM,            0, VENT-TEMP-SCH,                        "Ventilation Temperature Schedule", 13175, 32048, 0,  0, "Hourly indoor drybulb temperatures that natural ventilation attempts to achieve"
SYSTEM,            0, NATURAL-VENT-AC,          "Natural Ventilation Air Changes/Hour (fixed)", 13180, 32048, 0,  1, "Number of air changes per hour when the windows are open"
SYSTEM,            0, MAX-VENT-RATE,                 "Sherman-Grimsrud Air Changes/Hour (max)", 13177, 32048, 0,  1, "Maximum number of air changes per hour due to natural ventilation "
SYSTEM,            0, HOR-VENT-FRAC,       "Sherman-Grimsrud Horizontal Ventilation Area Frac", 13179, 32048, 0,  2, "Fraction of the ventilation area that is in the floor and ceiling"
SYSTEM,            0, FRAC-VENT-AREA,       "Sherman-Grimsrud Total Ventilation Area Fraction", 13178, 32048, 0,  2, "Total leakage area (as a fraction of floor area); typically = 0.6(open window area)/(floor area)"
SYSTEM,            0, NATURAL-VENT-SCH,                             "Ventilation Use Schedule", 13174, 32048, 0,  0, "Specifies when the windows can be open and when they are always closed"
SYSTEM,            0, OPEN-VENT-SCH,                        "Window Open Probability Schedule", 13176, 32048, 0,  0, "Probability that windows will be opened if conditions warrant natural ventilation"
SYSTEM,            0, HSUPPLY-FLOW,                                       "Heating Design cfm", 13425, 32048, 0,  0, "Design air flow rate of the hot air supply fan for the hot duct of a dual-duct dual fan system"
SYSTEM,            0, HSUPPLY-CFM,                                                          "", 13425, 32048, 0,  2, "Design air flow rate of the hot air supply fan for the hot duct of a dual-duct dual fan system"
SYSTEM,            0, HOT-DUCT-DT,                                          "Hot Duct Delta T", 13103, 32048, 0,  2, "Duct air temperature drop when delivering heated air in a dual duct system"
SYSTEM,            0, *HRATED-FLOW,                                        "Heating Rated cfm", 12917, 32048, 0,  0, "Nominal capacity of system heating supply fan;use if different than system design airflow rate"
SYSTEM,            0, *HRATED-CFM,                                                          "", 12917, 32048, 0,  2, "Nominal capacity of system heating supply fan;use if different than system design airflow rate"
SYSTEM,            0, DUCT-UA,                                                "Supply Duct UA", 13100, 32048, 0,  2, "Overall thermal conductivity of the supply ductwork (this is an alternative to Duct Delta T)"
SYSTEM,            0, HOT-DUCT-UA,                                               "Hot Duct UA", 13102, 32048, 0,  2, "Thermal conductivity of the hot duct in a dual duct system (an alternative to the Hot Duct DT)"
SYSTEM,            0, FAN-SCHEDULE,                                     "Cooling Fan Schedule", 12938, 32048, 0,  0, "Specifies when this system's cooling fans can operate"
SYSTEM,            0, FAN-CONTROL,                                       "Cooling Fan Control", 12941, 32048, 0,  2, "Specifies the type of flow reduction or control methods to be simulated"
SYSTEM,            0, SUPPLY-STATIC,                                    "Cooling Static in WG", 13433, 32048, 0,  2, "Total increase in air pressure across the supply air fan (at the design flow rate)"
SYSTEM,            0, SUPPLY-DELTA-T,                                        "Cooling Delta T", 13430, 32048, 0,  2, "Temp rise in the air stream across the supply fan (cooling fan for dual duct dual fan systems)"
SYSTEM,            0, SUPPLY-MECH-EFF,                         "Cooling Mechanical Efficiency", 13117, 32048, 0,  2, "Mechanical efficiency of the supply fan when the motor is located outside the air stream"
SYSTEM,            0, SUPPLY-EFF,                                   "Cooling Total Efficiency", 13436, 32048, 0,  2, "Overall efficiency of the supply air fan and motor (at the design flow rate)"
SYSTEM,            0, SUPPLY-KW/FLOW,                                  "Cooling Design kW/cfm", 12306, 32048, 0,  6, "Full load power consumption of supply fan (per unit of supply air moved per hour)"
SYSTEM,            0, SUPPLY-KW,                                                            "", 12306, 12306, 0,  2, "Full load power consumption of supply fan (per unit of supply air moved per hour)"
SYSTEM,            0, MOTOR-PLACEMENT,                               "Cooling Motor Placement", 13048, 32048, 0,  0, "Whether the supply and return fan motor heat is added to the airstream"
SYSTEM,            0, FAN-PLACEMENT,                                   "Cooling Fan Placement", 12966, 32048, 0,  0, "Whether supply fan is before or after the coils (applies to cooling fan for dual duct systems)"
SYSTEM,            0, RETURN-STATIC,                                     "Return Static in WG", 13435, 32048, 0,  2, "Total increase in air pressure across the return air fan (at the design flow rate)"
SYSTEM,            0, RETURN-DELTA-T,                                         "Return Delta T", 13432, 32048, 0,  2, "Temperature rise in the air stream across the return air fan"
SYSTEM,            0, RETURN-EFF,                                    "Return Total Efficiency", 13438, 32048, 0,  2, "Overall efficiency of the return air fan and motor (at the design flow rate)"
SYSTEM,            0, RETURN-KW/FLOW,                                   "Return Design kW/cfm", 12307, 32048, 0,  6, "Full load power consumption of return fan (per unit of return air moved per hour)"
SYSTEM,            0, RETURN-KW,                                                            "", 12307, 12307, 0,  2, "Full load power consumption of return fan (per unit of return air moved per hour)"
SYSTEM,            0, MAX-FAN-RATIO,                               "Cooling Maximum Fan Ratio", 12930, 32048, 0,  2, "Max allowable air flow through main fan for single duct (or cooling fan for dual duct systems)"
SYSTEM,            0, MIN-FAN-RATIO,                               "Cooling Minimum Fan Ratio", 12923, 32048, 0,  2, "Min allowable air flow through main fan for single duct (or cooling fan for dual duct systems)"
SYSTEM,            0, NIGHT-CYCLE-CTRL,                                  "Night Cycle Control", 12932, 32048, 0,  0, "The behavior of the system fans when the fan schedule is "off" (when Fan Schedule value=0)"
SYSTEM,            0, LOW-SPEED-RATIOS,                                    "Low Speed Ratios ", 13118, 32048, 0,  2, "Ratios of low speed air-flow, energy input, heat and cool capacities to those at high speed"
SYSTEM,            0, FAN-EIR-FPLR,            "Fan Electric Input Ratio = f(Part Load Ratio)", 13441, 32048, 0,  0, "Cubic Curve Fit: Electric Input Ratio as a function of the fan's part load ratio"
SYSTEM,            0, NIGHT-VENT-CTRL,                             "Night Ventilation Control", 12935, 32048, 0,  0, "Behavior of night fans when supply fans are off and Night Cycle Control hasn't cycled fans on"
SYSTEM,            0, NIGHT-VENT-SCH,                             "Night Ventilation Schedule", 12934, 32048, 0,  0, "The hours when night ventilation fans are allowed to run (if the main fans are scheduled off)"
SYSTEM,            0, NIGHT-VENT-DT,                               "Night Ventilation Delta T", 12937, 32048, 0,  2, "Night Vent Fans only operate if outside drybulb temp is < Control Zone temp by this amount"
SYSTEM,            0, NIGHT-VENT-RATIO,                              "Night Ventilation Ratio", 12936, 32048, 0,  2, "Air flow rate, power consumption, and temperature rise in the air due to the night fans"
SYSTEM,            0, HSUPPLY-KW/FLOW,                                 "Heating Design kW/cfm", 13066, 32048, 0,  6, "Full load power consumption of the heating supply fan, per unit heating supply air per hour"
SYSTEM,            0, HSUPPLY-KW,                                          "Heating Supply kW", 13066, 32048, 0,  2, "Full load power consumption of the heating supply fan, per unit heating supply air per hour"
SYSTEM,            0, HSUPPLY-DELTA-T,                                       "Heating Delta T", 13431, 32048, 0,  2, "The temperature rise in the air stream across the heating supply fan"
SYSTEM,            0, HFAN-CONTROL,                                      "Heating Fan Control", 12942, 32048, 0,  2, "Specifies the type of flow reduction or control methods to be simulated"
SYSTEM,            0, HFAN-EIR-FPLR,     "Heating Fan Electric Input Ratio = f(Part Load Rat)", 13442, 32048, 0,  0, "Cubic Curve Fit: Electric Input Ratio as a function of the fan's part load ratio"
SYSTEM,            0, INDOOR-FAN-MODE,                                       "Indoor Fan Mode", 12310, 32048, 0,  0, "Controls the operation of indoor fans within the deadband"
SYSTEM,            0, EXHAUST-FAN-SCH,                                  "Exhaust Fan Schedule", 12940, 32048, 0,  0, "Specifies when this system's central exhaust fans can operate"
SYSTEM,            0, HFAN-SCHEDULE,                                    "Heating Fan Schedule", 12939, 32048, 0,  0, "Specifies when this system's heating fans can operate"
SYSTEM,            0, HSUPPLY-STATIC,                                   "Heating Static in WG", 13434, 32048, 0,  2, "Total increase in air pressure across the heating supply air fan (for dual duct systems)"
SYSTEM,            0, HSUPPLY-EFF,                                  "Heating Total Efficiency", 13437, 32048, 0,  2, "Overall efficiency of the heating supply air fan and motor (at the design flow rate)"
SYSTEM,            0, HSUPPLY-MECH-EFF,                        "Heating Mechanical Efficiency", 12919, 32048, 0,  2, "Mechanical efficiency of heating supply fan when the motor is located outside the air stream"
SYSTEM,            0, HMOTOR-PLACEMENT,                              "Heating Motor Placement", 13049, 32048, 0,  0, "Whether the heating supply fan motor heat is added to the airstream"
SYSTEM,            0, HFAN-PLACEMENT,                                  "Heating Fan Placement", 12971, 32048, 0,  0, "Whether the heating supply fan is before or after the heating coils (in dual duct systems)"
SYSTEM,            0, HMAX-FAN-RATIO,                              "Heating Maximum Fan Ratio", 12931, 32048, 0,  2, "Maximum allowable air flow through heating fan for dual duct systems"
SYSTEM,            0, HMIN-FAN-RATIO,                              "Heating Minimum Fan Ratio", 12924, 32048, 0,  2, "Minimum allowable air flow through heating fan for dual duct systems"
SYSTEM,            0, RETURN-FAN-LOC,                                   "Return Fan Placement", 12990, 32048, 0,  0, "Location of the return fan (if present)"
SYSTEM,            0, RETURN-FAN-CONTR,                                   "Return Fan Control", 12943, 32048, 0,  0, "Specifies the kind of flow reduction or control methods to be simulated"
SYSTEM,            0, RETURN-EIR-FPLR,    "Return Fan Electric Input Ratio = f(Part Load Rat)", 13443, 32048, 0,  0, "Cubic Curve Fit: Electric Input Ratio as a function of the fan's part load ratio"
SYSTEM,            0, RETURN-CAP-RATIO,                                "Return Capacity Ratio", 12912, 32048, 0,  2, "Ratio of the default return (relief) fan capacity to the supply capacity"
SYSTEM,            0, REHEAT-DELTA-T,                                         "Reheat Delta T", 13483, 32048, 0,  1, "Maximum increase in supply air temperature due to system reheat coils"
SYSTEM,            0, INDUCTION-RATIO,                                       "Induction Ratio", 14512, 32048, 0,  2, "The ratio of induced air flow to primary air flow"
SYSTEM,            0, MIN-FLOW-RATIO,                             "Overall Minimum Flow Ratio", 13440, 32048, 0,  2, "Minimum allowable supply air flow rate (as a fraction of the design flow rate)"
SYSTEM,            0, MIN-CFM-RATIO,                                                        "", 13440, 32048, 0,  2, "Minimum allowable supply air flow rate (as a fraction of the design flow rate)"
SYSTEM,            0, HMIN-FLOW-RATIO,                            "Heating Minimum Flow Ratio", 12922, 32048, 0,  2, "Minimum airflow ratio of the hot duct damper controller (VAV only)"
SYSTEM,            0, HMIN-CFM-RATIO,                                                       "", 12922, 32048, 0,  2, "Minimum airflow ratio of the hot duct damper controller at the inlet of the mixing box (VAV only)"
SYSTEM,            0, CMIN-FLOW-RATIO,                            "Cooling Minimum Flow Ratio", 12921, 32048, 0,  2, "The minimum airflow ratio of the cold duct damper controller"
SYSTEM,            0, CMIN-CFM-RATIO,                                                       "", 12921, 32048, 0,  2, "The minimum airflow ratio of the cold duct damper controller"
SYSTEM,            0, MIN-FLOW/AREA,                               "Overall Minimum Flow/Area", 13439, 32048, 0,  2, "Minimum total supply air flow rate per unit floor area (alternative is Min Flow Ratio)"
SYSTEM,            0, MIN-CFM/SQFT,                                                         "", 13439, 32048, 0,  2, "Minimum total supply air flow rate per unit floor area (alternative is Min Flow Ratio)"
SYSTEM,            0, HMIN-FLOW/AREA,                              "Heating Minimum Flow/Area", 12920, 32048, 0,  2, "Minimum allowable heating supply air flow rate per square foot of floor area"
SYSTEM,            0, HMIN-CFM/SQFT,                                                        "", 12920, 32048, 0,  2, "Minimum allowable heating supply air flow rate per square foot of floor area"
SYSTEM,            0, CMIN-FLOW/AREA,                              "Cooling Minimum Flow/Area", 12918, 32048, 0,  2, "Minimum allowable cooling supply air flow rate per square foot of floor area"
SYSTEM,            0, CMIN-CFM/SQFT,                                                        "", 12918, 32048, 0,  2, "Minimum allowable cooling supply air flow rate per square foot of floor area."
SYSTEM,            0, MIN-FLOW-SOURCE,                                   "Minimum Flow Source", 13116, 32048, 0,  0, "Source of makeup air when the supply airflow falls below the Minimum Flow Ratio"
SYSTEM,            0, MIN-CFM-SOURCE,                                                       "", 13116, 32048, 0,  2, "Source of makeup air when the supply airflow falls below the Minimum Flow Ratio"
SYSTEM,            0, REFG-HREC-STAGE2,                                                     "", 14180,   751, 0,  2, "Fraction of total recoverable heat from compressors in holdback mode (2nd stage of heat rec)"
SYSTEM,            0, REFG-DIRECT-FRAC,                                                     "", 14178,   751, 0,  2, "The fraction of case-to-space load that goes directly back to the return air plenum"
SYSTEM,            0, DESC-COIL-HEAD,                                    "Desiccant Coil Head", 14518, 32048, 0,  2, "Pressure drop of fluid through the desiccant coil at design flow"
SYSTEM,            0, DESC-VALVE-TYPE,                                                      "", 14517, 32048, 0,  2, "2Way - flow varies with load; 3Way - bypasses extra fluid to maintain constant loop flowrate"
SYSTEM,            0, DESC-COIL-DT,                                                         "", 14519, 32048, 0,  2, "The temperature change through the coil (at the design conditions)"
SYSTEM,            0, DESC-LOOP,                                              "Desiccant Loop", 14515, 32048, 0,  2, "Name of loop that supplies heat to the desiccant unit"
SYSTEM,            0, HW-COIL-HEAD,                                             "HW Coil Head", 13401, 32048, 0,  1, "Pressure drop of the loop fluid through the coil at the design flowrate"
SYSTEM,            0, HW-VALVE-TYPE,                                           "HW Valve Type", 13402, 32048, 0,  0, "2Way - flow varies with load; 3Way - bypasses extra fluid to maintain constant loop flowrate"
SYSTEM,            0, HW-COIL-DT,                                            "HW Coil Delta T", 13404, 32048, 0,  1, "Temperature change through the coil at design conditions (used to calculate design flowrate)"
SYSTEM,            0, HW-LOOP,                                                       "HW Loop", 19098, 32048, 0,  0, "Name of loop that serves the system hot water coils (Loop Type = Hot Water or Two Pipe)"
SYSTEM,            0, PHW-COIL-HEAD,                                           "PHW Coil Head", 12620, 32048, 0,  1, "Pressure drop of the loop fluid through the preheat coil at the design flow rate"
SYSTEM,            0, PHW-VALVE-TYPE,                                         "PHW Valve Type", 12653, 32048, 0,  0, "2Way - flow varies with load; 3Way - bypasses extra fluid to maintain constant loop flowrate"
SYSTEM,            0, PHW-COIL-DT,                                          "PHW Coil Delta T", 12637, 32048, 0,  1, "Temperature change through the coil at design conditions (used to calculate design flowrate)"
SYSTEM,            0, PHW-LOOP,                                                     "PHW Loop", 19099, 32048, 0,  0, "Name of the loop to which the system's central preheat coil is connected"
SYSTEM,            0, CHW-COIL-HEAD,                                           "CHW Coil Head", 13228, 32048, 0,  1, "Pressure drop through the chilled water coil of the loop fluid (at the design flow rate)"
SYSTEM,            0, CHW-VALVE-TYPE,                                         "CHW Valve Type", 13246, 32048, 0,  0, "2Way - flow varies with load; 3Way - bypasses extra fluid to maintain constant loop flowrate"
SYSTEM,            0, CHW-COIL-DT,                                          "CHW Coil Delta T", 13229, 32048, 0,  1, "Temperature change through the coil at design conditions (used to calculate design flowrate)"
SYSTEM,            0, CHW-LOOP,                                                     "CHW Loop", 13247, 32048, 0,  0, "The loop that serves the system cooling coil (Loop Type must be Chilled Water or Two Pipe)"
SYSTEM,            0, CW-COIL-HEAD,                                "Condenser Water Coil Head", 13256, 32048, 0,  1, "Pressure drop of the loop fluid through the condenser at the design flowrate"
SYSTEM,            0, CW-VALVE,                                             "Isolation Valve?", 13258, 32048, 0,  0, "Whether an isolation valve regulates flow rate through condenser by cycling with compressor"
SYSTEM,            0, CW-COIL-DT,                               "Condenser Water Coil Delta T", 13257, 32048, 0,  1, "Temperature change through the coil at design conditions (used to calculate design flowrate)"
SYSTEM,            0, CW-LOOP,                                          "Condenser Water Loop", 19096, 32048, 0,  0, "If Condenser Type=Water Cooled, CW Loop is required & must be attached to Cooling Tower"
SYSTEM,            0, WSE-COIL-HEAD,                         "Water-Side Economizer Coil Head", 13265, 32048, 0,  1, "Pressure drop of the loop fluid through the coil at the design flowrate"
SYSTEM,            0, WSE-VALVE-TYPE,                       "Water-Side Economizer Valve Type", 13267, 32048, 0,  0, "2Way - flow varies with load; 3Way - bypasses extra fluid to maintain constant loop flowrate"
SYSTEM,            0, WSE-COIL-DT,                        "Water-Side Economizer Coil Delta T", 13266, 32048, 0,  1, "Temperature change through the coil at design conditions (used to calculate design flowrate)"
SYSTEM,            0, WSE-LOOP,                                   "Water-Side Economizer Loop", 19097, 32048, 0,  0, "Name of loop that serves the water-side economizer (Loop Type = Chilled Water or 2 Pipe)"
SYSTEM,            0, BBRD-COIL-HEAD,                                    "Baseboard Coil Head", 12718, 32048, 0,  1, "Pressure drop of the loop fluid through the baseboards at the design flowrate"
SYSTEM,            0, BBRD-VALVE-TYPE,                                  "Baseboard Valve Type", 13147, 32048, 0,  0, "2Way - flow varies with load; 3Way - bypasses extra fluid to maintain constant loop flowrate"
SYSTEM,            0, BBRD-COIL-DT,                                   "Baseboard Coil Delta T", 13098, 32048, 0,  1, "Temperature change through the coil at design conditions (used to calculate design flowrate)"
SYSTEM,            0, BBRD-LOOP,                                              "Baseboard Loop", 19100, 32048, 0,  0, "Name of loop that serves baseboard coils (Loop Type must be Hot Water, 2Pipe or Steam)"
SYSTEM,            0, DHW-LOOP,                                                     "DHW Loop", 19139, 32048, 0,  0, "Name of the Loop that provides Domestic Hot Water to the zones in this system"
SYSTEM,            0, REFG-CW-HEAD,                                    "Refrig Condenser Head", 14208,   751, 0,  2, "Pressure drop of fluid through the refrigerant condenser"
SYSTEM,            0, REFG-CW-VALVE,                                                        "", 14207,   751, 0,  0, "2Way - flow varies with load; 3Way - bypasses extra fluid to maintain constant loop flowrate"
SYSTEM,            0, REFG-CW-DT,                                                           "", 14209,   751, 0,  2, "Temperature change through the condenser at the design conditions"
SYSTEM,            0, REFG-CW-LOOP,                       "Refrig Water-Cooled Condenser Loop", 19102,   751, 0,  0, "Name of loop that removes condenser heat (must be Condenser Water)"
SYSTEM,            0, COOLING-CAPACITY,                                     "Cooling Capacity", 12285, 32048, 0,  0, "Total cooling capacity (at ARI conditions) of the system's chilled water or DX cooling coil"
SYSTEM,            0, COOL-CAP-FT,                                                          "", 13282, 32048, 0,  0, "Bi-Quadratic Curve Fit: Cooling Capacity as a function of entering temperatures"
SYSTEM,            0, COOLING-EIR,                              "Cooling Electric Input Ratio", 12383, 32048, 0,  4, "Electric Input Ratio (inverse of COP) of the cooling unit at ARI rated conditions"
SYSTEM,            0, COOL-EIR-FT,                                                          "", 13276, 32048, 0,  0, "Quadratic Curve Fit: EIR as a function of temp of water entering condenser & leaving chilled"
SYSTEM,            0, COOL-EIR-FPLR,                                                        "", 13279, 32048, 0,  0, "Cubic Curve Fit: Electric Input Ratio as a function of the part load ratio"
SYSTEM,            0, COOL-SH-CAP,                                          "Cool SH Capacity", 12286, 32048, 0,  0, "Sensible heat removal capacity of the system's air cooling device at ARI rated conditions"
SYSTEM,            0, COOL-SH-FT,                                                           "", 13290, 32048, 0,  0, "Bi-Quadratic Curve Fit: Sensible Cooling Capacity as a function of entering temperatures"
SYSTEM,            0, COIL-BF,                                            "Coil Bypass Factor", 13472, 32048, 0,  3, "Cooling coil full load bypass factor (at the ARI rating conditions)"
SYSTEM,            0, COIL-BF-FFLOW,                                                        "", 13294, 32048, 0,  0, "Cubic Equation: coil Bypass Factor as a function of total supply air flow rate"
SYSTEM,            0, COIL-BF-FCFM,                                                         "", 13294, 32048, 0,  0, "Cubic Equation: coil Bypass Factor as a function of total supply air flow rate"
SYSTEM,            0, COIL-BF-FT,                                                           "", 13293, 32048, 0,  0, "Bi-Quadratic Equation: coil Bypass Factor as a fct of entering air wet-bulb and dry-bulb temps"
SYSTEM,            0, COOL-CTRL-RANGE,                                    "Cool Control Range", 13213, 32048, 0,  1, "The throttling range of the cooling coil controller"
SYSTEM,            0, MIN-UNLOAD-RATIO,                                 "Minimum Unload Ratio", 13272, 32048, 0,  2, "PLR at which compressor unloading stops and hot gas bypass or cycling begins"
SYSTEM,            0, MIN-HGB-RATIO,                            "Minimum Hot Gas Bypass Ratio", 13273, 32048, 0,  2, "The part load ratio below which compressor cycling begins"
SYSTEM,            0, MAX-COND-RCVRY,                             "Maximum Condenser Recovery", 13254, 32048, 0,  2, "Max fraction of condenser heat that can be recovered (and used to replace active heating)"
SYSTEM,            0, CRANKCASE-HEAT,                                         "Crankcase Heat", 13274, 32048, 0,  2, "Electricity consumed to heat the crankcase of direct expansion (DX) compressors"
SYSTEM,            0, OUTSIDE-FAN-ELEC,                                 "Outside Fan Electric", 13253, 32048, 0,  2, "power consumption of outside fan (condenser fan when cooling; evaporator fan when heating)"
SYSTEM,            0, OUTSIDE-FAN-T,                                 "Outside Fan Temperature", 13252, 32048, 0,  1, "Outside air (drybulb) temp below which the condenser fan is not permitted to operate"
SYSTEM,            0, OUTSIDE-FAN-MODE,                                     "Outside Fan Mode", 13476, 32048, 0,  0, "Whether the outside fan cycles with the load or remains on"
SYSTEM,            0, COMPRESSOR-TYPE,                                       "Compressor Type", 12385, 32048, 0,  0, "Specifies the different speeds at which the compressor can operate"
SYSTEM,            0, HEATING-CAPACITY,                                     "Heating Capacity", 12275, 32048, 0,  0, "Heating capacity (ar ARI conditions) of the system heating HVAC system"
SYSTEM,            0, HEAT-CAP-FT,                                                          "", 13245, 32048, 0,  0, "Bi-Quadratic eqn: Heating Capacity of heat pump as fct of OA drybulb & entering air drybulb"
SYSTEM,            0, HEATING-EIR,                              "Heating Electric Input Ratio", 12384, 32048, 0,  4, "Electric Input Ratio (inverse of COP) for the heat pump at ARI rated conditions"
SYSTEM,            0, HEAT-EIR-FT,                                                          "", 13413, 32048, 0,  0, "Quadratic Curve Fit: EIR as a function of temp of entering water & outdoor drybulb"
SYSTEM,            0, HEAT-EIR-FPLR,                                                        "", 13416, 32048, 0,  0, "Cubic Curve Fit: Electric Input Ratio as a function of the part load ratio"
SYSTEM,            0, HP-SUPP-HT-CAP,                          "HP Supplemental Heat Capacity", 13193, 32048, 0,  0, "Supplemental heating capacity of a heat pump"
SYSTEM,            0, HP-SUPP-SOURCE,                                 "HP Supplemental Source", 13200, 32048, 0,  0, "The source of heat for the heat pump's supplemental heating"
SYSTEM,            0, MIN-HP-T,                                  "Minimum HP Heat Temperature", 13230, 32048, 0,  1, "Outside air (drybulb) temperature below which the heat pump is turned off"
SYSTEM,            0, MAX-HP-SUPP-T,                     "Maximum HP Supplemental Temperature", 13231, 32048, 0,  1, "Outside air drybulb temp below which heat pump supplemental heating is allowed"
SYSTEM,            0, DEFROST-TYPE,                                             "Defrost Type", 13237, 32048, 0,  0, "Whether heat pump is defrosted via electric resistance coils or a reverse cycle"
SYSTEM,            0, RESIST-CAP-RATIO,               "Resistive Capacity / HP Capacity Ratio", 13232, 32048, 0,  2, "Ratio of the default return (relief) fan capacity to the supply capacity"
SYSTEM,            0, DEFROST-CTRL,                                          "Defrost Control", 13238, 32048, 0,  0, "The defrost control method for the heat pump "
SYSTEM,            0, DEFROST-T,                                 "Maximum Defrost Temperature", 13239, 32048, 0,  1, "Outdoor air drybulb temp below which heat pump defrosts itself (when in the heating mode)"
SYSTEM,            0, FURNACE-AUX,                                    "Furnace Fuel Auxiliary", 13409, 32048, 0,  1, "For oil furnaces, aux consumed when furnace has load; for gas, consumed when no load"
SYSTEM,            0, FURNACE-HIR,                                  "Furnace Heat Input Ratio", 13408, 32048, 0,  4, "The ratio of fuel energy consumption to heating energy produced"
SYSTEM,            0, FURNACE-HIR-FPLR,        "Furnace Heat Input Ratio = f(Part Load Ratio)", 13411, 32048, 0,  0, "Cubic Curve Fit: the Heat Input Ratio as a function of the part load ratio"
SYSTEM,            0, COOL-FT-MIN,                  "Minimum Bypass Extrapolation Temperature", 13249, 32048, 0,  1, "Minimum outside air dry bulb temp for which the cooling Curve Fits are valid"
SYSTEM,            0, FURNACE-OFF-LOSS,                                     "Furnace Off Loss", 13412, 32048, 0,  0, "Cubic equation:fraction of unused furnace capacity that's an induced load as fct of OA drybulb"
SYSTEM,            0, HCOIL-WIPE-FFLOW,                  "Heating Coil Wipe = f(Cooling Flow)", 13382, 32048, 0,  0, ""
SYSTEM,            0, HCOIL-WIPE-FCFM,                                                      "", 13382, 32048, 0,  2, ""
SYSTEM,            0, CRANKCASE-MAX-T,                         "Maximum Crankcase Temperature", 13275, 32048, 0,  2, "Outdoor air (drybulb) temp above which the crankcase heater is not allowed to operate"
SYSTEM,            0, REFG-KW-FTCOND,           "Refrigeration kW = f(Condensing Temperature)", 13364,   751, 0,  0, "Cubic eqn: refrigerator power consumption as a function of the condensing temperature"
SYSTEM,            0, REFG-KW-FPLR,               "Refrigeration kW = f(Compressor Part Load)", 13367,   751, 0,  0, "Cubic eqn: refrigerator power consumption as a function of compressor part load ratio"
SYSTEM,            0, REFG-FAN-PWR-FPL,         "Refrig Condenser kW = f(Condenser Part Load)", 14186,   751, 0,  0, "Cubic eqn: power consumption of condenser fan as a function of condenser part load ratio"
SYSTEM,            0, T8-FWB1WB6,                    "Exit Temperature = f(Outdr WB & Ret WB)", 13196, 32048, 0,  0, "Bi-Quadratic eqn: supply air drybulb (before direct evap cooler) as fct of wetbulb of exh & OA"
SYSTEM,            0, T8PL-FWB1WB6,          "Exit Temperature, 25% pl = f(Outdr WB & Ret WB)", 13312, 32048, 0,  0, "Bi-Quadratic eqn: ln(1000*supply air Humidity Ratio) as fct of exh & OA wetbulb @ 25% PLR"
SYSTEM,            0, HR8-FWB1WB6,                "Exit Humidity Ratio = f(Outdr WB & Ret WB)", 13236, 32048, 0,  0, "Bi-Quadratic eqn: ln(1000*Humidity Ratio of supply air) as fct of exh & OA wetbulb"
SYSTEM,            0, HR8PL-FWB1WB6,      "Exit Humidity Ratio, 25% pl = f(Outdr WB & Ret WB)", 13323, 32048, 0,  0, "Bi-Quadratic eqn: ln(1000*supply air Humidity Ratio) as fct of exh & OA wetbulb at 25% PLR"
SYSTEM,            0, QREG-FWB1WB6,               "Regeneration Energy = f(Outdr WB & Ret WB)", 13324, 32048, 0,  0, "Bi-Quadratic eqn: regeneration energy as function of exhaust & OA wetbulb temps"
SYSTEM,            0, QREGPL-FWB1WB6,    "Regeneration Energy, 25%, pl = f(Outdr WB & Ret WB)", 13324, 32048, 0,  0, "Bi-Quadratic eqn: regeneration energy as a fct of exhaust & OA wetbulb at 25% PLR"
SYSTEM,            0, DESC-T-FTW,         "Exit Temperature = f(Entering Temp & Humidity Rat)", 13148, 32048, 0,  0, "Bi-Quadratic eqn: exit temperature as function of entering air temperature and humidity ratio"
SYSTEM,            0, DESC-W-FTW,           "Exit Humidity Ratio = f(Entering Temp & Hum Rat)", 13149, 32048, 0,  0, ""
SYSTEM,            0, DESC-GAS-FTW,       "Gas Usage = f(Entering Temperature & Humidity Rat)", 13150, 32048, 0,  0, "Bi-Quadratic eqn: fuel consumption as fct of entering air temperature and humidity ratio"
SYSTEM,            0, DESC-KW-FTW,          "Auxiliary kW = f(Entering Temperature & Hum Rat)", 13151, 32048, 0,  0, "Bi-Quadratic eqn: auxiliary power as fct of entering air temperature and humidity ratio"
SYSTEM,            0, HEAT-EXCH-EFF,                             "Heat Exchange Effectiveness", 13321, 32048, 0,  2, "The effectiveness of the sensible heat exchanger"
SYSTEM,            0, HEAT-EXCH-DELP,                                  "Heat Exchange Delta P", 13322, 32048, 0,  2, "Supply air pressure drop across the sensible heat exchanger"
SYSTEM,            0, MIN-SUPPLY-SCH,                                "Minimum Supply Schedule", 13215, 32048, 0,  0, "Lowest allowable temperature for air entering the zones (diffuser air temperature)"
SYSTEM,            0, EVAP-PCC-ELEC,                          "Evaporative Condenser Electric", 13262, 32048, 0,  2, "Electricity consumption of the evaporative precooling unit "
SYSTEM,            0, DESC-NOM-FLOW,                                  "Desiccant Nominal Flow", 13154, 32048, 0,  0, ""
SYSTEM,            0, DESC-NOM-CFM,                                                         "", 13154, 32048, 0,  2, ""
SYSTEM,            0, RES-EVAP-COOLER,                        "Residential Evaporative Cooler", 13302, 32048, 0,  0, "Whether a residential system has an add-on (direct) evaporative cooling unit"
SYSTEM,            0, RES-EVAP-CL-FLOW,                    "Residential Evaporative Cool Flow", 13303, 32048, 0,  0, "Air side capacity of the residential evaporative cooler (expressed in standard CFM)"
SYSTEM,            0, RES-EVAP-CL-CFM,                                                      "", 13303, 32048, 0,  2, "Air side capacity of the residential evaporative cooler (expressed in standard CFM)"
SYSTEM,            0, EVAP-CL-TYPE,                                  "Evaporative Cooler Type", 13458, 13458, 0,  0, "Type of evaporative cooling element (Direct and/or Indirect or None)"
SYSTEM,            0, EVAP-CL-KW/FLOW,                   "Evaporative Cooling Fan and Pump kW", 13300, 32048, 0,  5, "Power consumption of evaporative cooling pump and secondary fan (per unit air flow)"
SYSTEM,            0, EVAP-CL-KW,                                                           "", 13300, 32048, 0,  3, "Power consumption of evaporative cooling pump and secondary fan (per unit air flow)"
SYSTEM,            0, EVAP-CL+M-SUP,                            "Evaporative + Main Cool Coil", 13306, 32048, 0,  0, "Whether the evaporative cooler can operate in conjunction with mechanical cooling"
SYSTEM,            0, EVAP-CL+REC-RA,                      "Return Air Used At Indirect Stage", 13297, 32048, 0,  0, "Whether return air is used for the secondary air-stream of the indirect evaporative cooler"
SYSTEM,            0, DIRECT-EFF,                    "Evaporative Cooler Direct Effectiveness", 13298, 32048, 0,  2, "Rated (nominal) effectiveness of the direct evaporative cooler"
SYSTEM,            0, INDIR-EFF,                   "Evaporative Cooler Indirect Effectiveness", 13299, 32048, 0,  2, "Rated (nominal) effectiveness of the indirect evaporative cooler"
SYSTEM,            0, EVAP-CL-LIMIT-T,                                    "Drybulb High Limit", 13314, 32048, 0,  1, "Outside air (drybulb) temperature above which the evaporative cooler is turned off"
SYSTEM,            0, DIRECT-EFF-FFLOW,                   "Direct Effectiveness = f(air flow)", 13313, 32048, 0,  0, "Cubic eqn: effectiveness of direct evaporative cooling as a function of the air flow"
SYSTEM,            0, DIRECT-EFF-FCFM,                                                      "", 13313, 32048, 0,  0, "Cubic eqn: effectiveness of direct evaporative cooling as a function of the air flow"
SYSTEM,            0, INDIR-EFF-FFLOW,                  "Indirect Effectiveness = f(air flow)", 13317, 32048, 0,  2, "Cubic eqn: effectiveness of indirect evaporative cooling as a function of the air flow"
SYSTEM,            0, INDIR-EFF-FCFM,                                                       "", 13317, 32048, 0,  2, "Cubic eqn: effectiveness of indirect evaporative cooling as a function of the air flow"
SYSTEM,            0, EVAP-CL-AIR,                                 "Evaporative Flow Fraction", 13464, 32048, 0,  2, "Fraction of design supply air that is allowed to pass through the evaporative cooler"
SYSTEM,            0, CONDENSER-TYPE,                                         "Condenser Type", 12386, 32048, 0,  0, "Air Cooled=heat exchanger & condenser; Water Cooled=cooling tower & condenser loop"
SYSTEM,            0, WS-ECONO-XEFF,                             "WS Economizer Effectiveness", 13263, 32048, 0,  2, "Design coil effectiveness of heat exchanger between cooling tower water loop and CW loop "
SYSTEM,            0, COIL-BF-FPLR,                                                         "", 13295, 32048, 0,  2, "Cubic Equation: coil Bypass Factor as a function of part load ratio"
SYSTEM,            0, COOL-EIR-FRPM,                                                        "", 13280, 32048, 0,  0, "Quadratic Curve Fit: Electric Input Ratio as a function of compressor rpm"
SYSTEM,            0, COOL-WH-FT,        "Waste Heat to Cooling Capacity = f(Outdoor Drybulb)", 13399, 32048, 0,  0, "Quadratic eqn:availability of Cooling Waste Heat as fct of entering wetbulb & outside drybulb"
SYSTEM,            0, COOL-WH-FRPM,       "Waste Heat to Cooling Capacity = f(Compressor RPM)", 13419, 32048, 0,  0, "Quadratic eqn: waste heat generated by engine as a function of the of the compressor RPM"
SYSTEM,            0, OUTSIDE-FAN-CFLT,              "Outdoor Fan Power = f(Cool PLR, osa db)", 13255, 32048, 0,  0, "Bi-Quadratic:power consumption of outdoor fan as fct of cooling PLR and cond. entering temp"
SYSTEM,            0, HEAT-EIR-FRPM,                                                        "", 13417, 32048, 0,  0, "Cubic Curve Fit: Electric Input Ratio as a function of heat pump engine RPM"
SYSTEM,            0, HEAT-WH-FT,        "Waste Heat to Heating Capacity = f(Outdoor Drybulb)", 13421, 32048, 0,  0, "Quadratic eqn: availability of Heating Waste Heat as fct of outside drybulb temp"
SYSTEM,            0, HEAT-WH-FRPM,       "Waste Heat to Heating Capacity = f(Compressor RPM)", 13422, 32048, 0,  0, "Quadratic eqn: waste heat generated by engine as a function of the of the compressor RPM"
SYSTEM,            0, OUTSIDE-FAN-HFLT,              "Outdoor Fan Power = f(Heat PLR, osa db)", 13243, 32048, 0,  0, "Bi-Quadratic:power consumption of outdoor fan as fct of heating PLR and OA drybulb temp"
SYSTEM,            0, HEAT-CLOSS-FPLR,                                                      "", 13395, 32048, 0,  0, "Quadratic eqn: cycling fraction as a function of cycling part load ratio"
SYSTEM,            0, COOL-CLOSS-FPLR,                                                      "", 13288, 32048, 0,  0, "Quadratic Equation: cycling PLR/cycling fraction as a function of cycling PLR"
SYSTEM,            0, DEFROST-FRAC-FT,     "Defrost Runtime Fraction = f(Outdoor drybulb, WB)", 13240, 32048, 0,  0, "Bi-Quadratic eqn: defrost run time fraction as a fct of outside air wetbulb and drybulb temps"
SYSTEM,            0, COOL-CAP-FRPM,                                                        "", 13289, 32048, 0,  0, "Quadratic Equation: compressor cooling capacity as a function of motor RPM"
SYSTEM,            0, HEAT-CAP-FRPM,                                                        "", 13396, 32048, 0,  0, "Quadratic eqn: heating capacity as a function of the heat pump engine RPM"
SYSTEM,            0, COOL-EIR-LS-FT,                      "Cooling EIR f(T) at Minimum Speed", 13281, 32048, 0,  0, "Bi-Quadratic Curve Fit: EIR as a function of entering wetbulb temp & outside drybulb temp"
SYSTEM,            0, HEAT-EIR-LS-FT,                      "Heating EIR f(T) at Minimum Speed", 13418, 32048, 0,  0, "Bi-Quadratic eqn: heating EIR (at min RPM) as fct of entering air wetbulb and OA drybulb"
SYSTEM,            0, EVAP-PCC-EFF,                                  "Condenser Effectiveness", 13260, 32048, 0,  2, "The effectiveness of the evaporative pre-cooling unit"
SYSTEM,            0, EVAP-PCC-SCH,                                       "Condenser Schedule", 13261, 32048, 0,  0, "Specifies when the evaporatively-precooled condenser for air cooled units can operate"
SYSTEM,            0, HEAT-CLOSS-MIN,                    "Heating Min Cycling Part Load Ratio", 13400, 32048, 0,  2, "Min cycling PLR for which the Total Heating Capacity f(PLR) operating curve is valid"
SYSTEM,            0, COOL-CLOSS-MIN,                    "Cooling Min Cycling Part Load Ratio", 13227, 32048, 0,  2, "Min cycling PLR for which the Total Cooling Capacity f(PLR) operating curve is valid"
SYSTEM,            0, COOL-WASTE-HEAT,                     "Fraction of Heat Input to Cooling", 13398, 32048, 0,  2, "Fraction of heat input to gas cooling unit (or cooling load for electric) that is recoverable heat"
SYSTEM,            0, HEAT-WASTE-HEAT,                     "Fraction of Heat Input to Heating", 13420, 32048, 0,  2, "Fraction of heating load/input that's available for recovery (at full load and rated conditions)"
SYSTEM,            0, UNIT-PUMP-ELEC,                                         "Unit Pump Elec", 14513, 32048, 0,  2, "Pump power for the Gas Heat Pump, or supplemental boiler (per Btu Cooling Capacity)"
SYSTEM,            0, UNIT-AUX-KW,                                         "Unit Auxiliary kW", 14514, 32048, 0,  2, "Power consumption of Gas Heat Pump's auxiliaries (e.g., controls), that operate continuously"
SYSTEM,            0, FURNACE-AUX-KW,                             "Furnace Electric Auxiliary", 13410, 32048, 0,  2, "Electrical auxiliary power consumed by the furnace when it is on"
SYSTEM,            0, WASTE-HEAT-USE,                                         "Waste Heat Use", 13397, 32048, 0,  0, "The end use of the waste heat that is recovered from the Gas Heat Pump"
SYSTEM,            0, HEAT-RPM-LIMITS,                                   "Heating RPM Limits ", 13387, 32048, 0,  0, "Minimum allowable speed (RPM) of the heat pump engine during heating"
SYSTEM,            0, COOL-RPM-LIMITS,                                   "Cooling RPM Limits ", 13225, 32048, 0,  0, "Minimum engine RPM during cooling (for natural-gas-fired engine-driven heat pumps)"
SYSTEM,            0, PREHEAT-CAPACITY,                                     "Preheat Capacity", 12519, 32048, 0,  0, "Total capacity of the preheat coil at the design conditions"
SYSTEM,            0, ZONE-HW-LOOP,                                             "Zone HW Loop", 14600, 32048, 0,  2, "Name of the loop that provides heating to zonal reheat coils, baseboards, etc."
SYSTEM,            0, HW-CAP-FDT,                                                           "", 13391, 32048, 0,  0, "Quadratic eqn: coil capacity as fct of temp difference between entering air and entering water"
SYSTEM,            0, HW-CAP-FCFM,                                                          "", 13392, 32048, 0,  0, "Quadratic eqn: coil capacity as a function of supply air flow rate"
SYSTEM,            0, WS-ECONO-KW/FLOW,                                                     "", 14521, 32048, 0,  2, "Additional fan power required to overcome the air pressure drop through the economizer coil "
SYSTEM,            0, WS-ECONO-FAN-DT,                                                      "", 14520, 32048, 0,  2, "Additional fan temperature rise required to overcome air pressure drop thru economizer coil "
SYSTEM,            0, DESC-CHILLER,                                        "Dessicant Chiller", 14516, 32048, 0,  2, "Name of Chiller/Heater that provides heat to (and cools) the desiccant"
SYSTEM,            0, CHW-CAP-FEWBEWT,                                                      "", 13284, 32048, 0,  0, "Bi-Quadratic eqn: coil capacity as a fct of entering wetbulb temp and entering water temp"
SYSTEM,            0, CHW-CAP-FCFM,                                                         "", 13285, 32048, 0,  0, "Quadratic Equation: chilled water coil capacity as a function of the supply air flow rate"
SYSTEM,            0, REFG-WALKIN-LOAD,                                                     "",     0, 32048, 0,  2, ""
SYSTEM,            0, REFG-WALKIN-SCH,       "Schedule for Refrigeration Walkin Box Load Frac",   663, 32048, 0,  2, ""
SYSTEM,            0, REFG-WALKIN-LOC,                                                      "",     0, 32048, 0,  2, ""
SYSTEM,            0, DUAL-TEMP-DT,                                                         "",     0, 32048, 0,  2, ""
SYSTEM,            0, DUAL-ENTHALPY-DH,                                                     "",     0, 32048, 0,  2, ""
SYSTEM,            0, ECONO-MAX-W,                                                          "",     0, 32048, 0,  2, ""
SYSTEM,            0, ECONO-MIN-W,                                                          "",     0, 32048, 0,  2, ""
SYSTEM,            0, OA-SIZING-METHOD,                                     "OA Sizing Method",     0, 32048, 0,  0, "The method to calculate the design and hourly minimum outside air flow rate fraction for multi-zone systems"
SYSTEM,            0, ECONO-SCHEDULE,                                                       "",     0, 32048, 0,  0, ""
SYSTEM,            0, HW-CAP-FGPM,                                                          "", 13394, 32048, 0,  0, "Quadratic eqn: coil capacity as a function of hot water flow rate"
SYSTEM,            0, CHW-CAP-FGPM,                                                         "", 13287, 32048, 0,  0, "Quadratic Equation: chilled water coil capacity as a function of the chilled water flow rate"
SYSTEM,            0, HUMIDIFIER-LOC,                                                       "", 14532, 32048, 0,  0, "The location of supply air humidifier"
SYSTEM,            0, SIZING-OPTION,                                           "Sizing Option", 13108, 32048, 0,  0, "Whether supply fan capacity sized based on sum of peak loads or peak load for entire bldg"
SYSTEM,            0, REFG-SIZING-RAT,                                          "Sizing Ratio", 13594,   751, 0,  2, "Used to adjust the capacity of all compressors in the system"
SYSTEM,            0, REFG-COMP-CAP,             "Capacity of Refrigeration Compressor Group ", 13595,   751, 0,  0, "The installed compressor capacity at the corresponding operating temperature range"
SYSTEM,            0, REFG-COMP-EER,                  "EER of Refrigeration Compressor Group ", 13598,   751, 0,  3, "The efficiency of the compressor unit at the corresponding temperature level"
SYSTEM,            0, REFG-COMP-GROUP,       "Circuit Type of Refrigeration Compressor Group ", 13601,   751, 0,  0, "Whether the compressors are multiplexed or serve separate refrigeration circuits"
SYSTEM,            0, REFG-FAN-KW,                         "Refrigeration Condenser Fan Power", 14213,   751, 0,  2, "Power consumption of fans of air cooled condensers or cooling towers"
SYSTEM,            0, REFG-PUMP-KW,                       "Refrigeration Condenser Pump Power", 14214,   751, 0,  2, "Total power consumption of cooling tower condenser water pumps"
SYSTEM,            0, REFG-MIN-COND-T,           "Refrigeration Minimum Condensing Temperture", 14212,   751, 0,  1, "OA thermostat setpoint:modulates condenser (or cooling tower) to maintain condensing temp"
SYSTEM,            0, REFG-COND-TYPE,                    "Refrigeration System Condenser Type", 13356,   751, 0,  0, "The type of condenser serving the refrigerated casework"
SYSTEM,            0, REFG-MAX-HTREC,                                 "Total Recoverable Heat", 13362,   751, 0,  0, "Maximum amount of compressor heat that is recoverable"
SYSTEM,            0, REFG-HTREC-GROUP,                               "Heat Recovery Grouping", 13361,   751, 0,  0, "Governs how many condensers heat can be recovered from when a space heating load exists"
SYSTEM,            0, REFG-HTREC-UNITS,     "Heat Recovery of Refrigeration Compressor Group ", 13604,   751, 0,  0, "Whether compressor that serves the corresponding evaporator temp allows heat recovery"
SYSTEM,            0, REFG-HTREC-T,           "Refrigeration Heat Recovery Condenser Setpoint", 13363,   751, 0,  1, "Condensing setpoint temperature during the heat recovery mode"
SYSTEM,            0, REFG-SETPT-VAL,                                                       "", 14211,   751, 0,  1, "The condenser setpoint temperature"
SYSTEM,            0, DESICCANT,                                              "Desiccant Type", 14001, 32048, 0,  0, "The type of add-on (integrated) desiccant unit"
SYSTEM,            0, DESICCANT-AIR,                                 "Desiccant Flow Fraction", 14002, 32048, 0,  2, "Air flow rate through the desiccant (as a fraction of the design supply air flow rate)"
SYSTEM,            0, DESC-HEAT-SOURCE,                               "Desiccant Regeneration", 14003, 32048, 0,  0, "The source of heat used to regenerate (dry out) the desiccant and provide space heating"
SYSTEM,            0, OA-FROM-SYSTEM,                                "Outside Air From System", 12910, 32048, 0,  0, "Name of another system that supplies make-up air to this system"
SYSTEM,            0, DUCT-ZONE,                                                   "Duct Zone", 13104, 32048, 0,  0, "Name of the zone that contains the supply and return ducts (and receives duct thermal losses and air leakage)"
SYSTEM,            0, SYSTEM-REPORTS,                                         "System Reports", 13107, 32048, 0,  0, "Whether the standard verification and summary reports are produced as output"
SYSTEM,            0, MSTR-ELEC-METER,                                 "Master Electric Meter", 12205, 32079, 0,  0, "Name of Electric Meter that tallies all of the unassigned system electric consumption"
SYSTEM,            0, MSTR-FUEL-METER,                                     "Master Fuel Meter", 13589, 32079, 0,  0, "Name of Fuel Meter that tallies all of the unassigned system fuel consumption"
SYSTEM,            0, LIGHT-ELEC-METER,                         "Area Lighting Electric Meter", 12865, 32079, 0,  0, "Name of the Electric Meter that tallies the system's Area Lighting electric consumption"
SYSTEM,            0, TASK-ELEC-METER,                          "Task Lighting Electric Meter", 12925, 32079, 0,  0, "Electric Meter that tallies the system's Task Lighting electricity consumption"
SYSTEM,            0, EQUIP-ELEC-METER,                             "Electric Equipment Meter", 12926, 32079, 0,  0, "Name of Electric Meter that tallies the system's Equipment electricity consumption"
SYSTEM,            0, SOURCE-ELEC-METE,                                "Source Electric Meter", 13329, 32079, 0,  0, "Name of Electric Meter that tallies the zone's 'source' electric energy consumption"
SYSTEM,            0, HEAT-ELEC-METER,                          "Space Heating Electric Meter", 13545, 32079, 0,  0, "Name of Electric Meter that tallies the system's Space Heating electricity consumption"
SYSTEM,            0, COOL-ELEC-METER,                          "Space Cooling Electric Meter", 13585, 32079, 0,  0, "Name of Electric Meter that tallies the system's Space Cooling electric consumption"
SYSTEM,            0, HTREJ-ELEC-METER,                        "Heat Rejection Electric Meter", 13332, 32079, 0,  0, "Name of Electric Meter that tallies the electric energy required for the system's heat rejection"
SYSTEM,            0, AUX-ELEC-METER,                 "Pumps and Miscellaneous Eletric Meters", 13333, 32079, 0,  0, "Name of Electric Meter that tallies the system's auxiliary electric energy (e.g., pumps)"
SYSTEM,            0, VENT-ELEC-METER,                        "Ventilation Fan Electric Meter", 13586, 32079, 0,  0, "Electric Meter that tallies the system Ventilation Fans electricity consumption"
SYSTEM,            0, REFG-ELEC-METER,                          "Refrigeration Electric Meter", 13335, 32079, 0,  0, "Name of Electric Meter that tallies the zone's refrigeration electric energy consumption"
SYSTEM,            0, SUPP-ELEC-METER,                      "Supplemental Heat Electric Meter", 13587, 32079, 0,  0, "Electric Meter that tallies the system's electric consumption for supplemental heating"
SYSTEM,            0, DHW-ELEC-METER,                                     "DHW Electric Meter", 13588, 32079, 0,  0, "Name of Electric Meter that tallies the system's DHW heater electricity consumption"
SYSTEM,            0, SOURCE-FUEL-METE,                                    "Source Fuel Meter", 13339, 32079, 0,  0, "Name of Electric Meter that tallies the zone's 'source' fuel consumption"
SYSTEM,            0, HEAT-FUEL-METER,                              "Space Heating Fuel Meter", 13590, 32079, 0,  0, "Name of Electric Meter that tallies the system's Space Heating fuel consumption"
SYSTEM,            0, COOL-FUEL-METER,                              "Space Cooling Fuel Meter", 13591, 32079, 0,  0, "Name of the Fuel Meter that tallies the fuel consumption of this system's cooling system"
SYSTEM,            0, SUPP-FUEL-METER,                          "Supplemental Heat Fuel Meter", 13592, 32079, 0,  0, "Electric Meter that tallies the system's fuel consumption for supplemental heating"
SYSTEM,            0, DHW-FUEL-METER,                                         "DHW Fuel Meter", 13593, 32079, 0,  0, "Name of Electric Meter that tallies the system's DHW heater fuel consumption"
SYSTEM,            0, GET-IT-INTO-SYS,                                                      "",     0, 32048, 0,  2, ""
SYSTEM,            0, CONTROL-ZONE,                                             "Control Zone", 14249, 32048, 0,  2, "The zone that is the easiest to heat in the winter and the hardest to cool in the summer"
SYSTEM,            0, REFG-COND-SIZE,                                                       "", 14202,   751, 0,  2, "The capacities of the condensers; definition & units depends on the Condenser Type"
SYSTEM,            0, REFG-ASH-KW,                                                          "", 29080,   751, 0,  2, "Rated power consumption of the anti-sweat heaters (at corresponding operating temp)"
SYSTEM,            0, REFG-COND-CTRL,        "Refrigeration Condenser Capacity Control Method", 14601,   751, 0,  0, ""
SYSTEM,            0, REFG-SETPT-CTRL,                                                      "", 14210,   751, 0,  0, "The method used to control the refrigerators' condensers"
SYSTEM,            0, REFG-ASH-LOWW,                                                        "", 14196,   751, 0,  2, "Absolute humidity of return air temperature at which the anti-sweat heaters begin to operate"
SYSTEM,            0, REFG-ASH-HIGHW,                                                       "", 14197,   751, 0,  2, "Absolute humidity of return air temp at which the anti-sweat heaters operate at full capacity"
SYSTEM,            0, REFG-HREC-STAGE1,                                                     "", 14179,   751, 0,  2, "Fraction of total recoverable heat from compressors in normal mode (1st stage of heat rec)"
SYSTEM,            0, REFG-KW-HR-FTC,         "Refrigeration Compressor kW f(Heat Recovery T)", 14181,   751, 0,  0, "Cubic equation: compressor power as function of condensing temperature"
SYSTEM,            0, REFG-AUX-FRAC,                                                        "", 14198,   751, 0,  2, "Fraction of anti-sweat heater & Auxiliary power that is a load on casework compressors"
SYSTEM,            0, REFG-AMB-COND-FT,     "Refrig Ambient Ctrl Condenser Active Frac f(OAT)", 14185,   751, 0,  0, "Cubic eqn: fraction of condenser that is active as a fct of ambient temperature"
SYSTEM,            0, REFG-COND-CAP-FT,                                                     "", 14184,   751, 0,  0, "Bi-Quadratic eqn: Evap condenser capacity as fct of condensing wetbulb temp & OA wetbulb"
; SAC 1/16/03 - Added new ERV-related keywords
SYSTEM,            0, ERV-RECOVER-TYPE,                      "Energy Recovery Ventilator Type",     0, 32048, 0,  0, "the type of energy recovery ventilator"
SYSTEM,            0, ERV-OA-FLOW,                              "ERV - Design Outdoor Airflow",     0, 32048, 0,  2, "the design outdoor airflow at which the ERV is rated"
SYSTEM,            0, ERV-EXH-FLOW,                             "ERV - Design Exhaust Airflow",     0, 32048, 0,  2, "the design exhaust airflow at which the ERV is rated"
SYSTEM,            0, ERV-PURGE,                    "ERV - Frac OA Increase to Purge Ht Wheel",     0, 32048, 0,  4, "the fractional increase in the design outdoor airflow that purges the heat wheel"
SYSTEM,            0, ERV-HX-CONFIG,                      "ERV - Heat Exchanger Configuration",     0, 32048, 0,  0, "the heat exchanger configuration"
SYSTEM,            0, ERV-SENSIBLE-EFF,                         "ERV - Sensible Effectiveness",     0, 32048, 0,  4, "the sensible effectiveness at the design airflow"
SYSTEM,            0, ERV-SEN-FILM-RES,   "ERV - Frac Sensible HX Resistance Due to Air Films",     0, 32048, 0,  4, "the fraction of the design heat-exchanger resistance (1/UA) that is due to the air films"
SYSTEM,            0, ERV-SEN-FILM-EXP,  "ERV - Exponent Varying Sensible Air Film Resistance",     0, 32048, 0,  4, "the exponent used to vary an air film resistance as a function of the hourly airflow"
SYSTEM,            0, ERV-LATENT-EFF,                             "ERV - Latent Effectiveness",     0, 32048, 0,  4, "the latent effectiveness at the design airflow"
SYSTEM,            0, ERV-LAT-FILM-RES,     "ERV - Frac Latent HX Resistance Due to Air Films",     0, 32048, 0,  4, "the fraction of the design latent heat exchanger resistance (1/UA) that is due to the air films"
SYSTEM,            0, ERV-LAT-FILM-EXP,    "ERV - Exponent Varying Latent Air Film Resistance",     0, 32048, 0,  4, "the exponent used to vary an latent air film resistance as a function of the hourly airflow"
SYSTEM,            0, ERV-RUN-CTRL,                             "How ERV Operation Determined",     0, 32048, 0,  0, "determines when the ERV will operate"
SYSTEM,            0, ERV-SCHEDULE,                                   "ERV Operation Schedule",     0, 32048, 0,  0, "the schedule that defines when the ERV operates"
SYSTEM,            0, OA-EXHAUST-DT,                                                  "ERV - ",     0, 32048, 0,  2, "the temperature differential between the outside air and exhaust air streams"
SYSTEM,            0, OA-EXHAUST-DH,                                                  "ERV - ",     0, 32048, 0,  2, "the enthalpy differential between the outside air and exhaust air streams"
SYSTEM,            0, ERV-RECOVER-MODE,                                               "ERV - ",     0, 32048, 0,  0, "determines when the ERV will operate"
SYSTEM,            0, ERV-TEMP-CTRL,                                                  "ERV - ",     0, 32048, 0,  0, "the mechanism used to control the make-up air temperature leaving the ERV"
SYSTEM,            0, OA-HEAT-SETPT-T,              "ERV - Heating Make-up Air Setpoint Temp.",     0, 32048, 0,  1, "the outlet make-up air temperature setpoint when the air handler is in the heating mode (return temperature less than required mixed-air temperature)"
SYSTEM,            0, OA-COOL-SETPT-T,              "ERV - Cooling Make-up Air Setpoint Temp.",     0, 32048, 0,  1, "the outlet make-up air temperature setpoint when the air handler is in the cooling mode (return temperature greater than required mixed-air temperature)"
SYSTEM,            0, ERV-CAP-CTRL,                                   "ERV - Capacity Control",     0, 32048, 0,  0, "describes the ERV capacity control mechanism"
SYSTEM,            0, ERV-HX-KW,                                                      "ERV - ",     0, 32048, 0,  2, "the power consumption of the heat-exchanger"
SYSTEM,            0, ERV-HX-KW/FLOW,                                                 "ERV - ",     0, 32048, 0,  6, "the power consumption of the heat-exchanger per unit of flow"
SYSTEM,            0, ERV-HX-KW-FPLR,                                                 "ERV - ",     0, 32048, 0,  0, "a curve that modifies the heat-exchanger power consumption as a function of part load ratio"
SYSTEM,            0, ERV-FANS,                                                       "ERV - ",     0, 32048, 0,  0, "whether an ERV uses its own fans to overcome the pressure drop of the heat-exchange media, or the HVAC supply/return fans"
SYSTEM,            0, ERV-FAN-EFF,                                                    "ERV - ",     0, 32048, 0,  4, "the mechanical efficiency of the ERV fans"
SYSTEM,            0, ERV-MOTOR-CLASS,                                                "ERV - ",     0, 32048, 0,  0, "the motor class (efficiency) of the ERV fans"
SYSTEM,            0, ERV-FAN-KW-FFLOW,                                               "ERV - ",     0, 32048, 0,  0, "a curve that modifies the hourly fan power consumption as a function of airflow"
SYSTEM,            0, ERV-OA-KW,                                                      "ERV - ",     0, 32048, 0,  2, "the power consumption of the outside air makeup fan at the design outdoor airflow at which the ERV is rated"
SYSTEM,            0, ERV-OA-KW/FLOW,                                                 "ERV - ",     0, 32048, 0,  6, "the power consumption of the outside air makeup fan, normalized to the design outdoor airflow at which the ERV is rated"
SYSTEM,            0, ERV-OA-STATIC,                                                  "ERV - ",     0, 32048, 0,  3, "the static pressure drop of the air flowing through the outside-air side of the heat-exchanger at the design outdoor airflow at which the ERV is rated"
SYSTEM,            0, ERV-STATIC-EXP,                                                 "ERV - ",     0, 32048, 0,  3, "an exponent that modifies the outside or exhaust static pressure drop as a function of airflow"
SYSTEM,            0, ERV-EXH-KW,                                                     "ERV - ",     0, 32048, 0,  2, "the power consumption of the outside air makeup fan at the design exhaust airflow at which the ERV is rated"
SYSTEM,            0, ERV-EXH-KW/FLOW,                                                "ERV - ",     0, 32048, 0,  6, "the power consumption of the outside air makeup fan, normalized to the design exhaust airflow at which the ERV is rated"
SYSTEM,            0, ERV-EXH-STATIC,                                                 "ERV - ",     0, 32048, 0,  3, "the static pressure drop of the air flowing through the outside-air side of the heat-exchanger at the design exhaust airflow at which the ERV is rated"
SYSTEM,            0, ERV-FROST-CTRL,               "ERV Condensate/Frost Control Methodology",     0, 32048, 0,  0, "the condensate/frost control methodology"
SYSTEM,            0, ERV-PREHEAT-CTRL,             "ERV Preheat Temperature Control Strategy",     0, 32048, 0,  0, "the preheat temperature control strategy"
SYSTEM,            0, ERV-PREHEAT-T,                        "ERV Preheat Setpoint Temperature",     0, 32048, 0,  1, "the preheat setpoint temperature"
SYSTEM,            0, ERV-PREHEAT-SRC,                                 "ERV Preheat Coil Type",     0, 32048, 0,  0, "the type of preheat coil"
SYSTEM,            0, PREHEAT-AIR-DT,                                                 "ERV - ",     0, 32048, 0,  2, "the design air temperature rise through the preheat coil"
SYSTEM,            0, PREHEAT-HW-DT,                                                  "ERV - ",     0, 32048, 0,  2, "the design water temperature drop through the preheat coil"
SYSTEM,            0, PREHEAT-INLET-DT,                                               "ERV - ",     0, 32048, 0,  2, "the design temperature differential between the hot-water entering the preheat coil and the air entering the preheat coil"
; SAC 1/16/03 - Added other miscellaneous keywords
SYSTEM,            0, AIR/TEMP-CONTROL,                                                     "",     0, 32048, 0,  0, ""
SYSTEM,            0, NUM-COOL-STAGES,                                                      "",     0, 32048, 0,  0, ""
SYSTEM,            0, COOL-STAGES,                                                          "",     0, 32048, 0,  4, ""
SYSTEM,            0, COOL-STAGES-DT,                                                       "",     0, 32048, 0,  4, ""
SYSTEM,            0, NUM-HEAT-STAGES,                                                      "",     0, 32048, 0,  0, ""
SYSTEM,            0, HEAT-STAGES,                                                          "",     0, 32048, 0,  4, ""
SYSTEM,            0, HEAT-STAGES-DT,                                                       "",     0, 32048, 0,  4, ""
SYSTEM,            0, SIZING-METHOD,                                                        "",     0, 32048, 0,  0, ""
SYSTEM,            0, FLOW/CAPACITY,                                                        "",     0, 32048, 0,  1, ""
SYSTEM,            0, MAX-FLOW/CAPACIT,                                                     "",     0, 32048, 0,  1, ""
SYSTEM,            0, MIN-FLOW/CAPACIT,                                                     "",     0, 32048, 0,  1, ""
SYSTEM,            0, ZONE-NAMES,                                                           "",     0, 32048, 0,  2, "The names of all zones served by this system (each zone must appear in one system)"
ZONE,              0, TYPE,                                                        "Zone Type", 12263, 32055, 0,  0, "Whether the zone is Conditioned, Unconditioned or a Plenum"
ZONE,              0, ZONE-AIR,                                                             "",     0, 32055, 0,  2, ""
ZONE,              0, ZONE-CONTROL,                                                         "",     0, 32055, 0,  2, ""
ZONE,              0, ZONE-FANS,                                                            "",     0, 32055, 0,  2, ""
ZONE,              0, MIN-FLOW-RATIO,                                     "Minimum Flow Ratio", 12249, 32055, 0,  2, "Minimum allowable supply air flow rate (as a fraction of the design flow rate)"
ZONE,              0, MIN-CFM-RATIO,                                                        "", 12249, 32055, 0,  2, "Minimum allowable supply air flow rate (as a fraction of the design flow rate)"
ZONE,              0, MIN-FLOW-SCH,                                                         "", 60000, 32055, 0,  2, "Scheduled minimum allowable total supply air flow rate per sqare foot of floor area"
ZONE,              0, MIN-CFM-SCH,                                                          "", 60000, 32055, 0,  2, "Scheduled minimum allowable total supply air flow rate per sqare foot of floor area"
ZONE,              0, HEATING-CAPACITY,                                     "Heating Capacity", 13051, 32055, 0,  0, "Heating capacity (ar ARI conditions) of the zonal heating HVAC system"
ZONE,              0, COOLING-CAPACITY,                                     "Cooling Capacity", 13050, 32055, 0,  0, "Total zonal cooling capacity (at ARI conditions) of the chilled water or DX cooling coil"
ZONE,              0, COOL-SH-CAP,                                          "Cool SH Capacity", 13052, 32055, 0,  0, "Sensible heat removal capacity of the zone's air cooling device at ARI rated conditions"
ZONE,              0, MULTIPLIER,                                                 "Multiplier", 12246,   769, 0,  1, "Number of zones in the facility identical to this one, and served by the same HVAC system"
ZONE,              0, MAX-HEAT-RATE,                                       "Maximum Heat Rate", 13030, 32055, 0,  0, "Maximum zonal heating rate, not including baseboards (limits PowerDOE's sizing calculation)"
ZONE,              0, MAX-COOL-RATE,                                       "Maximum Cool Rate", 13045, 32055, 0,  0, "Maximum net cooling rate for the zone (limits PowerDOE's sizing calculation)"
ZONE,              0, BASEBOARD-RATING,                                   "Baseboard Capacity", 13061, 32055, 0,  0, "Rated baseboard heating capacity for the zone (required for baseboard simulation)"
ZONE,              0, PANEL-LOSS-RATIO,                                                     "", 60013, 32055, 0,  2, "Heat loss from the zonal heating panel (as a fraction of the panel's heating capacity)"
ZONE,              0, FUNCTION,                                                             "",     0, 32055, 0,  2, ""
ZONE,              0, *RATED-FLOW,                                                "Rated Flow", 13014, 32055, 0,  0, "Nominal capacity of zonal supply air fan, use if different than zonal design air flow rate"
ZONE,              0, *RATED-CFM,                                                           "", 13014, 32055, 0,  2, "Nominal capacity of zonal supply air fan, use if different than zonal design air flow rate"
ZONE,              0, AIR-CHANGES/HR,                                                       "", 12259, 32055, 0,  2, "Design cooling supply air flow rate (number of times air in the zone is replaced in an hour)"
ZONE,              0, FLOW/AREA,                                                 "Design Flow", 12247, 32055, 0,  1, "Minimum design supply air flow rate for the zone (standard cfm per unit zone floor area)"
ZONE,              0, CFM/SQFT,                                                             "", 12261, 32055, 0,  2, "Minimum design supply air flow rate for the zone (standard cfm per unit zone floor area)"
ZONE,              0, OA-CHANGES,                                        "Outdoor Air Changes", 13020, 32055, 0,  2, "Minimum zonal outside air flow rate(# of times per hour total volume of air is replaced)"
ZONE,              0, OA-FLOW/PER,                                   "Outdoor Air Flow/Person", 12248, 32055, 0,  1, "Minimum flow rate of outside air (standard cfm) per zone occupant, at peak occupancy"
ZONE,              0, OA-CFM/PER,                                                           "", 12248, 32055, 0,  2, "Minimum flow rate of outside air (standard cfm) per zone occupant, at peak occupancy"
ZONE,              0, OUTSIDE-AIR-FLOW,                                     "Outdoor Air Flow", 13018, 32055, 0,  0, "Minimum zonal outside air flow rate (in standard cfm); this method takes precedence"
ZONE,              0, OUTSIDE-AIR-CFM,                                                      "", 13018, 32055, 0,  2, "Minimum zonal outside air flow rate (in standard cfm); this method takes precedence"
ZONE,              0, ASSIGNED-FLOW,                                            "Zone Airflow", 12257, 32055, 0,  0, "Assigned flow rate into zone"
ZONE,              0, ASSIGNED-CFM,                                                         "", 12257, 32055, 0,  2, ""
ZONE,              0, EXHAUST-FLOW,                                         "Exhaust Air Flow", 13021, 32055, 0,  1, "Flow rate of air that is directly exhausted from the zone (in standard cfm)"
ZONE,              0, EXHAUST-CFM,                                                          "", 13021, 32055, 0,  2, "Flow rate of air that is directly exhausted from the zone (in standard cfm)"
ZONE,              0, EXHAUST-STATIC,                            "Exhaust Air Static Pressure", 13023, 32055, 0,  2, "Total pressure produced by the zonal exhaust fan (in inches of water)"
ZONE,              0, EXHAUST-EFF,                        "Exhaust Air Efficiency (mech+elec)", 13024, 32055, 0,  2, "The combined efficiency of the zonal exhaust fan and motor (at design conditions)"
ZONE,              0, EXHAUST-KW/FLOW,                               "Exhaust Air kW per Flow", 13022, 32055, 0,  6, "Electrical energy consumption of the zonal exhaust fan (per standard cfm of exhaust air)"
ZONE,              0, EXHAUST-KW,                                                           "", 13022, 13022, 0,  2, "Electrical energy consumption of the zonal exhaust fan (per standard cfm of exhaust air)"
ZONE,              0, SS-FLOW-T-SCH,                                                        "", 60028,   753, 0,  2, "If the temp of Next To space is above this, air doesn't flow into that space from the Sunspace"
ZONE,              0, SS-FLOW-SCH,                                                          "", 60029,   753, 0,  2, "A scheduled multiplier on the air flow across an Interior Wall in a Sunspace"
ZONE,              0, SS-VENT-CST,                                                          "", 60030,   753, 0,  2, "Used to calculate the # of outside air changes per hour in Sunspace due to natural convection"
ZONE,              0, SS-VENT-WND,                                                          "", 60031,   753, 0,  2, "Used to calculate the # of outside air changes per hour in Sunspace due to natural convection"
ZONE,              0, SS-VENT-TEMP,                                                         "", 60032,   753, 0,  2, "Used to calculate the # of outside air changes per hour in Sunspace due to natural convection"
ZONE,              0, SS-VENT-T-SCH,                                                        "", 60033,   753, 0,  2, "If the Sunspace air is above this temperature, ventilation is allowed"
ZONE,              0, SS-VENT-SCH,                                                          "", 60034,   753, 0,  2, "On-off schedule that specifies when a Sunspace can be ventilated"
ZONE,              0, SS-VENT-LIMIT-T,                                                      "", 60035,   753, 0,  2, "If outside air drybulb is below this scheduled temperature, ventilation is allowed"
ZONE,              0, SS-VENT-KW/FLOW,                                                      "", 60036,   753, 0,  2, "Electric consumption of the Sunspace vent fan, per unit air flow (i.e., in units of kW/cfm)"
ZONE,              0, HASSIGNED-FLOW,                                                       "", 12258, 32055, 0,  0, "Design heating supply air flow rate into the zone (in standard cfm)"
ZONE,              0, HASSIGNED-CFM,                                                        "", 12258, 32055, 0,  2, "Design heating supply air flow rate into the zone (in standard cfm)"
ZONE,              0, HFLOW/AREA,                                                           "", 12256, 32055, 0,  2, "Minimum design heating zonal supply air flow rate (standard cfm per unit floor area)"
ZONE,              0, HCFM/SQFT,                                                            "", 12256, 32055, 0,  2, ""
ZONE,              0, HAIR-CHANGES/HR,                                                      "", 12260, 32055, 0,  2, "Design heating supply air flow rate (number of times air in the zone is replaced in an hour)"
ZONE,              0, MIN-FLOW/AREA,                                            "Minimum Flow", 13015, 32055, 0,  2, "Minimum total supply air flow rate per square foot of floor area (alternative is Min Flow Ratio)"
ZONE,              0, MIN-CFM/SQFT,                                                         "", 13015, 32055, 0,  2, "Minimum total supply air flow rate per square foot of floor area (alternative is Min Flow Ratio)"
ZONE,              0, HMIN-FLOW/AREA,                                                       "", 12262, 32055, 0,  2, "Minimum allowable heating supply air flow rate per square foot of floor area."
ZONE,              0, HMIN-CFM/SQFT,                                                        "", 12262, 32055, 0,  2, "Minimum allowable heating supply air flow rate per square foot of floor area."
ZONE,              0, CMIN-FLOW/AREA,                                                       "", 12261, 32055, 0,  2, "Minimum allowable cooling supply air flow rate per square foot of floor area."
ZONE,              0, CMIN-CFM/SQFT,                                                        "", 12261, 32055, 0,  2, "Minimum allowable cooling supply air flow rate per square foot of floor area."
ZONE,              0, DESIGN-HEAT-T,                              "Heating Design Temperature", 12252, 32055, 0,  1, "Desired space T, used to calculate supply airflow rate required for peak zonal heating loads"
ZONE,              0, HEAT-TEMP-SCH,                                "Heat Thermostat Schedule", 12181, 32055, 0,  0, "A schedule that specifies the setpoint of the zone cooling thermostat"
ZONE,              0, DESIGN-COOL-T,                              "Cooling Design Temperature", 12251, 32055, 0,  1, "Desired space T, used to calculate supply airflow rate required for peak zonal cooling loads"
ZONE,              0, COOL-TEMP-SCH,                                "Cool Thermostat Schedule", 12178, 32055, 0,  0, "A schedule that specifies the setpoint of the zone cooling thermostat"
ZONE,              0, BASEBOARD-CTRL,                                      "Baseboard Control", 13063, 32055, 0,  0, "Thermostatic=based on zone air T; Outdoor Reset=based on outdoor air T, via reset schedule"
ZONE,              0, THERMOSTAT-TYPE,                                                      "", 60003, 32055, 0,  2, "2-Position=on/off; Proportional=capacity is linear f(DT); Reverse Action=for VAV's"
ZONE,              0, THROTTLING-RANGE,                                                     "", 60004, 32055, 0,  2, "Degrees that room temp must go thru for heat/cool output to go from zero to the maximum"
ZONE,              0, ZONE-FAN-FLOW,                                                        "", 60001, 32055, 0,  2, "The capacity of the fan in the terminal box of a Powered Induction Unit (PIU) system"
ZONE,              0, ZONE-FAN-CFM,                                                         "", 60001, 32055, 0,  2, "The capacity of the fan in the terminal box of a Powered Induction Unit (PIU) system"
ZONE,              0, ZONE-FAN-KW/FLOW,                                                     "", 60002, 32055, 0,  2, "Power consumption of the fan in the terminal box of a PIU system (kW per cfm)"
ZONE,              0, ZONE-FAN-KW,                                                          "", 60002, 60002, 0,  2, "Power consumption of the fan in the terminal box of a PIU system (kW per cfm)"
ZONE,              0, ZONE-FAN-T-SCH,                          "Zone Fan Temperature Schedule", 13055, 32055, 0,  0, "Space air temperature at which the fan (in the terminal box of a PIU system) turns on"
ZONE,              0, ZONE-FAN-RATIO,                                         "Zone Fan Ratio", 13056, 32055, 0,  2, "Zone air flow rate, expressed as a fraction of the primary supply air flow rate"
ZONE,              0, SIZING-OPTION,                                           "Sizing Option", 12250, 32055, 0,  0, "Method of sizing equipment & air flow rates; Adjust Loads=more detailed calculation"
ZONE,              0, TROM-VENT-SCH,                                                        "",     0, 32055, 0,  2, ""
ZONE,              0, FLOOR-MULTIPLIER,                                     "Floor Multiplier", 12245,   769, 0,  1, "The number of floors in the facility that are identical, and served by the same HVAC system"
ZONE,              0, TERMINAL-TYPE,                                                        "", 13013, 32055, 0,  0, "(PIU only) VAV=VAV or CV reheat; Series=primary & 2nd air; Parallel=2nd air only"
ZONE,              0, REHEAT-DELTA-T,                                         "Reheat Delta T", 13026, 32055, 0,  1, "Maximum increase in supply air temperature due to zonal reheat coils"
ZONE,              0, INDUCED-AIR-ZONE,                                     "Induced Air Zone", 13054, 32055, 0,  0, "Another zone, whose return air is the source of this zone's secondary air stream"
ZONE,              0, HOT-AIR-FRACTION,                                                     "",     0, 32055, 0,  2, ""
ZONE,              0, REFG-ZONE-LOAD,                                  "Evaporator Temp Range", 13623,   751, 0,  0, "Total cooling to zone due to air from open refrigeration cases, and heat radiating to the cases"
ZONE,              0, REFG-ZONE-SHR,                                         "Sens Heat Ratio", 13626,   751, 0,  3, "Ratio of sensible to total heat removed from zone by refrigeration cases"
ZONE,              0, REFG-DISCHARGE-T,                                     "Case Temperature", 13635,   751, 0,  1, "Temperature of air inside the refrigeration casework"
ZONE,              0, REFG-EVAP-T,                                                          "", 60019,   751, 0,  2, "The three dewpoint temperatures at which the evaporator operates"
ZONE,              0, REFG-SENS-SCH,                                                        "", 60020,   751, 0,  2, "Used to simulate covers on refrigeration casework that inhibit sensible cooling effect to zone"
ZONE,              0, REFG-LAT-SCH,                                                         "", 60021,   751, 0,  2, "Used to simulate covers on refrigeration casework that inhibit latent cooling effect to zone"
ZONE,              0, REFG-ZONE-DES-T,                                                      "", 60022,   751, 0,  2, "Drybulb temperature of zone air at which the refrigeration casework is rated (typically 75°F)"
ZONE,              0, REFG-ZONE-DES-RH,                                                     "", 60023,   751, 0,  2, "Relative Humidity of zone air at which the refrigeration casework is rated (typically 55%)"
ZONE,              0, REFG-AUX-KW,                                                          "", 60024,   751, 0,  2, "Rated electric consumption of equipment within the refrigeration casework (lights, fan, etc.)"
ZONE,              0, REFG-AUX-SCH,                                                         "", 60026,   751, 0,  2, "On-off schedule, applies to both auxiliary electrical and auxiliary heat loads"
ZONE,              0, REFG-DEF-MECH,                                            "Defrost Type", 13629,   751, 0,  0, "Resistance=electric coils; Freon=hot gas defrost; Time-Off=timed off cycle; No Defrost = none"
ZONE,              0, REFG-DEF-EFF,                                                         "", 60027,   751, 0,  2, "Efficiency of the defroster (if one exists, see Refrigeration Defrost Type)"
ZONE,              0, REFG-DEF-CTRL,                                         "Defrost Control", 13632,   751, 0,  0, "The type of defrost control (controls when defroster activates)"
ZONE,              0, REFG-AUX-HEAT,                                                        "", 60025,   751, 0,  2, "Rated fuel consumption associated with refrigeration (e.g., resurfacing ice rinks with hot water)"
ZONE,              0, ZONE-REPORTS,                                                         "", 60005, 32055, 0,  2, "Whether or not PowerDOE includes summary reports for this zone in the output reports"
ZONE,              0, MSTR-ELEC-METER,                                 "Master Electric Meter", 13608, 32079, 0,  0, "Name of Electric Meter that tallies all of the unassigned zonal electric consumption"
ZONE,              0, MSTR-FUEL-METER,                                     "Master Fuel Meter", 13617, 32079, 0,  0, "Name of Fuel Meter that tallies all of the unassigned zonal fuel consumption"
ZONE,              0, LIGHT-ELEC-METER,                         "Area Lighting Electric Meter", 13609, 32079, 0,  0, "Name of the Electric Meter that tallies the zone's Area Lighting electric consumption"
ZONE,              0, TASK-ELEC-METER,                           "Task Lighting Eletric Meter", 13610, 32079, 0,  0, "Electric Meter that tallies the zone's Task Lighting electricity consumption"
ZONE,              0, EQUIP-ELEC-METER,                             "Electric Equipment Meter", 13611, 32079, 0,  0, "Name of Electric Meter that tallies the zone's Equipment electricity consumption"
ZONE,              0, SOURCE-ELEC-METE,                                                     "", 60014, 32079, 0,  0, "Name of Electric Meter that tallies the zone's 'source' electric energy consumption"
ZONE,              0, HEAT-ELEC-METER,                          "Space Heating Electric Meter", 13612, 32079, 0,  0, "Name of Electric Meter that tallies the zone's Space Heating electricity consumption"
ZONE,              0, COOL-ELEC-METER,                          "Space Cooling Electric Meter", 13613, 32079, 0,  0, "Name of Electric Meter that tallies the zone's Space Cooling electric consumption"
ZONE,              0, HTREJ-ELEC-METER,                                                     "", 60015, 32079, 0,  0, "Name of Electric Meter that tallies the electric energy required for the zone's heat rejection"
ZONE,              0, AUX-ELEC-METER,                                                       "", 60016, 32079, 0,  0, "Name of Electric Meter that tallies the zone's auxiliary electric energy (e.g., pumps)"
ZONE,              0, VENT-ELEC-METER,                       "Ventilation Fans Electric Meter", 13614, 32079, 0,  0, "Electric Meter that tallies the zone's Ventilation Fans electricity consumption"
ZONE,              0, REFG-ELEC-METER,                                                      "", 60017, 32079, 0,  0, "Name of Electric Meter that tallies the zone's refrigeration electric energy consumption"
ZONE,              0, SUPP-ELEC-METER,                      "Supplemental Heat Electric Meter", 13616, 32079, 0,  0, "Electric Meter that tallies the zone's electric consumption for supplemental heating"
ZONE,              0, DHW-ELEC-METER,                                     "DHW Electric Meter", 13615, 32079, 0,  0, "Name of Electric Meter that tallies the zone's DHW heater electricity consumption"
ZONE,              0, ADD1-ELEC-METER,                                                      "",     0, 32079, 0,  0, ""
ZONE,              0, SOURCE-FUEL-METE,                                                     "", 60018, 32079, 0,  0, "Name of Electric Meter that tallies the zone's 'source' fuel consumption"
ZONE,              0, HEAT-FUEL-METER,                              "Space Heating Fuel Meter", 13618, 32079, 0,  0, "Name of Electric Meter that tallies the zone's Space Heating fuel consumption"
ZONE,              0, COOL-FUEL-METER,                              "Space Cooling Fuel Meter", 13619, 32079, 0,  0, "Name of the Fuel Meter that tallies the fuel consumption of this zone's cooling system"
ZONE,              0, SUPP-FUEL-METER,                          "Supplemental Heat Fuel Meter", 13620, 32079, 0,  0, "Electric Meter that tallies the zone's fuel consumption for supplemental heating"
ZONE,              0, DHW-FUEL-METER,                                         "DHW Fuel Meter", 13621, 32079, 0,  0, "Name of Electric Meter that tallies the zone's DHW heater fuel consumption"
ZONE,              0, ADD1-FUEL-METER,                                                      "",     0, 32079, 0,  0, ""
ZONE,              0, HMIN-FLOW-RATIO,                            "Heating Minimum Flow Ratio", 13027, 32055, 0,  2, "Minimum airflow ratio of the hot duct damper controller at the inlet of the mixing box (VAV only)"
ZONE,              0, HMIN-CFM-RATIO,                                                       "", 13027, 32055, 0,  2, "Minimum airflow ratio of the hot duct damper controller at the inlet of the mixing box (VAV only)"
ZONE,              0, HMIN-FLOW-SCH,                                                        "", 60010, 32055, 0,  2, "Scheduled Cooling Min flow Ratio of the hot duct damper at the inlet of the mixing box"
ZONE,              0, HMIN-CFM-SCH,                                                         "", 60010, 32055, 0,  2, "Scheduled Cooling Min flow Ratio of the hot duct damper at the inlet of the mixing box"
ZONE,              0, CMIN-FLOW-RATIO,                            "Cooling Minimum Flow Ratio", 13041, 32055, 0,  2, "The min airflow ratio of the cold duct damper controller at the inlet of the mixing box"
ZONE,              0, CMIN-CFM-RATIO,                                                       "", 13041, 32055, 0,  2, "The min airflow ratio of the cold duct damper controller at the inlet of the mixing box"
ZONE,              0, CMIN-FLOW-SCH,                                                        "", 63000, 32055, 0,  2, "Scheduled Cooling Min Flow Ratio of the cold duct damper at the inlet of the mixing box"
ZONE,              0, CMIN-CFM-SCH,                                                         "", 63000, 32055, 0,  2, "Scheduled Cooling Min Flow Ratio of the cold duct damper at the inlet of the mixing box"
ZONE,              0, MIN-FLOW-SOURCE,                                   "Minimum Flow Source", 13017, 32055, 0,  0, "Source of makeup air when the supply airflow falls below the Minimum Flow Ratio"
ZONE,              0, MIN-CFM-SOURCE,                                                       "", 13017, 32055, 0,  2, "Source of makeup air when the supply airflow falls below the Minimum Flow Ratio"
ZONE,              0, HW-COIL-HEAD,                                             "HW Coil Head", 13035, 32055, 0,  1, "Pressure drop of the loop fluid through the coil at the design flowrate"
ZONE,              0, HW-VALVE-TYPE,                                           "HW Valve Type", 13034, 32055, 0,  0, "2Way - flow varies with load; 3Way - bypasses extra fluid to maintain constant loop flowrate"
ZONE,              0, HW-COIL-DT,                                            "HW Coil Delta T", 13036, 32055, 0,  1, "Temperature change through the coil at design conditions (used to calculate design flowrate)"
ZONE,              0, HW-LOOP,                                                       "HW Loop", 19079, 32055, 0,  0, "Name of the loop that serves the zonal hot water coil (Loop type = Hot Water, Two Pipe or Steam)"
ZONE,              0, BBRD-COIL-HEAD,                                    "Baseboard Coil Head", 13710, 32055, 0,  1, "Pressure drop of the loop fluid through the baseboards at the design flowrate"
ZONE,              0, BBRD-VALVE-TYPE,                                  "Baseboard Valve Type", 60011, 32055, 0,  2, "2Way - flow varies with load; 3Way - bypasses extra fluid to maintain constant loop flowrate"
ZONE,              0, BBRD-COIL-DT,                                   "Baseboard Coil Delta T", 60012, 32055, 0,  2, "Temperature change through the coil at design conditions (used to calculate design flowrate)"
ZONE,              0, BBRD-LOOP,                                              "Baseboard Loop", 19086, 19086, 0,  0, "The name of the loop that serves baseboard coils (Loop Type must be Hot Water, Two Pipe, or Steam)"
ZONE,              0, CHW-COIL-HEAD,                                           "CHW Coil Head", 13039, 32055, 0,  1, "Pressure drop of the loop fluid through the coil at the design flowrate"
ZONE,              0, CHW-VALVE-TYPE,                                         "CHW Valve Type", 13038, 32055, 0,  0, "2Way - flow varies with load; 3Way - bypasses extra fluid to maintain constant loop flowrate"
ZONE,              0, CHW-COIL-DT,                                          "CHW Coil Delta T", 13040, 32055, 0,  1, "Temperature change through the coil at design conditions (used to calculate design flowrate)"
ZONE,              0, CHW-LOOP,                                                     "CHW Loop", 19077, 32055, 0,  0, "The loop that serves the zonal cooling coil (Loop Type must be Chilled Water or Two Pipe)"
ZONE,              0, CW-COIL-HEAD,                                                         "", 60006, 32055, 0,  2, "Pressure drop of the loop fluid through the coil at the design flowrate"
ZONE,              0, CW-VALVE,                                             "Isolation Valve?", 60007, 32055, 0,  2, "2Way - flow varies with load; 3Way - bypasses extra fluid to maintain constant loop flowrate"
ZONE,              0, CW-COIL-DT,                                                           "", 60008, 32055, 0,  2, "Temperature change through the coil at design conditions (used to calculate design flowrate)"
ZONE,              0, CW-LOOP,                                                       "CW Loop", 60009, 32055, 0,  2, "If Condenser Type=Water Cooled, CW Loop is required & must be attached to Cooling Tower"
ZONE,              0, WSE-COIL-HEAD,                              "Water-side Econo Coil Head", 13059, 32055, 0,  1, "Pressure drop of the loop fluid through the coil at the design flowrate"
ZONE,              0, WSE-VALVE-TYPE,                            "Water-side Econo Valve Type", 13058, 32055, 0,  0, "2Way - flow varies with load; 3Way - bypasses extra fluid to maintain constant loop flowrate"
ZONE,              0, WSE-COIL-DT,                             "Water-side Econo Coil Delta T", 13060, 32055, 0,  1, "Temperature change through the coil at design conditions (used to calculate design flowrate)"
ZONE,              0, WSE-LOOP,                                        "Water-side Econo Loop", 19078, 32055, 0,  0, "Name of loop that serves the water-side economizer (Loop Type = Chilled Water or 2 Pipe)"
ZONE,              0, MIN-FLOW-CTRL,                                    "Minimum Flow Control",     0, 32055, 0,  0, "the method used to set the hourly minimum VAV box flow fraction"
ZONE,              0, SPACE,                                                           "Space", 12018, 32055, 0,  2, "Name of the space that comprises this thermal zone (must be 1 to 1 correlation)"
ZONE,              0, OA-FLOW/AREA,                                             "OA Flow/Area",     0, 32055, 0,  0, "Minimum flow rate of outside air (standard cfm) per unit of zone area"
ZONE,              0, DHW-LOOP,                                                     "DHW Loop",   695, 32055, 0,  0, "Name of the Loop that provides Domestic Hot Water to this zone"
SYSTEMS-REPORT,    0, VERIFICATION,                                                         "",     0, 32059, 0,  2, ""
SYSTEMS-REPORT,    0, SUMMARY,                                                              "",     0, 32059, 0,  2, ""
SYSTEMS-REPORT,    0, DUMP-OPTIONS,                                                         "",     0, 32059, 0,  2, ""
SYSTEMS-REPORT,    0, REPORT-FREQUENCY,                                                     "",     0, 32059, 0,  2, ""
SYSTEMS-REPORT,    0, HOURLY-DATA-SAVE,                                                     "",     0, 32059, 0,  2, ""
CURVE-FIT,         1, TYPE,                                                       "Curve Type", 12244, 32061, 0,  2, "The form of the Curve Fit: Linear, Bi-Linear, Quadratic, Bi-Quadratic, or Cubic"
CURVE-FIT,         1, INPUT-TYPE,                                         "Type of Curve Data", 12264, 32061, 0,  2, "Whether curve coefficients or curve data points are specified"
CURVE-FIT,         1, OUTPUT-MIN,                                                           "", 12266, 32061, 0,  2, "Lowest allowable value of the dependent variables; below this, this value is used"       
CURVE-FIT,         1, OUTPUT-MAX,                                                           "", 12283, 32061, 0,  2, "Highest allowable value of the dependent variables; above this, this value is used"       
CURVE-FIT,         1, COEFFICIENTS,                                            "Coefficients ", 63200, 32061, 0,  8, "List of up to 6 Coefficients that define the Currently Active Curve"     
CURVE-FIT,         1, INDEPENDENT,                                        "Input Data Values ", 63201, 32061, 0,  2, "Input data points used to calculate the Coefficients of the Curve Fit"    
CURVE-FIT,         1, DEPENDENT,                                        "Curve Output Values ", 63201, 32061, 0,  2, "Output data points used to calculate the Coefficients of the Curve Fit"         
CURVE-FIT,         2, TYPE,                                                       "Curve Type", 12244, 32061, 0,  2, "The form of the Curve Fit: Linear, Bi-Linear, Quadratic, Bi-Quadratic, or Cubic"                          
CURVE-FIT,         2, INPUT-TYPE,                                         "Type of Curve Data", 12264, 32061, 0,  2, "Whether curve coefficients or curve data points are specified"              
CURVE-FIT,         2, OUTPUT-MIN,                                                           "", 12266, 32061, 0,  2, "Lowest allowable value of the dependent variables; below this, this value is used"              
CURVE-FIT,         2, OUTPUT-MAX,                                                           "", 12283, 32061, 0,  2, "Highest allowable value of the dependent variables; above this, this value is used"              
CURVE-FIT,         2, COEFFICIENTS,                                            "Coefficients ", 63200, 32061, 0,  8, "List of up to 6 Coefficients that define the Currently Active Curve"          
CURVE-FIT,         2, INDEPENDENT-1,                                "First Input Data Values ", 63201, 32061, 0,  2, "Input data points used to calculate the Coefficients of the Curve Fit"       
CURVE-FIT,         2, INDEPENDENT-2,                               "Second Input Data Values ", 63201, 32061, 0,  2, "Input data points used to calculate the Coefficients of the Curve Fit"       
CURVE-FIT,         2, DEPENDENT,                                        "Curve Output Values ", 63201, 32061, 0,  2, "Output data points used to calculate the Coefficients of the Curve Fit"               
CURVE-FIT,         3, TYPE,                                                       "Curve Type", 12244, 32061, 0,  2, "The form of the Curve Fit: Linear, Bi-Linear, Quadratic, Bi-Quadratic, or Cubic"                           
CURVE-FIT,         3, INPUT-TYPE,                                         "Type of Curve Data", 12264, 32061, 0,  2, "Whether curve coefficients or curve data points are specified"               
CURVE-FIT,         3, OUTPUT-MIN,                                                           "", 12266, 32061, 0,  2, "Lowest allowable value of the dependent variables; below this, this value is used"               
CURVE-FIT,         3, OUTPUT-MAX,                                                           "", 12283, 32061, 0,  2, "Highest allowable value of the dependent variables; above this, this value is used"               
CURVE-FIT,         3, COEFFICIENTS,                                            "Coefficients ", 63200, 32061, 0,  8, "List of up to 6 Coefficients that define the Currently Active Curve"     
CURVE-FIT,         3, INDEPENDENT,                                        "Input Data Values ", 63201, 32061, 0,  2, "Input data points used to calculate the Coefficients of the Curve Fit"    
CURVE-FIT,         3, DEPENDENT,                                        "Curve Output Values ", 63201, 32061, 0,  2, "Output data points used to calculate the Coefficients of the Curve Fit"         
CURVE-FIT,         4, TYPE,                                                       "Curve Type", 12244, 32061, 0,  2, "The form of the Curve Fit: Linear, Bi-Linear, Quadratic, Bi-Quadratic, or Cubic"                           
CURVE-FIT,         4, INPUT-TYPE,                                         "Type of Curve Data", 12264, 32061, 0,  2, "Whether curve coefficients or curve data points are specified"       
CURVE-FIT,         4, OUTPUT-MIN,                                                           "", 12266, 32061, 0,  2, "Lowest allowable value of the dependent variables; below this, this value is used"               
CURVE-FIT,         4, OUTPUT-MAX,                                                           "", 12283, 32061, 0,  2, "Highest allowable value of the dependent variables; above this, this value is used"               
CURVE-FIT,         4, COEFFICIENTS,                                            "Coefficients ", 63200, 32061, 0,  8, "List of up to 6 Coefficients that define the Currently Active Curve"          
CURVE-FIT,         4, INDEPENDENT-1,                                "First Input Data Values ", 63201, 32061, 0,  2, "Input data points used to calculate the Coefficients of the Curve Fit"       
CURVE-FIT,         4, INDEPENDENT-2,                               "Second Input Data Values ", 63201, 32061, 0,  2, "Input data points used to calculate the Coefficients of the Curve Fit"       
CURVE-FIT,         4, DEPENDENT,                                        "Curve Output Values ", 63201, 32061, 0,  2, "Output data points used to calculate the Coefficients of the Curve Fit"    
CURVE-FIT,         5, TYPE,                                                       "Curve Type", 12244, 32061, 0,  2, "The form of the Curve Fit: Linear, Bi-Linear, Quadratic, Bi-Quadratic, or Cubic"                           
CURVE-FIT,         5, INPUT-TYPE,                                         "Type of Curve Data", 12264, 32061, 0,  2, "Whether curve coefficients or curve data points are specified"              
CURVE-FIT,         5, OUTPUT-MIN,                                                           "", 12266, 32061, 0,  2, "Lowest allowable value of the dependent variables; below this, this value is used"               
CURVE-FIT,         5, OUTPUT-MAX,                                                           "", 12283, 32061, 0,  2, "Highest allowable value of the dependent variables; above this, this value is used"               
CURVE-FIT,         5, COEFFICIENTS,                                            "Coefficients ", 63200, 32061, 0,  8, "List of up to 6 Coefficients that define the Currently Active Curve"     
CURVE-FIT,         5, INDEPENDENT,                                 "Input Data Values ", 63201, 32061, 0,  2, "Input data points used to calculate the Coefficients of the Curve Fit"    
CURVE-FIT,         5, DEPENDENT,                                        "Curve Output Values ", 63201, 32061, 0,  2, "Output data points used to calculate the Coefficients of the Curve Fit"         
CURVE-FIT,         6, TYPE,                                                       "Curve Type", 12244, 32061, 0,  2, "The form of the Curve Fit: Linear, Bi-Linear, Quadratic, Bi-Quadratic, or Cubic"                           
CURVE-FIT,         6, INPUT-TYPE,                                         "Type of Curve Data", 12264, 32061, 0,  2, "Whether curve coefficients or curve data points are specified"       
CURVE-FIT,         6, OUTPUT-MIN,                                                           "", 12266, 32061, 0,  2, "Lowest allowable value of the dependent variables; below this, this value is used"               
CURVE-FIT,         6, OUTPUT-MAX,                                                           "", 12283, 32061, 0,  2, "Highest allowable value of the dependent variables; above this, this value is used"               
CURVE-FIT,         6, COEFFICIENTS,                                            "Coefficients ", 63200, 32061, 0,  8, "List of up to 6 Coefficients that define the Currently Active Curve"          
CURVE-FIT,         6, INDEPENDENT-1,                       "First Input - Temperature Values ", 63201, 32061, 0,  2, "Input data points used to calculate the Coefficients of the Curve Fit"       
CURVE-FIT,         6, INDEPENDENT-2,                      "Second Input - Temperature Values ", 63201, 32061, 0,  2, "Input data points used to calculate the Coefficients of the Curve Fit"       
CURVE-FIT,         6, DEPENDENT,                                        "Curve Output Values ", 63201, 32061, 0,  2, "Output data points used to calculate the Coefficients of the Curve Fit"               
CURVE-FIT,         7, TYPE,                                                       "Curve Type", 12244, 32061, 0,  2, "The form of the Curve Fit: Linear, Bi-Linear, Quadratic, Bi-Quadratic, or Cubic"                           
CURVE-FIT,         7, INPUT-TYPE,                                         "Type of Curve Data", 12264, 32061, 0,  2, "Whether curve coefficients or curve data points are specified"              
CURVE-FIT,         7, OUTPUT-MIN,                                                           "", 12266, 32061, 0,  2, "Lowest allowable value of the dependent variables; below this, this value is used"               
CURVE-FIT,         7, OUTPUT-MAX,                                                           "", 12283, 32061, 0,  2, "Highest allowable value of the dependent variables; above this, this value is used"               
CURVE-FIT,         7, COEFFICIENTS,                                            "Coefficients ", 63200, 32061, 0,  8, "List of up to 6 Coefficients that define the Currently Active Curve"     
CURVE-FIT,         7, INDEPENDENT,                                 "Input Temperature Values ", 63201, 32061, 0,  2, "Input data points used to calculate the Coefficients of the Curve Fit"    
CURVE-FIT,         7, DEPENDENT,                                        "Curve Output Values ", 63201, 32061, 0,  2, "Output data points used to calculate the Coefficients of the Curve Fit"         
CURVE-FIT,         8, TYPE,                                                       "Curve Type", 12244, 32061, 0,  2, "The form of the Curve Fit: Linear, Bi-Linear, Quadratic, Bi-Quadratic, or Cubic"                           
CURVE-FIT,         8, INPUT-TYPE,                                         "Type of Curve Data", 12264, 32061, 0,  2, "Whether curve coefficients or curve data points are specified"              
CURVE-FIT,         8, OUTPUT-MIN,                                                           "", 12266, 32061, 0,  2, "Lowest allowable value of the dependent variables; below this, this value is used"               
CURVE-FIT,         8, OUTPUT-MAX,                                                           "", 12283, 32061, 0,  2, "Highest allowable value of the dependent variables; above this, this value is used"               
CURVE-FIT,         8, COEFFICIENTS,                                            "Coefficients ", 63200, 32061, 0,  8, "List of up to 6 Coefficients that define the Currently Active Curve"          
CURVE-FIT,         8, INDEPENDENT-1,                       "First Input - Temperature Values ", 63201, 32061, 0,  2, "Input data points used to calculate the Coefficients of the Curve Fit"       
CURVE-FIT,         8, INDEPENDENT-2,                      "Second Input - Temperature Values ", 63201, 32061, 0,  2, "Input data points used to calculate the Coefficients of the Curve Fit"       
CURVE-FIT,         8, DEPENDENT,                                        "Curve Output Values ", 63201, 32061, 0,  2, "Output data points used to calculate the Coefficients of the Curve Fit"               
CURVE-FIT,         9, TYPE,                                                       "Curve Type", 12244, 32061, 0,  2, "The form of the Curve Fit: Linear, Bi-Linear, Quadratic, Bi-Quadratic, or Cubic"                           
CURVE-FIT,         9, INPUT-TYPE,                                         "Type of Curve Data", 12264, 32061, 0,  2, "Whether curve coefficients or curve data points are specified"              
CURVE-FIT,         9, OUTPUT-MIN,                                                           "", 12266, 32061, 0,  2, "Lowest allowable value of the dependent variables; below this, this value is used"               
CURVE-FIT,         9, OUTPUT-MAX,                                                           "", 12283, 32061, 0,  2, "Highest allowable value of the dependent variables; above this, this value is used"               
CURVE-FIT,         9, COEFFICIENTS,                                            "Coefficients ", 63200, 32061, 0,  8, "List of up to 6 Coefficients that define the Currently Active Curve"          
CURVE-FIT,         9, INDEPENDENT-1,                 "First Input - Delta-Temperature Values ", 63201, 32061, 0,  2, "Input data points used to calculate the Coefficients of the Curve Fit"       
CURVE-FIT,         9, INDEPENDENT-2,                      "Second Input - Temperature Values ", 63201, 32061, 0,  2, "Input data points used to calculate the Coefficients of the Curve Fit"       
CURVE-FIT,         9, DEPENDENT,                                        "Curve Output Values ", 63201, 32061, 0,  2, "Output data points used to calculate the Coefficients of the Curve Fit"               
CURVE-FIT,        10, TYPE,                                                       "Curve Type", 12244, 32061, 0,  2, "The form of the Curve Fit: Linear, Bi-Linear, Quadratic, Bi-Quadratic, or Cubic"                           
CURVE-FIT,        10, INPUT-TYPE,                                         "Type of Curve Data", 12264, 32061, 0,  2, "Whether curve coefficients or curve data points are specified"              
CURVE-FIT,        10, OUTPUT-MIN,                                                           "", 12266, 32061, 0,  2, "Lowest allowable value of the dependent variables; below this, this value is used"               
CURVE-FIT,        10, OUTPUT-MAX,                                                           "", 12283, 32061, 0,  2, "Highest allowable value of the dependent variables; above this, this value is used"               
CURVE-FIT,        10, COEFFICIENTS,                                            "Coefficients ", 63200, 32061, 0,  8, "List of up to 6 Coefficients that define the Currently Active Curve"          
CURVE-FIT,        10, INDEPENDENT-1,                             "First Input - Ratio Values ", 63201, 32061, 0,  2, "Input data points used to calculate the Coefficients of the Curve Fit"       
CURVE-FIT,        10, INDEPENDENT-2,                      "Second Input - Temperature Values ", 63201, 32061, 0,  2, "Input data points used to calculate the Coefficients of the Curve Fit"       
CURVE-FIT,        10, DEPENDENT,                                        "Curve Output Values ", 63201, 32061, 0,  2, "Output data points used to calculate the Coefficients of the Curve Fit"               
CURVE-FIT,        11, TYPE,                                                       "Curve Type", 12244, 32061, 0,  2, "The form of the Curve Fit: Linear, Bi-Linear, Quadratic, Bi-Quadratic, or Cubic"                           
CURVE-FIT,        11, INPUT-TYPE,                                         "Type of Curve Data", 12264, 32061, 0,  2, "Whether curve coefficients or curve data points are specified"              
CURVE-FIT,        11, OUTPUT-MIN,                                                           "", 12266, 32061, 0,  2, "Lowest allowable value of the dependent variables; below this, this value is used"               
CURVE-FIT,        11, OUTPUT-MAX,                                                           "", 12283, 32061, 0,  2, "Highest allowable value of the dependent variables; above this, this value is used"
CURVE-FIT,        11, COEFFICIENTS,                                            "Coefficients ", 63200, 32061, 0,  8, "List of up to 6 Coefficients that define the Currently Active Curve"     
CURVE-FIT,        11, INDEPENDENT,                                 "Input Temperature Values ", 63201, 32061, 0,  2, "Input data points used to calculate the Coefficients of the Curve Fit"    
CURVE-FIT,        11, DEPENDENT,                                        "Curve Output Values ", 63201, 32061, 0,  2, "Output data points used to calculate the Coefficients of the Curve Fit"         
CURVE-FIT,        12, TYPE,                                                       "Curve Type", 12244, 32061, 0,  2, "The form of the Curve Fit: Linear, Bi-Linear, Quadratic, Bi-Quadratic, or Cubic"                           
CURVE-FIT,        12, INPUT-TYPE,                                         "Type of Curve Data", 12264, 32061, 0,  2, "Whether curve coefficients or curve data points are specified"              
CURVE-FIT,        12, OUTPUT-MIN,                                                           "", 12266, 32061, 0,  2, "Lowest allowable value of the dependent variables; below this, this value is used"               
CURVE-FIT,        12, OUTPUT-MAX,                                                           "", 12283, 32061, 0,  2, "Highest allowable value of the dependent variables; above this, this value is used"               
CURVE-FIT,        12, COEFFICIENTS,                                            "Coefficients ", 63200, 32061, 0,  8, "List of up to 6 Coefficients that define the Currently Active Curve"          
CURVE-FIT,        12, INDEPENDENT-1,                       "First Input - Temperature Values ", 63201, 32061, 0,  2, "Input data points used to calculate the Coefficients of the Curve Fit"       
CURVE-FIT,        12, INDEPENDENT-2,                            "Second Input - Ratio Values ", 63201, 32061, 0,  2, "Input data points used to calculate the Coefficients of the Curve Fit"       
CURVE-FIT,        12, DEPENDENT,                                        "Curve Output Values ", 63201, 32061, 0,  2, "Output data points used to calculate the Coefficients of the Curve Fit"               
CURVE-FIT,        13, TYPE,                                                       "Curve Type", 12244, 32061, 0,  2, "The form of the Curve Fit: Linear, Bi-Linear, Quadratic, Bi-Quadratic, or Cubic"                           
CURVE-FIT,        13, INPUT-TYPE,                                         "Type of Curve Data", 12264, 32061, 0,  2, "Whether curve coefficients or curve data points are specified"               
CURVE-FIT,        13, OUTPUT-MIN,                                                           "", 12266, 32061, 0,  2, "Lowest allowable value of the dependent variables; below this, this value is used"               
CURVE-FIT,        13, OUTPUT-MAX,                                                           "", 12283, 32061, 0,  2, "Highest allowable value of the dependent variables; above this, this value is used"               
CURVE-FIT,        13, COEFFICIENTS,                                            "Coefficients ", 63200, 32061, 0,  8, "List of up to 6 Coefficients that define the Currently Active Curve"     
CURVE-FIT,        13, INDEPENDENT,                           "Input Delta-Temperature Values ", 63201, 32061, 0,  2, "Input data points used to calculate the Coefficients of the Curve Fit"    
CURVE-FIT,        13, DEPENDENT,                                        "Curve Output Values ", 63201, 32061, 0,  2, "Output data points used to calculate the Coefficients of the Curve Fit"         
SUBR-FUNCTIONS,    0, BERNOU-1,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, CFMINF-0,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, CFMINF-1,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, CONCHN-1,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, DAYCLS-1,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, DAYCLS-2,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, DAYCLS-3,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, DAYCLS-4,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, DAYCLS-5,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, DAYCLS-6,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, DDSF-0,                                                               "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, DDSF-1,                                                               "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, DESFO-0,                                                              "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, DESFO-1,                                                              "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, DESIGN-1,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, DESIND-0,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, DESIND-1,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, DESPIU-0,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, DESPIU-1,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, DKTEMP-0,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, DKTEMP-1,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, DKTEMP-2,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, DKTEMP-3,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, DOETRM-0,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, DOETRM-1,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, DOUBLE-0,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, DOUBLE-1,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, EBAL-0,                                                               "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, EBAL-1,                                                               "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, ECONO-1,                                                              "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, ECONO-2,                                                              "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, ECONO-3,                                                              "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, ECONO-4,                                                              "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, FANPWR-1,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, FCOIL-0,                                                              "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, FCOIL-1Z,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, FCOIL-2Z,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, FCOIL-3,                                                              "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, FTDEV-1,                                                              "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, FURNAC-1,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, HE-1,                                                                 "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, HOURIN-1,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, HPUNIT-1,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, HTPUMP-0Z,                                                            "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, HTPUMP-1Z,                                                            "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, HTPUMP-2,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, HVUNIT-0,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, HVUNIT-1Z,                                                            "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, HVUNIT-2,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, HVUNIT-3,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, INDUC-0,                                                              "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, INDUC-1Z,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, INDUC-2,                                                              "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, OPSTRT-1,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, PANEL-0Z,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, PANEL-1,                                                              "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, PIU-0,                                                                "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, PIU-1,                                                                "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, PTAC-0,                                                               "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, PTAC-1Z,                                                              "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, PTAC-2,                                                               "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, RESVVT-0,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, RESVVT-1,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, RESVVT-2Z,                                                            "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, RESVVT-3,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, RESVVT-4,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, RESYS-0,                                                              "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, RESYS-1Z,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, RESYS-2Z,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, RESYS-3Z,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, RESYS-4Z,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, RESYS-5,                                                              "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, SDSF-0,                                                               "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, SDSF-1,                                                               "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, SSBASB-1,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, SSFCOR-1,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, SUM-1,                                                                "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, SUM-2Z,                                                               "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, SUM-3Z,                                                               "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, SUM-4Z,                                                               "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, SUM-5,                                                                "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, SZCI-0,                                                               "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, SZCI-1Z,                                                              "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, SZCI-2,                                                               "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, TDVPIU-0,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, TDVPIU-1,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, TEMDEV-0,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, TEMDEV-1,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, TEMDEV-2,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, TEMDEV-3,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, TSOLVE-0,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, TSOLVE-1,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, UNITH-0,                                                              "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, UNITH-1Z,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, UNITH-2Z,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, UNITH-3,                                                              "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, UNITV-0,                                                              "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, UNITV-1Z,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, UNITV-2,                                                              "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, VARVOL-0,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, VARVOL-1Z,                                                            "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, VARVOL-2,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, VARVOL-3,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, FNSYS1-1,                                                             "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, FNSYS1-2Z,                                                            "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, FNSYS1-3Z,                                                            "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, FNSYS1-4Z,                                                            "",     0, 32062, 0,  2, ""
SUBR-FUNCTIONS,    0, FNSYS1-5,                                                             "",     0, 32062, 0,  2, ""
PUMP,              0, FLOW,                                                      "Design Flow", 12853, 32063, 0,  0, "Design flowrate of the pump"
PUMP,              0, FLOW-RATIO,                                                 "Flow Ratio", 12855, 32063, 0,  0, "When autosizing, PowerDOE oversizes the design flowrate of the Loop Pump using this ratio"
PUMP,              0, NUMBER,                                                         "Number", 12856, 32063, 0,  0, "Number of identical pumps attached to this equipment"
PUMP,              0, HEAD,                                                      "Design Head", 12852, 32063, 0,  0, "Design pressure rise of the fluid across the pump (when the pump is running)"
PUMP,              0, HEAD-RATIO,                                                 "Head Ratio", 12854, 32063, 0,  0, "When Autosizing, PowerDOE oversizes the head imparted by the Loop Pump using this ratio"
PUMP,              0, HEAD-SETPT,                                              "Head Setpoint",   678, 32063, 0,  0, "The design set-point of the pump's differential head pressure sensor"
PUMP,              0, HEAD-SETPT-RATIO,                                  "Head Setpoint Ratio", 12854, 32063, 0,  0, "A safety factor applied to the pump’s default Head Setpoint (if auto-sized)"
PUMP,              0, MECH-EFF,                                        "Mechanical Efficiency", 12859, 32063, 0,  0, "Mechanical efficiency of the pump impeller"
PUMP,              0, MOTOR-EFF,                                            "Motor Efficiency", 12858, 32063, 0,  0, "Efficiency of the pump motor (default is based on Motor Class & Pump Power)"
PUMP,              0, MOTOR-CLASS,                                               "Motor Class", 12861, 32063, 0,  0, "Efficiency classification of the motor (high & premium eff. are based on NEMA standards)"
PUMP,              0, PUMP-KW,                                                       "Pump kW", 12857, 32063, 0,  0, "The design power consumption of the pump"
PUMP,              0, CAP-CTRL,                                             "Capacity Control", 12862, 32063, 0,  0, "A pump can 'rides its curve' (if a 2 way valve exists), be 2-speed or variable speed"
PUMP,              0, MIN-SPEED,                                               "Minimum Speed", 12860, 32063, 0,  0, "The lower speed of a 2-speed pump, or the minimum speed of a variable-speed pump"
PUMP,              0, PUMP-HEAD-FFLOW,                                     "Pump Head f(Flow)", 12863, 32063, 0,  0, "Cubic Curve Fit: the head imparted by the pump as a function of the flow rate"
PUMP,              0, PUMP-HP-FFLOW,                                      "Pump Power f(Flow)", 12864, 32063, 0,  0, "Cubic Curve Fit: the horsepower input to the pump as a function of the flow rate"
PUMP,              0, PUMP-MAX-RATIO,                                                       "",   993, 32063, 0,  2, "Maximum flow rate that the pump can impart (as a fraction of the design pump flow rate)"
PUMP,              0, PUMP-POWER-EXP,                                                       "",   994, 32063, 0,  2, "How pump horsepower varies with speed (when all other parameters obey the ideal pump laws)"
PUMP,              0, VFD-LOSS,                       "Full load (at peak pump kw) VFD losses",   994, 32063, 0,  2, "The ratio of VFD losses (kw) to pump power (kw) at full pump load"
PUMP,              0, VFD-LOSS-FPLR,                     "VFD losses as a function of pump kw",   994, 32063, 0,  2, "Modifier (multiplier) on VFD losses as a function of pump PLR (hourly pump kw over peak kw)"
PUMP,              0, ELEC-METER,                                                           "", 63025, 32063, 0,  2, "Name of the Electric Meter that tallies the electricity consumption of the pump"
PUMP,              0, COST-DATA,                                                   "Cost Data", 12927, 32063, 0,  0, "Name of a set of Materials Costs, which specifies first costs, maintenance costs, etc."
PUMP,              0, EQUIPMENT-REPORT,                                                     "",     0, 32063, 0,  2, "Whether or not a PS-H report is created for this pump"
PUMP,              0, PICTURE,                                                              "",     0, 32063, 0,  2, ""
PUMP,              0, DRAWING,                                                              "",     0, 32063, 0,  2, ""
CIRCULATION-LOOP,  0, TYPE,                                                             "Type", 12777, 32064, 0,  0, "Each loop must be one of six available types"
CIRCULATION-LOOP,  0, SUBTYPE,                                                       "Subtype", 12778, 32064, 0,  0, "Secondary loops are served exclusively by primary loops"
CIRCULATION-LOOP,  0, LOOP-DESIGN-DT,                                    "Loop Design Delta T", 12780, 32064, 0,  1, "Design temperature change of the fluid in the loop"
CIRCULATION-LOOP,  0, SIZING-OPTION,                                           "Sizing Option", 12779, 32064, 0,  0, "Whether the loop is sized based on the loads it serves or the equipment that serves it"
CIRCULATION-LOOP,  0, LOOP-SIZE-RATIO,                                       "Loop Size Ratio", 12787, 32064, 0,  1, "A safety factor applied to the primary equipment (e.g., boilers, etc.) in the loop sizing routine"
CIRCULATION-LOOP,  0, FLUID-VOLUME,                                             "Fluid Volume", 12781, 32064, 0,  0, "Total volume of the fluid in the loop"
CIRCULATION-LOOP,  0, AVG-CIRC-TIME,                                "Average Circulation Time", 12782, 32064, 0,  1, "Average time it takes for the fluid to circulate through the loop (at the design flow rate)"
; SAC 10/28/01 - Removed certain keywords
; CIRCULATION-LOOP,  0, BRINE-TYPE,                                                 "Brine Type", 12788, 32064, 0,  0, "The type of fluid circulating in the loop"
; CIRCULATION-LOOP,  0, BRINE-PCT,                                               "Brine Percent", 12789, 32064, 0,  1, "The percent (by weight) of the glycol or salt in the working fluid of the loop"
CIRCULATION-LOOP,  0, LOOP-MIN-FLOW,                                       "Loop Minimum Flow", 12786, 32064, 0,  2, "Minimum allowable flow rate in the loop, expressed as a fraction of the design flow rate"
CIRCULATION-LOOP,  0, LOOP-RECIRC-FLOW,                              "Loop Recirculation Flow", 12783, 32064, 0,  1, "Recirculating flow rate of the fluid in the loop when the pump is running"
CIRCULATION-LOOP,  0, PIPE-HEAD,                                                   "Pipe Head", 12784, 32064, 0,  1, "Friction loss in the loop due to the piping and related trim"
CIRCULATION-LOOP,  0, STATIC-HEAD,                                               "Static Head", 12785, 32064, 0,  2, "Loop static head (independent of the fluid flow rate)"
CIRCULATION-LOOP,  0, PRIMARY-LOOP,                                    "Attached Primary Loop", 19143, 19143, 0,  2, "Name of the primary loop that this secondary loop is attached to (and served by)"
CIRCULATION-LOOP,  0, PRIMARY-FLOW-PCT,                                                     "", 14509, 32064, 0,  2, "Percentage of secondary loop flow that transfers to primary loop flow (at design conditions)"
CIRCULATION-LOOP,  0, VALVE-TYPE-2ND,                                             "Valve Type", 12812, 32064, 0,  0, "Type of valve that meters the primary fluid into the secondary loop or heat-exchanger"
CIRCULATION-LOOP,  0, VALVE-HEAD-2ND,                                   "Secondary Valve Head", 12884, 32064, 0,  1, "Head loss of fluid across the valve that meters the flow between primary and secondary loops"
CIRCULATION-LOOP,  0, LOOP-OPERATION,                                         "Loop Operation", 12840, 32064, 0,  0, "Specifies when the loop is active"
CIRCULATION-LOOP,  0, HEATING-SCHEDULE,                                     "Heating Schedule", 12842, 32064, 0,  0, "Specifies when the primary heating equipment is enabled"
CIRCULATION-LOOP,  0, COOLING-SCHEDULE,                                     "Cooling Schedule", 12841, 32064, 0,  0, "Specifies when the primary cooling or heat-rejection equipment is enabled"
CIRCULATION-LOOP,  0, PUMP-SCHEDULE,                                           "Pump Schedule", 12843, 32064, 0,  0, "Specifies when the loop's pump is enabled"
CIRCULATION-LOOP,  0, SNAP-T,                                               "Snap Temperature", 12839, 32064, 0,  1, "Temperature at which the snap occurs (i.e., at which the Loop turns on or off)"
CIRCULATION-LOOP,  0, SNAP-LOCN,                                               "Snap Location", 12838, 32064, 0,  0, "Location of the snap-acting temperature sensor that turns the loop on or off"
CIRCULATION-LOOP,  0, SNAP-ZONE,                                                   "Snap Zone", 12844, 32064, 0,  0, "The zone whose temperature is monitored to determine whether the loop is active"
; SAC 8/19/03 - Added DESIGN-HEAT-T
CIRCULATION-LOOP,  0, DESIGN-HEAT-T,                                   "Design HW Temperature",     0, 32064, 0,  1, "Design hot water temperature of the fluid in the loop"
CIRCULATION-LOOP,  0, HEAT-SETPT-CTRL,                                 "Heat Setpoint Control", 12766, 32064, 0,  0, "The loop temperature control sequence"
CIRCULATION-LOOP,  0, HEAT-SETPT-T,                                "Heat Setpoint Temperature", 12767, 32064, 0,  1, "The loop heating setpoint"
CIRCULATION-LOOP,  0, HEAT-RESET-SCH,                                    "Heat Reset Schedule", 12768, 32064, 0,  0, "A Reset Temperature Schedule that specifies the heating setpoint"
CIRCULATION-LOOP,  0, HEAT-SETPT-SCH,                                 "Heat Setpoint Schedule", 12769, 32064, 0,  0, "Specifies the loop heating setpoint (a Temperature Schedule)"
; SAC 8/19/03 - Added DESIGN-COOL-T
CIRCULATION-LOOP,  0, DESIGN-COOL-T,                                  "Design CHW Temperature",     0, 32064, 0,  1, "Design chilled water temperature of the fluid in the loop"
CIRCULATION-LOOP,  0, COOL-SETPT-CTRL,                                 "Cool Setpoint Control", 12771, 32064, 0,  0, "The loop temperature control sequence"
CIRCULATION-LOOP,  0, COOL-SETPT-T,                                "Cool Setpoint Temperature", 12772, 32064, 0,  1, "The loop cooling setpoint"
CIRCULATION-LOOP,  0, COOL-RESET-SCH,                                    "Cool Reset Schedule", 12773, 32064, 0,  0, "A Reset Temperature Schedule that specifies the cooling setpoint"
CIRCULATION-LOOP,  0, COOL-SETPT-SCH,                                 "Cool Setpoint Schedule", 12774, 32064, 0,  0, "Specifies the loop cooling setpoint (a Temperature Schedule)"
CIRCULATION-LOOP,  0, LOOP-SETPT-RNG,                                    "Loop Setpoint Range", 12765, 32064, 0,  1, "Throttling range of the loop temperature controller"
CIRCULATION-LOOP,  0, RESTART-AIR-T,                                                        "", 13734, 32064, 0,  1, "The temperature at (or below) which the loop restarts and runs to provide freeze protection"
CIRCULATION-LOOP,  0, RESTART-SETPT-T,                                                      "", 13735, 32064, 0,  1, "The heating setpoint of the loop when a WLHP restarts to avoid freezing"
CIRCULATION-LOOP,  0, LOOP-FLOW-RESET,                                       "Loop Flow Reset", 12764, 32064, 0,  0, "Fraction of design flow rate to which the flow is reduced, prior to initiating a temperature reset"
CIRCULATION-LOOP,  0, MAX-RESET-T,                                 "Maximum Reset Temperature", 12893, 32064, 0,  1, "The maximum allowable supply-side loop temperature (for Chilled Water or Two Pipe loops)"
CIRCULATION-LOOP,  0, MIN-RESET-T,                                 "Minimum Reset Temperature", 12894, 32064, 0,  1, "The minimum allowable supply-side loop temperature (for Hot Water or Two Pipe loops)"
CIRCULATION-LOOP,  0, MAX-ALARM-T,                                 "Maximum Alarm Temperature", 12895, 32064, 0,  1, "WLHP units are turned off when the supply temperature exceeds this value"
CIRCULATION-LOOP,  0, MIN-ALARM-T,                                 "Minimum Alarm Temperature", 12896, 32064, 0,  1, "WLHP units are turned off when the supply temperature falls below this value"
CIRCULATION-LOOP,  0, LOOP-PUMP,                                       "Loop Circulation Pump", 12851, 32064, 0,  2, "Name of the dedicated Pump that pumps this loop"
CIRCULATION-LOOP,  0, HEAD-SETPT-CTRL,                                 "Head Setpoint Control", 12830, 32064, 0,  0, "Type of control sequence used to control the head setpoint of the loop circulation pumps"
CIRCULATION-LOOP,  0, HEAD-SETPT,                                              "Head Setpoint", 12832, 32064, 0,  1, "Design setpoint of the differential head pressure sensor"
CIRCULATION-LOOP,  0, HEAD-SETPT-RATIO,                                  "Head Setpoint Ratio", 12834, 32064, 0,  1, "A safety factor applied to the default Head Setpoint"
CIRCULATION-LOOP,  0, HEAD-SETPT-RNG,                                    "Head Setpoint Range", 12833, 32064, 0,  1, "Throttling range of the head setpoint controller"
CIRCULATION-LOOP,  0, HEAD-SENSOR-LOCN,                                 "Head Sensor Location", 12831, 32064, 0,  0, "Location of the differential head pressure sensor"
CIRCULATION-LOOP,  0, SUPPLY-UA,                                                   "Supply UA", 12816, 32064, 0,  1, "Thermal conductivity of the loop on the supply side (from entering loop to attached coils, etc.)"
CIRCULATION-LOOP,  0, SUPPLY-LOSS-DT,                                    "Supply Loss Delta T", 12817, 32064, 0,  1, "Thermal conductivity of the loop on the supply side (from entering loop to attached coils, etc.)"
CIRCULATION-LOOP,  0, RETURN-UA,                                                   "Return UA", 12818, 32064, 0,  1, "Thermal conductivity of the loop on the return side"
CIRCULATION-LOOP,  0, RETURN-LOSS-DT,                                    "Return Loss Delta T", 12819, 32064, 0,  1, "Temperature change in the working fluid of the loop on the return side"
CIRCULATION-LOOP,  0, HEATING-ENVIR-T,                       "Heating Environment Temperature", 12821, 32064, 0,  1, "Design temperature of the pipe's environment when the loop is in heating mode"
CIRCULATION-LOOP,  0, COOLING-ENVIR-T,                       "Cooling Environment Temperature", 12820, 32064, 0,  1, "Design temperature of the pipe's environment when the loop is in cooling mode"
CIRCULATION-LOOP,  0, LOOP-LOCN,                                               "Loop Location", 12822, 32064, 0,  0, "Location of the loop piping (determines the temperature at which losses occur)"
CIRCULATION-LOOP,  0, LOOP-LOSS-ZONE,                                              "Loss Zone", 12825, 32064, 0,  0, "The zone that the loop is in (the loop's thermal losses appear a loads in this zone)"
CIRCULATION-LOOP,  0, LOOP-TUNNEL-T,                                      "Tunnel Temperature", 12823, 32064, 0,  1, ""
CIRCULATION-LOOP,  0, LOOP-TUNNEL-SCH,                                       "Tunnel Schedule", 12824, 32064, 0,  0, ""
CIRCULATION-LOOP,  0, ASSIGN-LOSSES-TO,                                                     "", 14508, 32064, 0,  0, "The end-use category in which the loop thermal losses are included in output reports"
CIRCULATION-LOOP,  0, PROCESS-LOAD,                                                         "",   992, 32064, 0,  2, "Maximum process load thermal demand (+ for heat added to loop, - for heat removed)"
CIRCULATION-LOOP,  0, PROCESS-FLOW,                                             "Process Flow", 12868, 32064, 0,  1, "Peak Process Load flow rate"
CIRCULATION-LOOP,  0, PROCESS-SCH,                                     "Process Load Schedule", 12867, 32064, 0,  0, "A Fraction Schedule that modifies the Process Load"
CIRCULATION-LOOP,  0, PROCESS-LOAD-DT,                                  "Process Load Delta T", 12869, 32064, 0,  1, "Delta T of the process load fluid (used to calculate Process Flow Rate, sign is irrelevant)"
CIRCULATION-LOOP,  0, LOOP-AUX-KW,                                         "Loop Auxiliary kW", 12848, 32064, 0,  1, "Maximum input power required by auxiliary electrical loads on this loop"
CIRCULATION-LOOP,  0, LOOP-AUX-SCH,                                  "Loop Auxiliary Schedule", 12849, 32064, 0,  0, "A fractional schedule that adjusts the Loop's Auxiliary Power"
CIRCULATION-LOOP,  0, LOOP-AUX-METER,                                   "Loop Auxiliary Meter", 12850, 32064, 0,  0, "The electrical meter that tallies the Loop's Auxiliary Load"
CIRCULATION-LOOP,  0, HEAT-EQUIP-CTRL,                                "Heat Equipment Control", 12770, 32064, 0,  0, "An Equipment Control sequence for the primary heating equipment that serves this loop"
CIRCULATION-LOOP,  0, COOL-EQUIP-CTRL,                                "Cool Equipment Control", 12775, 32064, 0,  0, "An Equipment Control sequence for the primary cooling equipment that serves this loop"
CIRCULATION-LOOP,  0, DHW-INLET-T,                                     "DHW Inlet Temperature", 12870, 32064, 0,  1, "Inlet temperature of the potable water supplied to the DHW heater"
CIRCULATION-LOOP,  0, DHW-INLET-T-SCH,                        "DHW Inlet Temperature Schedule", 12871, 32064, 0,  0, "Scheduled inlet temperature of the potable water supplied to the DHW heater"
CIRCULATION-LOOP,  0, COST-DATA,                                                            "", 12790, 32064, 0,  2, "Name of a set of Materials Costs, which specifies first costs, maintenance costs, etc."
CIRCULATION-LOOP,  0, LOSSES-BASED-ON,                                        "Base Losses on", 12826, 32064, 0,  0, "Whether design loop thermal losses are based on heating or cooling mode of operation"
CIRCULATION-LOOP,  0, EQUIPMENT-REPORT,                                                     "",     0, 32064, 0,  2, "Whether or not a PS-H report is created for this loop"
CIRCULATION-LOOP,  0, PICTURE,                                                              "",     0, 32064, 0,  2, ""
CIRCULATION-LOOP,  0, DRAWING,                                                              "",     0, 32064, 0,  2, ""
CHILLER,           1, TYPE,                                                             "Type", 12873, 32065, 0,  0, "PowerDOE has models for nine types of chillers"
CHILLER,           1, CAPACITY,                                                     "Capacity", 13792, 32065, 0,  1, "Nominal (rated) chiller cooling capacity in MBTU/hr (e.g., 100 ton = 1.2 MBTU/hr)"
CHILLER,           1, CAPACITY-RATIO,                                         "Capactiy Ratio", 13793, 32065, 0,  1, "Capacity as fraction of max cooling load (used only if PowerDOE sizes the chiller)"
CHILLER,           1, CAPACITY-FT,                                               "Capacity FT", 12968, 32065, 0,  0, "Bi-Quadratic Curve: Capacity as function of temp of entering condenser & exiting chilled water"
CHILLER,           1, MIN-RATIO,                                               "Minimum Ratio", 12953, 32065, 0,  2, "Minimum chiller operating ratio (a fraction of the Capacity); below this, it cycles on & off"
; SAC 4/18/02 - removed CHILLER:MAX-RATIO
; CHILLER,           1, MAX-RATIO,                                               "Maximum Ratio", 12954, 32065, 0,  2, "Maximum allowable chiller operating ratio (fraction of Capacity, also called max overload ratio)"
CHILLER,           1, HGB-RATIO,                                                   "HGB Ratio", 12952, 32065, 0,  2, "Maximum allowable part-load ratio of the chiller, above which hot gas bypass occures"
CHILLER,           1, ELEC-INPUT-RATIO,                                 "Electric Input Ratio", 12879, 32065, 0,  2, "Dimensionless ratio of electric input power to nominal capacity (i.e., invers of COP)"
CHILLER,           1, EIR-FT,                                                               "", 12967, 32065, 0,  0, "Quadratic Curve Fit: EIR as a function of temp of water entering condenser & leaving chilled"
CHILLER,           1, EIR-FPLR,                                                             "", 12969, 32065, 0,  0, "Quadratic Curve Fit: Electric Input Ratio as a function of the part load ratio"
CHILLER,           1, ELEC-TO-COND,                                    "Electric To Condenser", 12957, 32065, 0,  2, "Efficiency of compressor: i.e., fraction of chiller electricity input rejected to condenser, as heat"
CHILLER,           1, HEAT-INPUT-RATIO,                                     "Heat Input Ratio", 12956, 32065, 0,  2, "Ratio of fuel heat input (in Btus) to full load cooling capacity (in Btus), as rated conditions"
CHILLER,           1, HIR-FT,                                                               "", 12964, 32065, 0,  0, "Bi-Quadratic Curve: HIR as a function of temp of entering condenser and exiting chilled water"
CHILLER,           1, HIR-FPLR,                                                             "", 12965, 32065, 0,  0, "Quadratic Curve Fit: Heat Input Ratio as a function of the part load ratio"
CHILLER,           1, HEAT-TO-COND,                                        "Heat to Condenser", 12882, 32065, 0,  2, "Fraction of fuel or heat input to chiller that is rejected to condenser, as heat"
CHILLER,           1, START-UP-TIME,                                                        "", 13644, 32065, 0,  2, "Equivalent full-load time required to start up the chiller (in hours or fraction of hours)"
CHILLER,           1, SHUT-DOWN-TIME,                                                       "", 13649, 32065, 0,  2, "Equivalent full-load time required to shut down the chiller (in hours or fraction of hours)"
CHILLER,           1, HGB-RATIO-HTREC,                                                      "", 12970, 32065, 0,  2, "The hot gas bypass ratio when the chiller is in the heat recovery mode"
CHILLER,           1, SOLUTION-PUMP-KW,                                                     "", 13650, 32065, 0,  2, "Electricity consumption of the solution pump"
CHILLER,           1, GAS-HCAP-FPLRC,                                                       "", 13787, 32065, 0,  2, "Quadratic Curve: heating capacity as a function of the cooling part load ratio"
CHILLER,           1, GAS-HW-XEFF,                                                          "", 13780, 32065, 0,  2, "The burner efficiency (when the chiller is in the heating mode)"
CHILLER,           1, GAS-DESC-XEFF,                                                        "", 13781, 32065, 0,  2, "The burner efficiency when regenerating a desiccant system"
CHILLER,           1, GAS-COMB-FAN-KW,                                                      "", 13778, 32065, 0,  2, "Electricity consumption of the combustion blower"
CHILLER,           1, GAS-HIR-FDESCT,                                                       "", 13788, 32065, 0,  2, "Quadratic Curve: Heat Input Ratio as a function of the desiccant regeneration temperature"
CHILLER,           1, GAS-QREG-FDESCT,                                                      "", 13789, 32065, 0,  2, "Quadratic Curve: available regeneration energy as a function of the required regeneration temp"
CHILLER,           1, ENG-HEAT-TO-JAC,                                                      "", 13848, 32065, 0,  2, "Fraction of design fuel consumption that is recoverable from the jacket of an engine-chiller"
CHILLER,           1, ENG-HEAT-TO-EXH,                                                      "", 13849, 32065, 0,  2, "Fraction of design fuel consumption that is recoverable from the exhaust of an engine-chiller"
CHILLER,           1, ENG-HTREJ-FT,                                                         "", 13785, 32065, 0,  2, "Quadratic Curve: the amount of recoverable heat as a function of the entering condenser temp"
CHILLER,           1, ENG-HTREJ-FPLR,                                                       "", 13784, 32065, 0,  2, "Quadratic Curve: amount of recoverable heat as a function of the cooling part load ratio"
CHILLER,           1, HEAT/COOL-CAP,                                           "HEAT/COOL-CAP",     0, 32065, 0,  3, "HEAT/COOL-CAP"
CHILLER,           1, HEAT-CAP-FT,                                               "HEAT-CAP-FT",     0, 32065, 0,  0, "HEAT-CAP-FT"
CHILLER,           1, HEAT-CAP-FT-FRST,                                     "HEAT-CAP-FT-FRST",     0, 32065, 0,  0, "HEAT-CAP-FT-FRST"
CHILLER,           1, HEAT-EIR,                                                     "HEAT-EIR",     0, 32065, 0,  3, "HEAT-EIR"
CHILLER,           1, HEAT-EIR-FT,                                               "HEAT-EIR-FT",     0, 32065, 0,  0, "HEAT-EIR-FT"
CHILLER,           1, HEAT-EIR-FT-FRST,                                     "HEAT-EIR-FT-FRST",     0, 32065, 0,  0, "HEAT-EIR-FT-FRST"
CHILLER,           1, HEAT-EIR-FPLR,                                           "HEAT-EIR-FPLR",     0, 32065, 0,  0, "HEAT-EIR-FPLR"
CHILLER,           1, AUX-KW,                                                   "Auxiliary kW", 13795, 32065, 0,  2, "Auxiliary electric power consumption of the chiler (e.g., control panels)"
CHILLER,           1, AUX-MODE,                                                             "", 12987, 32065, 0,  2, "Always=all hours;When On=If chiller on;When Off=if chiller off;Scheduled=use Aux Schedule"
CHILLER,           1, AUX-SCHEDULE,                                       "Auxiliary Schedule", 12988, 32065, 0,  2, "Schedule for Auxiliary Power consumption (set Auxiliary Mode to Scheduled to activate this)"
CHILLER,           1, AUX-METER,                                                            "", 12989, 32065, 0,  0, "Name of the Electric Meter that tallies the electricity consumption of this chiller's auxiliaries"
CHILLER,           1, ELEC-METER,                                             "Electric Meter", 12948, 32065, 0,  0, "Name of the Electric Meter that tallies the electric consumption of this chiller"
CHILLER,           1, FUEL-METER,                                                 "Fuel Meter", 12949, 32065, 0,  0, "Name of the Fuel Meter that tallies the fuel consumption of this chiller"
CHILLER,           1, CHW-LOOP,                                                     "CHW Loop", 19111, 32065, 0,  0, "Name of the primary Chiller Water Loop that this chiller serves"
CHILLER,           1, CHW-PUMP,                                                     "CHW Pump", 13800, 32065, 0,  0, "Name of a Pump that serves the chiller's chilled water loop"
CHILLER,           1, CHW-DT,                                                    "CHW Delta T", 12974, 32065, 0,  2, "Design temperature change of the chilled water through the chiller"
CHILLER,           1, CHW-HEAD,                                                             "", 12975, 32065, 0,  2, "Head loss through the chilled water piping at the design flow rate"
CHILLER,           1, CHW-STATIC-HEAD,                                                      "", 12976, 32065, 0,  2, "The static head in the chiller circuit (typically zero)"
CHILLER,           1, CHW-FLOW-CTRL,                                                        "", 12973, 32065, 0,  2, "The type of flow through the chiller evaporator"
CHILLER,           1, CHW-MIN-FLOW,                                                         "", 12977, 32065, 0,  2, "Minimum allowable fraction of the design flow rate through the evaporator"
CHILLER,           1, CHW-MAX-FLOW,                                                         "", 13491, 32065, 0,  2, "Maximum allowable fraction of the design flow rate through the evaporator"
CHILLER,           1, HW-LOOP,                                                       "HW Loop", 19117, 32065, 0,  0, "Name of HW loop that provides heat to an absorption chiller; or that a chiller/heater heats"
CHILLER,           1, HW-PUMP,                                                              "", 12991, 32065, 0,  2, "Hot Water pump: if not specified, the head requirement is passed to the primary loop"
CHILLER,           1, HW-DT,                                                      "HW Delta T", 12993, 32065, 0,  2, "Design temp change of hot water through the boiler (used to size recirculation pump)"
CHILLER,           1, HW-HEAD,                                                              "", 12994, 32065, 0,  2, "Pressure drop of the hot water through the chiller at the design flowrate"
CHILLER,           1, HW-STATIC-HEAD,                                                       "", 12995, 32065, 0,  2, "Static HW pressure drop through the chiller; use if pumping fluid at atm pressure into loop"
CHILLER,           1, HW-FLOW-CTRL,                                                         "", 12992, 32065, 0,  2, "Constant Flow = independent of the load; Variable Flow = varies linearly with load"
CHILLER,           1, HW-MIN-FLOW,                                                          "", 12996, 32065, 0,  2, "Min hot water flow rate through chiller; used only if Hot Water Flow Control = Variable Flow"
CHILLER,           1, HW-MAX-FLOW,                                                          "", 13492, 32065, 0,  2, "Max hot water flow rate through chiller; used only if Hot Water Flow Control = Variable Flow"
CHILLER,           1, CONDENSER-TYPE,                                         "Condenser Type", 12875, 32065, 0,  0, "Air Cooled=heat exchanger & condenser; Water Cooled=cooling tower & condenser loop"
CHILLER,           1, CW-LOOP,                                                       "CW Loop", 19112, 32065, 0,  0, "If Condenser Type=Water Cooled, CW Loop is required & must be attached to Cooling Tower"
CHILLER,           1, CW-PUMP,                                                       "CW Pump", 12929, 32065, 0,  0, "Name of a Pump that serves the (dedicated) evaporator recirculation loop"
CHILLER,           1, CW-DT,                                                      "CW Delta T", 12981, 32065, 0,  2, "Design temperature change of the water flowing through the condenser"
CHILLER,           1, CW-HEAD,                                                              "", 12982, 32065, 0,  2, "Pressure drop through the condenser at the design flow rate"
CHILLER,           1, CW-STATIC-HEAD,                                                       "", 12983, 32065, 0,  2, "Static pressure drop through the condenser at the design flow rate"
CHILLER,           1, CW-FLOW-CTRL,                                                         "", 12980, 32065, 0,  2, "The type of flow through the condenser"
CHILLER,           1, CW-MIN-FLOW,                                                          "", 12984, 32065, 0,  2, "Minimum allowable flow rate through the condenser (as a fraction of the design flow rate)"
CHILLER,           1, COND-SETPT-CTRL,                                       "COND-SETPT-CTRL",     0, 32065, 0,  0, "COND-SETPT-CTRL"
CHILLER,           1, COND-FAN-CTRL,                                           "COND-FAN-CTRL",     0, 32065, 0,  0, "COND-FAN-CTRL"
CHILLER,           1, COND-SETPT-T,                                             "COND-SETPT-T",     0, 32065, 0,  1, "COND-SETPT-T"
CHILLER,           1, COND-SETPT-DT,                                           "COND-SETPT-DT",     0, 32065, 0,  2, "COND-SETPT-DT"
CHILLER,           1, MIN-COND-T,                                                 "MIN-COND-T",     0, 32065, 0,  1, "MIN-COND-T"
CHILLER,           1, COND-CAPACITY,                                           "COND-CAPACITY",     0, 32065, 0,  3, "COND-CAPACITY"
CHILLER,           1, SCT-AMB-DT,                                                 "SCT-AMB-DT",     0, 32065, 0,  2, "SCT-AMB-DT"
CHILLER,           1, COND-FAN-EIR,                                             "COND-FAN-EIR",     0, 32065, 0,  4, "COND-FAN-EIR"
CHILLER,           1, COND-PUMP-EIR,                                           "COND-PUMP-EIR",     0, 32065, 0,  4, "COND-PUMP-EIR"
CHILLER,           1, COND-CAP-FT,                                               "COND-CAP-FT",     0, 32065, 0,  0, "COND-CAP-FT"
CHILLER,           1, AMB-FRAC-FT,                                               "AMB-FRAC-FT",     0, 32065, 0,  0, "AMB-FRAC-FT"
CHILLER,           1, COND-PWR-FPLR,                                           "COND-PWR-FPLR",     0, 32065, 0,  0, "COND-PWR-FPLR"
CHILLER,           1, MAX-HTREC,                                       "Maximum Heat Recovery", 12960, 32065, 0,  2, "Maximum fraction of design condenser heat that is available for heat recovery"
CHILLER,           1, HTREC-LOOP,                                         "Heat Recovery Loop", 19114, 19114, 0,  0, "Name of the Heat Recovery Loop that this chiller rejects heat to"
CHILLER,           1, MAX-RECOVER-T,                                                        "", 13531, 32065, 0,  2, "Maximum temperature at which heat can be recovered from the chiller"
CHILLER,           1, HTREC-PUMP,                                                           "", 12998, 32065, 0,  2, "Name of pump dedicated to provide chiller's Heat Recovery Head and Heat Rec. Static Head"
CHILLER,           1, HTREC-DT,                                        "Heat Recovery Delta T", 13005, 32065, 0,  2, "Design temperature change of the water flowing through the heat-recovery condenser"
CHILLER,           1, HTREC-HEAD,                                                           "", 13001, 32065, 0,  2, "Pressure drop through the heat recovery heat exchanger at the design flow rate"
CHILLER,           1, HTREC-STATIC-HEA,                                                     "", 13002, 32065, 0,  2, "Static pressure drop through the heat recovery heat exchanger"
CHILLER,           1, HTREC-FLOW-CTRL,                                                      "", 12999, 32065, 0,  2, "The type of heat recovery water flow through the chiller"
CHILLER,           1, HTREC-MIN-FLOW,                                                       "", 13003, 32065, 0,  2, "Minimum allowable flow rate through the heat-recovery condenser"
CHILLER,           1, EVAP-HX-TD,                                                 "EVAP-HX-TD",     0, 32065, 0,  3, "EVAP-HX-TD"
CHILLER,           1, EVAP-HX-SETPT-T,                                       "EVAP-HX-SETPT-T",     0, 32065, 0,  2, "EVAP-HX-SETPT-T"
CHILLER,           1, COND-HX-TD,                                                 "COND-HX-TD",     0, 32065, 0,  3, "COND-HX-TD"
CHILLER,           1, COND-HX-SETPT-T,                                       "COND-HX-SETPT-T",     0, 32065, 0,  2, "COND-HX-SETPT-T"
CHILLER,           1, COST-DATA,                                                            "", 13799, 32065, 0,  2, "Name of a set of Materials Costs, which specifies first costs, maintenance costs, etc."
CHILLER,           1, EQUIPMENT-REPORT,                                                     "",     0, 32065, 0,  2, "Whether or not a PS-H report is created for this chiller"
CHILLER,           1, PICTURE,                                                              "",     0, 32065, 0,  2, ""
CHILLER,           1, DRAWING,                                                              "",     0, 32065, 0,  2, ""
CHILLER,           2, TYPE,                                                             "Type", 12873, 32065, 0,  0, "PowerDOE has models for nine types of chillers"
CHILLER,           2, CAPACITY,                                                     "Capacity", 13792, 32065, 0,  1, "Nominal (rated) chiller cooling capacity in MBTU/hr (e.g., 100 ton = 1.2 MBTU/hr)"
CHILLER,           2, CAPACITY-RATIO,                                         "Capactiy Ratio", 13793, 32065, 0,  1, "Capacity as fraction of max cooling load (used only if PowerDOE sizes the chiller)"
CHILLER,           2, CAPACITY-FT,                                               "Capacity FT", 12968, 32065, 0,  0, "Bi-Quadratic Curve: Capacity as function of temp of entering condenser & exiting chilled water"
CHILLER,           2, MIN-RATIO,                                               "Minimum Ratio", 12953, 32065, 0,  2, "Minimum chiller operating ratio (a fraction of the Capacity); below this, it cycles on & off"
; SAC 4/18/02 - removed CHILLER:MAX-RATIO
; CHILLER,           2, MAX-RATIO,                                               "Maximum Ratio", 12954, 32065, 0,  2, "Maximum allowable chiller operating ratio (fraction of Capacity, also called max overload ratio)"
CHILLER,           2, HGB-RATIO,                                                   "HGB Ratio", 12952, 32065, 0,  2, "Maximum allowable part-load ratio of the chiller, above which hot gas bypass occures"
CHILLER,           2, ELEC-INPUT-RATIO,                                 "Electric Input Ratio", 12879, 32065, 0,  2, "Dimensionless ratio of electric input power to nominal capacity (i.e., invers of COP)"
CHILLER,           2, EIR-FT,                                                               "", 12967, 32065, 0,  0, "Quadratic Curve Fit: EIR as a function of temp of water entering condenser & leaving chilled"
CHILLER,           2, EIR-FPLR,                                                             "", 12969, 32065, 0,  0, "Quadratic Curve Fit: Electric Input Ratio as a function of the part load ratio"
CHILLER,           2, ELEC-TO-COND,                                    "Electric To Condenser", 12957, 32065, 0,  2, "Efficiency of compressor: i.e., fraction of chiller electricity input rejected to condenser, as heat"
CHILLER,           2, HEAT-INPUT-RATIO,                                     "Heat Input Ratio", 12956, 32065, 0,  2, "Ratio of fuel heat input (in Btus) to full load cooling capacity (in Btus), as rated conditions"
CHILLER,           2, HIR-FT,                                                               "", 12964, 32065, 0,  0, "Bi-Quadratic Curve: HIR as a function of temp of entering condenser and exiting chilled water"
CHILLER,           2, HIR-FPLR,                                                             "", 12965, 32065, 0,  0, "Quadratic Curve Fit: Heat Input Ratio as a function of the part load ratio"
CHILLER,           2, HEAT-TO-COND,                                        "Heat to Condenser", 12882, 32065, 0,  2, "Fraction of fuel or heat input to chiller that is rejected to condenser, as heat"
CHILLER,           2, START-UP-TIME,                                                        "", 13644, 32065, 0,  2, "Equivalent full-load time required to start up the chiller (in hours or fraction of hours)"
CHILLER,           2, SHUT-DOWN-TIME,                                                       "", 13649, 32065, 0,  2, "Equivalent full-load time required to shut down the chiller (in hours or fraction of hours)"
CHILLER,           2, HGB-RATIO-HTREC,                                                      "", 12970, 32065, 0,  2, "The hot gas bypass ratio when the chiller is in the heat recovery mode"
CHILLER,           2, SOLUTION-PUMP-KW,                                                     "", 13650, 32065, 0,  2, "Electricity consumption of the solution pump"
CHILLER,           2, GAS-HCAP-FPLRC,                                                       "", 13787, 32065, 0,  2, "Quadratic Curve: heating capacity as a function of the cooling part load ratio"
CHILLER,           2, GAS-HW-XEFF,                                                          "", 13780, 32065, 0,  2, "The burner efficiency (when the chiller is in the heating mode)"
CHILLER,           2, GAS-DESC-XEFF,                                                        "", 13781, 32065, 0,  2, "The burner efficiency when regenerating a desiccant system"
CHILLER,           2, GAS-COMB-FAN-KW,                                                      "", 13778, 32065, 0,  2, "Electricity consumption of the combustion blower"
CHILLER,           2, GAS-HIR-FDESCT,                                                       "", 13788, 32065, 0,  2, "Quadratic Curve: Heat Input Ratio as a function of the desiccant regeneration temperature"
CHILLER,           2, GAS-QREG-FDESCT,                                                      "", 13789, 32065, 0,  2, "Quadratic Curve: available regeneration energy as a function of the required regeneration temp"
CHILLER,           2, ENG-HEAT-TO-JAC,                                                      "", 13848, 32065, 0,  2, "Fraction of design fuel consumption that is recoverable from the jacket of an engine-chiller"
CHILLER,           2, ENG-HEAT-TO-EXH,                                                      "", 13849, 32065, 0,  2, "Fraction of design fuel consumption that is recoverable from the exhaust of an engine-chiller"
CHILLER,           2, ENG-HTREJ-FT,                                                         "", 13785, 32065, 0,  2, "Quadratic Curve: the amount of recoverable heat as a function of the entering condenser temp"
CHILLER,           2, ENG-HTREJ-FPLR,                                                       "", 13784, 32065, 0,  2, "Quadratic Curve: amount of recoverable heat as a function of the cooling part load ratio"
CHILLER,           2, HEAT/COOL-CAP,                                           "HEAT/COOL-CAP",     0, 32065, 0,  3, "HEAT/COOL-CAP"
CHILLER,           2, HEAT-CAP-FT,                                               "HEAT-CAP-FT",     0, 32065, 0,  0, "HEAT-CAP-FT"
CHILLER,           2, HEAT-CAP-FT-FRST,                                     "HEAT-CAP-FT-FRST",     0, 32065, 0,  0, "HEAT-CAP-FT-FRST"
CHILLER,           2, HEAT-EIR,                                                     "HEAT-EIR",     0, 32065, 0,  3, "HEAT-EIR"
CHILLER,           2, HEAT-EIR-FT,                                               "HEAT-EIR-FT",     0, 32065, 0,  0, "HEAT-EIR-FT"
CHILLER,           2, HEAT-EIR-FT-FRST,                                     "HEAT-EIR-FT-FRST",     0, 32065, 0,  0, "HEAT-EIR-FT-FRST"
CHILLER,           2, HEAT-EIR-FPLR,                                           "HEAT-EIR-FPLR",     0, 32065, 0,  0, "HEAT-EIR-FPLR"
CHILLER,           2, AUX-KW,                                                   "Auxiliary kW", 13795, 32065, 0,  2, "Auxiliary electric power consumption of the chiler (e.g., control panels)"
CHILLER,           2, AUX-MODE,                                                             "", 12987, 32065, 0,  2, "Always=all hours;When On=If chiller on;When Off=if chiller off;Scheduled=use Aux Schedule"
CHILLER,           2, AUX-SCHEDULE,                                       "Auxiliary Schedule", 12988, 32065, 0,  2, "Schedule for Auxiliary Power consumption (set Auxiliary Mode to Scheduled to activate this)"
CHILLER,           2, AUX-METER,                                                            "", 12989, 32065, 0,  0, "Name of the Electric Meter that tallies the electricity consumption of this chiller's auxiliaries"
CHILLER,           2, ELEC-METER,                                             "Electric Meter", 12948, 32065, 0,  0, "Name of the Electric Meter that tallies the electric consumption of this chiller"
CHILLER,           2, FUEL-METER,                                                 "Fuel Meter", 12949, 32065, 0,  0, "Name of the Fuel Meter that tallies the fuel consumption of this chiller"
CHILLER,           2, CHW-LOOP,                                                     "CHW Loop", 19111, 32065, 0,  0, "Name of the primary Chiller Water Loop that this chiller serves"
CHILLER,           2, CHW-PUMP,                                                     "CHW Pump", 13800, 32065, 0,  0, "Name of a Pump that serves the chiller's chilled water loop"
CHILLER,           2, CHW-DT,                                                    "CHW Delta T", 12974, 32065, 0,  2, "Design temperature change of the chilled water through the chiller"
CHILLER,           2, CHW-HEAD,                                                             "", 12975, 32065, 0,  2, "Head loss through the chilled water piping at the design flow rate"
CHILLER,           2, CHW-STATIC-HEAD,                                                      "", 12976, 32065, 0,  2, "The static head in the chiller circuit (typically zero)"
CHILLER,           2, CHW-FLOW-CTRL,                                                        "", 12973, 32065, 0,  2, "The type of flow through the chiller evaporator"
CHILLER,           2, CHW-MIN-FLOW,                                                         "", 12977, 32065, 0,  2, "Minimum allowable fraction of the design flow rate through the evaporator"
CHILLER,           2, CHW-MAX-FLOW,                                                         "", 13491, 32065, 0,  2, "Maximum allowable fraction of the design flow rate through the evaporator"
CHILLER,           2, HW-LOOP,                                                       "HW Loop", 19117, 32065, 0,  0, "Name of HW loop that provides heat to an absorption chiller; or that a chiller/heater heats"
CHILLER,           2, HW-PUMP,                                                              "", 12991, 32065, 0,  2, "Hot Water pump: if not specified, the head requirement is passed to the primary loop"
CHILLER,           2, HW-DT,                                                      "HW Delta T", 12993, 32065, 0,  2, "Design temp change of hot water through the boiler (used to size recirculation pump)"
CHILLER,           2, HW-HEAD,                                                              "", 12994, 32065, 0,  2, "Pressure drop of the hot water through the chiller at the design flowrate"
CHILLER,           2, HW-STATIC-HEAD,                                                       "", 12995, 32065, 0,  2, "Static HW pressure drop through the chiller; use if pumping fluid at atm pressure into loop"
CHILLER,           2, HW-FLOW-CTRL,                                                         "", 12992, 32065, 0,  2, "Constant Flow = independent of the load; Variable Flow = varies linearly with load"
CHILLER,           2, HW-MIN-FLOW,                                                          "", 12996, 32065, 0,  2, "Min hot water flow rate through chiller; used only if Hot Water Flow Control = Variable Flow"
CHILLER,           2, HW-MAX-FLOW,                                                          "", 13492, 32065, 0,  2, "Max hot water flow rate through chiller; used only if Hot Water Flow Control = Variable Flow"
CHILLER,           2, CONDENSER-TYPE,                                         "Condenser Type", 12875, 32065, 0,  0, "Air Cooled=heat exchanger & condenser; Water Cooled=cooling tower & condenser loop"
CHILLER,           2, CW-LOOP,                                                       "CW Loop", 19112, 32065, 0,  0, "If Condenser Type=Water Cooled, CW Loop is required & must be attached to Cooling Tower"
CHILLER,           2, CW-PUMP,                                                       "CW Pump", 12929, 32065, 0,  0, "Name of a Pump that serves the (dedicated) evaporator recirculation loop"
CHILLER,           2, CW-DT,                                                      "CW Delta T", 12981, 32065, 0,  2, "Design temperature change of the water flowing through the condenser"
CHILLER,           2, CW-HEAD,                                                              "", 12982, 32065, 0,  2, "Pressure drop through the condenser at the design flow rate"
CHILLER,           2, CW-STATIC-HEAD,                                                       "", 12983, 32065, 0,  2, "Static pressure drop through the condenser at the design flow rate"
CHILLER,           2, CW-FLOW-CTRL,                                                         "", 12980, 32065, 0,  2, "The type of flow through the condenser"
CHILLER,           2, CW-MIN-FLOW,                                                          "", 12984, 32065, 0,  2, "Minimum allowable flow rate through the condenser (as a fraction of the design flow rate)"
CHILLER,           2, COND-SETPT-CTRL,                                       "COND-SETPT-CTRL",     0, 32065, 0,  0, "COND-SETPT-CTRL"
CHILLER,           2, COND-FAN-CTRL,                                           "COND-FAN-CTRL",     0, 32065, 0,  0, "COND-FAN-CTRL"
CHILLER,           2, COND-SETPT-T,                                             "COND-SETPT-T",     0, 32065, 0,  1, "COND-SETPT-T"
CHILLER,           2, COND-SETPT-DT,                                           "COND-SETPT-DT",     0, 32065, 0,  2, "COND-SETPT-DT"
CHILLER,           2, MIN-COND-T,                                                 "MIN-COND-T",     0, 32065, 0,  1, "MIN-COND-T"
CHILLER,           2, COND-CAPACITY,                                           "COND-CAPACITY",     0, 32065, 0,  3, "COND-CAPACITY"
CHILLER,           2, SCT-AMB-DT,                                                 "SCT-AMB-DT",     0, 32065, 0,  2, "SCT-AMB-DT"
CHILLER,           2, COND-FAN-EIR,                                             "COND-FAN-EIR",     0, 32065, 0,  4, "COND-FAN-EIR"
CHILLER,           2, COND-PUMP-EIR,                                           "COND-PUMP-EIR",     0, 32065, 0,  4, "COND-PUMP-EIR"
CHILLER,           2, COND-CAP-FT,                                               "COND-CAP-FT",     0, 32065, 0,  0, "COND-CAP-FT"
CHILLER,           2, AMB-FRAC-FT,                                               "AMB-FRAC-FT",     0, 32065, 0,  0, "AMB-FRAC-FT"
CHILLER,           2, COND-PWR-FPLR,                                           "COND-PWR-FPLR",     0, 32065, 0,  0, "COND-PWR-FPLR"
CHILLER,           2, MAX-HTREC,                                       "Maximum Heat Recovery", 12960, 32065, 0,  2, "Maximum fraction of design condenser heat that is available for heat recovery"
CHILLER,           2, HTREC-LOOP,                                         "Heat Recovery Loop", 19114, 19114, 0,  0, "Name of the Heat Recovery Loop that this chiller rejects heat to"
CHILLER,           2, MAX-RECOVER-T,                                                        "", 13531, 32065, 0,  2, "Maximum temperature at which heat can be recovered from the chiller"
CHILLER,           2, HTREC-PUMP,                                                           "", 12998, 32065, 0,  2, "Name of pump dedicated to provide chiller's Heat Recovery Head and Heat Rec. Static Head"
CHILLER,           2, HTREC-DT,                                        "Heat Recovery Delta T", 13005, 32065, 0,  2, "Design temperature change of the water flowing through the heat-recovery condenser"
CHILLER,           2, HTREC-HEAD,                                                           "", 13001, 32065, 0,  2, "Pressure drop through the heat recovery heat exchanger at the design flow rate"
CHILLER,           2, HTREC-STATIC-HEA,                                                     "", 13002, 32065, 0,  2, "Static pressure drop through the heat recovery heat exchanger"
CHILLER,           2, HTREC-FLOW-CTRL,                                                      "", 12999, 32065, 0,  2, "The type of heat recovery water flow through the chiller"
CHILLER,           2, HTREC-MIN-FLOW,                                                       "", 13003, 32065, 0,  2, "Minimum allowable flow rate through the heat-recovery condenser"
CHILLER,           2, EVAP-HX-TD,                                                 "EVAP-HX-TD",     0, 32065, 0,  3, "EVAP-HX-TD"
CHILLER,           2, EVAP-HX-SETPT-T,                                       "EVAP-HX-SETPT-T",     0, 32065, 0,  2, "EVAP-HX-SETPT-T"
CHILLER,           2, COND-HX-TD,                                                 "COND-HX-TD",     0, 32065, 0,  3, "COND-HX-TD"
CHILLER,           2, COND-HX-SETPT-T,                                       "COND-HX-SETPT-T",     0, 32065, 0,  2, "COND-HX-SETPT-T"
CHILLER,           2, COST-DATA,                                                            "", 13799, 32065, 0,  2, "Name of a set of Materials Costs, which specifies first costs, maintenance costs, etc."
CHILLER,           2, EQUIPMENT-REPORT,                                                     "",     0, 32065, 0,  2, "Whether or not a PS-H report is created for this chiller"
CHILLER,           2, PICTURE,                                                              "",     0, 32065, 0,  2, ""
CHILLER,           2, DRAWING,                                                              "",     0, 32065, 0,  2, ""
CHILLER,           3, TYPE,                                                             "Type", 12873, 32065, 0,  0, "PowerDOE has models for nine types of chillers"
CHILLER,           3, CAPACITY,                                                     "Capacity", 13792, 32065, 0,  1, "Nominal (rated) chiller cooling capacity in MBTU/hr (e.g., 100 ton = 1.2 MBTU/hr)"
CHILLER,           3, CAPACITY-RATIO,                                         "Capactiy Ratio", 13793, 32065, 0,  1, "Capacity as fraction of max cooling load (used only if PowerDOE sizes the chiller)"
CHILLER,           3, CAPACITY-FT,                                               "Capacity FT", 12968, 32065, 0,  0, "Bi-Quadratic Curve: Capacity as function of temp of entering condenser & exiting chilled water"
CHILLER,           3, MIN-RATIO,                                               "Minimum Ratio", 12953, 32065, 0,  2, "Minimum chiller operating ratio (a fraction of the Capacity); below this, it cycles on & off"
; SAC 4/18/02 - removed CHILLER:MAX-RATIO
; CHILLER,           3, MAX-RATIO,                                               "Maximum Ratio", 12954, 32065, 0,  2, "Maximum allowable chiller operating ratio (fraction of Capacity, also called max overload ratio)"
CHILLER,           3, HGB-RATIO,                                                   "HGB Ratio", 12952, 32065, 0,  2, "Maximum allowable part-load ratio of the chiller, above which hot gas bypass occures"
CHILLER,           3, ELEC-INPUT-RATIO,                                 "Electric Input Ratio", 12879, 32065, 0,  2, "Dimensionless ratio of electric input power to nominal capacity (i.e., invers of COP)"
CHILLER,           3, EIR-FT,                                                               "", 12967, 32065, 0,  0, "Quadratic Curve Fit: EIR as a function of temp of water entering condenser & leaving chilled"
CHILLER,           3, EIR-FPLR,                                                             "", 12969, 32065, 0,  0, "Quadratic Curve Fit: Electric Input Ratio as a function of the part load ratio"
CHILLER,           3, ELEC-TO-COND,                                    "Electric To Condenser", 12957, 32065, 0,  2, "Efficiency of compressor: i.e., fraction of chiller electricity input rejected to condenser, as heat"
CHILLER,           3, HEAT-INPUT-RATIO,                                     "Heat Input Ratio", 12956, 32065, 0,  2, "Ratio of fuel heat input (in Btus) to full load cooling capacity (in Btus), as rated conditions"
CHILLER,           3, HIR-FT,                                                               "", 12964, 32065, 0,  0, "Bi-Quadratic Curve: HIR as a function of temp of entering condenser and exiting chilled water"
CHILLER,           3, HIR-FPLR,                                                             "", 12965, 32065, 0,  0, "Quadratic Curve Fit: Heat Input Ratio as a function of the part load ratio"
CHILLER,           3, HEAT-TO-COND,                                        "Heat to Condenser", 12882, 32065, 0,  2, "Fraction of fuel or heat input to chiller that is rejected to condenser, as heat"
CHILLER,           3, START-UP-TIME,                                                        "", 13644, 32065, 0,  2, "Equivalent full-load time required to start up the chiller (in hours or fraction of hours)"
CHILLER,           3, SHUT-DOWN-TIME,                                                       "", 13649, 32065, 0,  2, "Equivalent full-load time required to shut down the chiller (in hours or fraction of hours)"
CHILLER,           3, HGB-RATIO-HTREC,                                                      "", 12970, 32065, 0,  2, "The hot gas bypass ratio when the chiller is in the heat recovery mode"
CHILLER,           3, SOLUTION-PUMP-KW,                                                     "", 13650, 32065, 0,  2, "Electricity consumption of the solution pump"
CHILLER,           3, GAS-HCAP-FPLRC,                                                       "", 13787, 32065, 0,  2, "Quadratic Curve: heating capacity as a function of the cooling part load ratio"
CHILLER,           3, GAS-HW-XEFF,                                                          "", 13780, 32065, 0,  2, "The burner efficiency (when the chiller is in the heating mode)"
CHILLER,           3, GAS-DESC-XEFF,                                                        "", 13781, 32065, 0,  2, "The burner efficiency when regenerating a desiccant system"
CHILLER,           3, GAS-COMB-FAN-KW,                                                      "", 13778, 32065, 0,  2, "Electricity consumption of the combustion blower"
CHILLER,           3, GAS-HIR-FDESCT,                                                       "", 13788, 32065, 0,  2, "Quadratic Curve: Heat Input Ratio as a function of the desiccant regeneration temperature"
CHILLER,           3, GAS-QREG-FDESCT,                                                      "", 13789, 32065, 0,  2, "Quadratic Curve: available regeneration energy as a function of the required regeneration temp"
CHILLER,           3, ENG-HEAT-TO-JAC,                                                      "", 13848, 32065, 0,  2, "Fraction of design fuel consumption that is recoverable from the jacket of an engine-chiller"
CHILLER,           3, ENG-HEAT-TO-EXH,                                                      "", 13849, 32065, 0,  2, "Fraction of design fuel consumption that is recoverable from the exhaust of an engine-chiller"
CHILLER,           3, ENG-HTREJ-FT,                                                         "", 13785, 32065, 0,  2, "Quadratic Curve: the amount of recoverable heat as a function of the entering condenser temp"
CHILLER,           3, ENG-HTREJ-FPLR,                                                       "", 13784, 32065, 0,  2, "Quadratic Curve: amount of recoverable heat as a function of the cooling part load ratio"
CHILLER,           3, HEAT/COOL-CAP,                                           "HEAT/COOL-CAP",     0, 32065, 0,  3, "HEAT/COOL-CAP"
CHILLER,           3, HEAT-CAP-FT,                                               "HEAT-CAP-FT",     0, 32065, 0,  0, "HEAT-CAP-FT"
CHILLER,           3, HEAT-CAP-FT-FRST,                                     "HEAT-CAP-FT-FRST",     0, 32065, 0,  0, "HEAT-CAP-FT-FRST"
CHILLER,           3, HEAT-EIR,                                                     "HEAT-EIR",     0, 32065, 0,  3, "HEAT-EIR"
CHILLER,           3, HEAT-EIR-FT,                                               "HEAT-EIR-FT",     0, 32065, 0,  0, "HEAT-EIR-FT"
CHILLER,           3, HEAT-EIR-FT-FRST,                                     "HEAT-EIR-FT-FRST",     0, 32065, 0,  0, "HEAT-EIR-FT-FRST"
CHILLER,           3, HEAT-EIR-FPLR,                                           "HEAT-EIR-FPLR",     0, 32065, 0,  0, "HEAT-EIR-FPLR"
CHILLER,           3, AUX-KW,                                                   "Auxiliary kW", 13795, 32065, 0,  2, "Auxiliary electric power consumption of the chiler (e.g., control panels)"
CHILLER,           3, AUX-MODE,                                                             "", 12987, 32065, 0,  2, "Always=all hours;When On=If chiller on;When Off=if chiller off;Scheduled=use Aux Schedule"
CHILLER,           3, AUX-SCHEDULE,                                       "Auxiliary Schedule", 12988, 32065, 0,  2, "Schedule for Auxiliary Power consumption (set Auxiliary Mode to Scheduled to activate this)"
CHILLER,           3, AUX-METER,                                                            "", 12989, 32065, 0,  0, "Name of the Electric Meter that tallies the electricity consumption of this chiller's auxiliaries"
CHILLER,           3, ELEC-METER,                                             "Electric Meter", 12948, 32065, 0,  0, "Name of the Electric Meter that tallies the electric consumption of this chiller"
CHILLER,           3, FUEL-METER,                                                 "Fuel Meter", 12949, 32065, 0,  0, "Name of the Fuel Meter that tallies the fuel consumption of this chiller"
CHILLER,           3, CHW-LOOP,                                                     "CHW Loop", 19111, 32065, 0,  0, "Name of the primary Chiller Water Loop that this chiller serves"
CHILLER,           3, CHW-PUMP,                                                     "CHW Pump", 13800, 32065, 0,  0, "Name of a Pump that serves the chiller's chilled water loop"
CHILLER,           3, CHW-DT,                                                    "CHW Delta T", 12974, 32065, 0,  2, "Design temperature change of the chilled water through the chiller"
CHILLER,           3, CHW-HEAD,                                                             "", 12975, 32065, 0,  2, "Head loss through the chilled water piping at the design flow rate"
CHILLER,           3, CHW-STATIC-HEAD,                                                      "", 12976, 32065, 0,  2, "The static head in the chiller circuit (typically zero)"
CHILLER,           3, CHW-FLOW-CTRL,                                                        "", 12973, 32065, 0,  2, "The type of flow through the chiller evaporator"
CHILLER,           3, CHW-MIN-FLOW,                                                         "", 12977, 32065, 0,  2, "Minimum allowable fraction of the design flow rate through the evaporator"
CHILLER,           3, CHW-MAX-FLOW,                                                         "", 13491, 32065, 0,  2, "Maximum allowable fraction of the design flow rate through the evaporator"
CHILLER,           3, HW-LOOP,                                                       "HW Loop", 19117, 32065, 0,  0, "Name of HW loop that provides heat to an absorption chiller; or that a chiller/heater heats"
CHILLER,           3, HW-PUMP,                                                              "", 12991, 32065, 0,  2, "Hot Water pump: if not specified, the head requirement is passed to the primary loop"
CHILLER,           3, HW-DT,                                                      "HW Delta T", 12993, 32065, 0,  2, "Design temp change of hot water through the boiler (used to size recirculation pump)"
CHILLER,           3, HW-HEAD,                                                              "", 12994, 32065, 0,  2, "Pressure drop of the hot water through the chiller at the design flowrate"
CHILLER,           3, HW-STATIC-HEAD,                                                       "", 12995, 32065, 0,  2, "Static HW pressure drop through the chiller; use if pumping fluid at atm pressure into loop"
CHILLER,           3, HW-FLOW-CTRL,                                                         "", 12992, 32065, 0,  2, "Constant Flow = independent of the load; Variable Flow = varies linearly with load"
CHILLER,           3, HW-MIN-FLOW,                                                          "", 12996, 32065, 0,  2, "Min hot water flow rate through chiller; used only if Hot Water Flow Control = Variable Flow"
CHILLER,           3, HW-MAX-FLOW,                                                          "", 13492, 32065, 0,  2, "Max hot water flow rate through chiller; used only if Hot Water Flow Control = Variable Flow"
CHILLER,           3, CONDENSER-TYPE,                                         "Condenser Type", 12875, 32065, 0,  0, "Air Cooled=heat exchanger & condenser; Water Cooled=cooling tower & condenser loop"
CHILLER,           3, CW-LOOP,                                                       "CW Loop", 19112, 32065, 0,  0, "If Condenser Type=Water Cooled, CW Loop is required & must be attached to Cooling Tower"
CHILLER,           3, CW-PUMP,                                                       "CW Pump", 12929, 32065, 0,  0, "Name of a Pump that serves the (dedicated) evaporator recirculation loop"
CHILLER,           3, CW-DT,                                                      "CW Delta T", 12981, 32065, 0,  2, "Design temperature change of the water flowing through the condenser"
CHILLER,           3, CW-HEAD,                                                              "", 12982, 32065, 0,  2, "Pressure drop through the condenser at the design flow rate"
CHILLER,           3, CW-STATIC-HEAD,                                                       "", 12983, 32065, 0,  2, "Static pressure drop through the condenser at the design flow rate"
CHILLER,           3, CW-FLOW-CTRL,                                                         "", 12980, 32065, 0,  2, "The type of flow through the condenser"
CHILLER,           3, CW-MIN-FLOW,                                                          "", 12984, 32065, 0,  2, "Minimum allowable flow rate through the condenser (as a fraction of the design flow rate)"
CHILLER,           3, COND-SETPT-CTRL,                                       "COND-SETPT-CTRL",     0, 32065, 0,  0, "COND-SETPT-CTRL"
CHILLER,           3, COND-FAN-CTRL,                                           "COND-FAN-CTRL",     0, 32065, 0,  0, "COND-FAN-CTRL"
CHILLER,           3, COND-SETPT-T,                                             "COND-SETPT-T",     0, 32065, 0,  1, "COND-SETPT-T"
CHILLER,           3, COND-SETPT-DT,                                           "COND-SETPT-DT",     0, 32065, 0,  2, "COND-SETPT-DT"
CHILLER,           3, MIN-COND-T,                                                 "MIN-COND-T",     0, 32065, 0,  1, "MIN-COND-T"
CHILLER,           3, COND-CAPACITY,                                           "COND-CAPACITY",     0, 32065, 0,  3, "COND-CAPACITY"
CHILLER,           3, SCT-AMB-DT,                                                 "SCT-AMB-DT",     0, 32065, 0,  2, "SCT-AMB-DT"
CHILLER,           3, COND-FAN-EIR,                                             "COND-FAN-EIR",     0, 32065, 0,  4, "COND-FAN-EIR"
CHILLER,           3, COND-PUMP-EIR,                                           "COND-PUMP-EIR",     0, 32065, 0,  4, "COND-PUMP-EIR"
CHILLER,           3, COND-CAP-FT,                                               "COND-CAP-FT",     0, 32065, 0,  0, "COND-CAP-FT"
CHILLER,           3, AMB-FRAC-FT,                                               "AMB-FRAC-FT",     0, 32065, 0,  0, "AMB-FRAC-FT"
CHILLER,           3, COND-PWR-FPLR,                                           "COND-PWR-FPLR",     0, 32065, 0,  0, "COND-PWR-FPLR"
CHILLER,           3, MAX-HTREC,                                       "Maximum Heat Recovery", 12960, 32065, 0,  2, "Maximum fraction of design condenser heat that is available for heat recovery"
CHILLER,           3, HTREC-LOOP,                                         "Heat Recovery Loop", 19114, 19114, 0,  0, "Name of the Heat Recovery Loop that this chiller rejects heat to"
CHILLER,           3, MAX-RECOVER-T,                                                        "", 13531, 32065, 0,  2, "Maximum temperature at which heat can be recovered from the chiller"
CHILLER,           3, HTREC-PUMP,                                                           "", 12998, 32065, 0,  2, "Name of pump dedicated to provide chiller's Heat Recovery Head and Heat Rec. Static Head"
CHILLER,           3, HTREC-DT,                                        "Heat Recovery Delta T", 13005, 32065, 0,  2, "Design temperature change of the water flowing through the heat-recovery condenser"
CHILLER,           3, HTREC-HEAD,                                                           "", 13001, 32065, 0,  2, "Pressure drop through the heat recovery heat exchanger at the design flow rate"
CHILLER,           3, HTREC-STATIC-HEA,                                                     "", 13002, 32065, 0,  2, "Static pressure drop through the heat recovery heat exchanger"
CHILLER,           3, HTREC-FLOW-CTRL,                                                      "", 12999, 32065, 0,  2, "The type of heat recovery water flow through the chiller"
CHILLER,           3, HTREC-MIN-FLOW,                                                       "", 13003, 32065, 0,  2, "Minimum allowable flow rate through the heat-recovery condenser"
CHILLER,           3, EVAP-HX-TD,                                                 "EVAP-HX-TD",     0, 32065, 0,  3, "EVAP-HX-TD"
CHILLER,           3, EVAP-HX-SETPT-T,                                       "EVAP-HX-SETPT-T",     0, 32065, 0,  2, "EVAP-HX-SETPT-T"
CHILLER,           3, COND-HX-TD,                                                 "COND-HX-TD",     0, 32065, 0,  3, "COND-HX-TD"
CHILLER,           3, COND-HX-SETPT-T,                                       "COND-HX-SETPT-T",     0, 32065, 0,  2, "COND-HX-SETPT-T"
CHILLER,           3, COST-DATA,                                                            "", 13799, 32065, 0,  2, "Name of a set of Materials Costs, which specifies first costs, maintenance costs, etc."
CHILLER,           3, EQUIPMENT-REPORT,                                                     "",     0, 32065, 0,  2, "Whether or not a PS-H report is created for this chiller"
CHILLER,           3, PICTURE,                                                              "",     0, 32065, 0,  2, ""
CHILLER,           3, DRAWING,                                                              "",     0, 32065, 0,  2, ""
CHILLER,           4, TYPE,                                                             "Type", 12873, 32065, 0,  0, "PowerDOE has models for nine types of chillers"
CHILLER,           4, CAPACITY,                                                     "Capacity", 13792, 32065, 0,  1, "Nominal (rated) chiller cooling capacity in MBTU/hr (e.g., 100 ton = 1.2 MBTU/hr)"
CHILLER,           4, CAPACITY-RATIO,                                         "Capactiy Ratio", 13793, 32065, 0,  1, "Capacity as fraction of max cooling load (used only if PowerDOE sizes the chiller)"
CHILLER,           4, CAPACITY-FT,                                               "Capacity FT", 12968, 32065, 0,  0, "Bi-Quadratic Curve: Capacity as function of temp of entering condenser & exiting chilled water"
CHILLER,           4, MIN-RATIO,                                               "Minimum Ratio", 12953, 32065, 0,  2, "Minimum chiller operating ratio (a fraction of the Capacity); below this, it cycles on & off"
; SAC 4/18/02 - removed CHILLER:MAX-RATIO
; CHILLER,           4, MAX-RATIO,                                               "Maximum Ratio", 12954, 32065, 0,  2, "Maximum allowable chiller operating ratio (fraction of Capacity, also called max overload ratio)"
CHILLER,           4, HGB-RATIO,                                                   "HGB Ratio", 12952, 32065, 0,  2, "Maximum allowable part-load ratio of the chiller, above which hot gas bypass occures"
CHILLER,           4, ELEC-INPUT-RATIO,                                 "Electric Input Ratio", 12879, 32065, 0,  2, "Dimensionless ratio of electric input power to nominal capacity (i.e., invers of COP)"
CHILLER,           4, EIR-FT,                                                               "", 12967, 32065, 0,  0, "Quadratic Curve Fit: EIR as a function of temp of water entering condenser & leaving chilled"
CHILLER,           4, EIR-FPLR,                                                             "", 12969, 32065, 0,  0, "Quadratic Curve Fit: Electric Input Ratio as a function of the part load ratio"
CHILLER,           4, ELEC-TO-COND,                                    "Electric To Condenser", 12957, 32065, 0,  2, "Efficiency of compressor: i.e., fraction of chiller electricity input rejected to condenser, as heat"
CHILLER,           4, HEAT-INPUT-RATIO,                                     "Heat Input Ratio", 12956, 32065, 0,  2, "Ratio of fuel heat input (in Btus) to full load cooling capacity (in Btus), as rated conditions"
CHILLER,           4, HIR-FT,                                                               "", 12964, 32065, 0,  0, "Bi-Quadratic Curve: HIR as a function of temp of entering condenser and exiting chilled water"
CHILLER,           4, HIR-FPLR,                                                             "", 12965, 32065, 0,  0, "Quadratic Curve Fit: Heat Input Ratio as a function of the part load ratio"
CHILLER,           4, HEAT-TO-COND,                                        "Heat to Condenser", 12882, 32065, 0,  2, "Fraction of fuel or heat input to chiller that is rejected to condenser, as heat"
CHILLER,           4, START-UP-TIME,                                                        "", 13644, 32065, 0,  2, "Equivalent full-load time required to start up the chiller (in hours or fraction of hours)"
CHILLER,           4, SHUT-DOWN-TIME,                                                       "", 13649, 32065, 0,  2, "Equivalent full-load time required to shut down the chiller (in hours or fraction of hours)"
CHILLER,           4, HGB-RATIO-HTREC,                                                      "", 12970, 32065, 0,  2, "The hot gas bypass ratio when the chiller is in the heat recovery mode"
CHILLER,           4, SOLUTION-PUMP-KW,                                                     "", 13650, 32065, 0,  2, "Electricity consumption of the solution pump"
CHILLER,           4, GAS-HCAP-FPLRC,                                                       "", 13787, 32065, 0,  2, "Quadratic Curve: heating capacity as a function of the cooling part load ratio"
CHILLER,           4, GAS-HW-XEFF,                                                          "", 13780, 32065, 0,  2, "The burner efficiency (when the chiller is in the heating mode)"
CHILLER,           4, GAS-DESC-XEFF,                                                        "", 13781, 32065, 0,  2, "The burner efficiency when regenerating a desiccant system"
CHILLER,           4, GAS-COMB-FAN-KW,                                                      "", 13778, 32065, 0,  2, "Electricity consumption of the combustion blower"
CHILLER,           4, GAS-HIR-FDESCT,                                                       "", 13788, 32065, 0,  2, "Quadratic Curve: Heat Input Ratio as a function of the desiccant regeneration temperature"
CHILLER,           4, GAS-QREG-FDESCT,                                                      "", 13789, 32065, 0,  2, "Quadratic Curve: available regeneration energy as a function of the required regeneration temp"
CHILLER,           4, ENG-HEAT-TO-JAC,                                                      "", 13848, 32065, 0,  2, "Fraction of design fuel consumption that is recoverable from the jacket of an engine-chiller"
CHILLER,           4, ENG-HEAT-TO-EXH,                                                      "", 13849, 32065, 0,  2, "Fraction of design fuel consumption that is recoverable from the exhaust of an engine-chiller"
CHILLER,           4, ENG-HTREJ-FT,                                                         "", 13785, 32065, 0,  2, "Quadratic Curve: the amount of recoverable heat as a function of the entering condenser temp"
CHILLER,           4, ENG-HTREJ-FPLR,                                                       "", 13784, 32065, 0,  2, "Quadratic Curve: amount of recoverable heat as a function of the cooling part load ratio"
CHILLER,           4, HEAT/COOL-CAP,                                           "HEAT/COOL-CAP",     0, 32065, 0,  3, "HEAT/COOL-CAP"
CHILLER,           4, HEAT-CAP-FT,                                               "HEAT-CAP-FT",     0, 32065, 0,  0, "HEAT-CAP-FT"
CHILLER,           4, HEAT-CAP-FT-FRST,                                     "HEAT-CAP-FT-FRST",     0, 32065, 0,  0, "HEAT-CAP-FT-FRST"
CHILLER,           4, HEAT-EIR,                                                     "HEAT-EIR",     0, 32065, 0,  3, "HEAT-EIR"
CHILLER,           4, HEAT-EIR-FT,                                               "HEAT-EIR-FT",     0, 32065, 0,  0, "HEAT-EIR-FT"
CHILLER,           4, HEAT-EIR-FT-FRST,                                     "HEAT-EIR-FT-FRST",     0, 32065, 0,  0, "HEAT-EIR-FT-FRST"
CHILLER,           4, HEAT-EIR-FPLR,                                           "HEAT-EIR-FPLR",     0, 32065, 0,  0, "HEAT-EIR-FPLR"
CHILLER,           4, AUX-KW,                                                   "Auxiliary kW", 13795, 32065, 0,  2, "Auxiliary electric power consumption of the chiler (e.g., control panels)"
CHILLER,           4, AUX-MODE,                                                             "", 12987, 32065, 0,  2, "Always=all hours;When On=If chiller on;When Off=if chiller off;Scheduled=use Aux Schedule"
CHILLER,           4, AUX-SCHEDULE,                                       "Auxiliary Schedule", 12988, 32065, 0,  2, "Schedule for Auxiliary Power consumption (set Auxiliary Mode to Scheduled to activate this)"
CHILLER,           4, AUX-METER,                                                            "", 12989, 32065, 0,  0, "Name of the Electric Meter that tallies the electricity consumption of this chiller's auxiliaries"
CHILLER,           4, ELEC-METER,                                             "Electric Meter", 12948, 32065, 0,  0, "Name of the Electric Meter that tallies the electric consumption of this chiller"
CHILLER,           4, FUEL-METER,                                                 "Fuel Meter", 12949, 32065, 0,  0, "Name of the Fuel Meter that tallies the fuel consumption of this chiller"
CHILLER,           4, CHW-LOOP,                                                     "CHW Loop", 19111, 32065, 0,  0, "Name of the primary Chiller Water Loop that this chiller serves"
CHILLER,           4, CHW-PUMP,                                                     "CHW Pump", 13800, 32065, 0,  0, "Name of a Pump that serves the chiller's chilled water loop"
CHILLER,           4, CHW-DT,                                                    "CHW Delta T", 12974, 32065, 0,  2, "Design temperature change of the chilled water through the chiller"
CHILLER,           4, CHW-HEAD,                                                             "", 12975, 32065, 0,  2, "Head loss through the chilled water piping at the design flow rate"
CHILLER,           4, CHW-STATIC-HEAD,                                                      "", 12976, 32065, 0,  2, "The static head in the chiller circuit (typically zero)"
CHILLER,           4, CHW-FLOW-CTRL,                                                        "", 12973, 32065, 0,  2, "The type of flow through the chiller evaporator"
CHILLER,           4, CHW-MIN-FLOW,                                                         "", 12977, 32065, 0,  2, "Minimum allowable fraction of the design flow rate through the evaporator"
CHILLER,           4, CHW-MAX-FLOW,                                                         "", 13491, 32065, 0,  2, "Maximum allowable fraction of the design flow rate through the evaporator"
CHILLER,           4, HW-LOOP,                                                       "HW Loop", 19117, 32065, 0,  0, "Name of HW loop that provides heat to an absorption chiller; or that a chiller/heater heats"
CHILLER,           4, HW-PUMP,                                                              "", 12991, 32065, 0,  2, "Hot Water pump: if not specified, the head requirement is passed to the primary loop"
CHILLER,           4, HW-DT,                                                      "HW Delta T", 12993, 32065, 0,  2, "Design temp change of hot water through the boiler (used to size recirculation pump)"
CHILLER,           4, HW-HEAD,                                                              "", 12994, 32065, 0,  2, "Pressure drop of the hot water through the chiller at the design flowrate"
CHILLER,           4, HW-STATIC-HEAD,                                                       "", 12995, 32065, 0,  2, "Static HW pressure drop through the chiller; use if pumping fluid at atm pressure into loop"
CHILLER,           4, HW-FLOW-CTRL,                                                         "", 12992, 32065, 0,  2, "Constant Flow = independent of the load; Variable Flow = varies linearly with load"
CHILLER,           4, HW-MIN-FLOW,                                                          "", 12996, 32065, 0,  2, "Min hot water flow rate through chiller; used only if Hot Water Flow Control = Variable Flow"
CHILLER,           4, HW-MAX-FLOW,                                                          "", 13492, 32065, 0,  2, "Max hot water flow rate through chiller; used only if Hot Water Flow Control = Variable Flow"
CHILLER,           4, CONDENSER-TYPE,                                         "Condenser Type", 12875, 32065, 0,  0, "Air Cooled=heat exchanger & condenser; Water Cooled=cooling tower & condenser loop"
CHILLER,           4, CW-LOOP,                                                       "CW Loop", 19112, 32065, 0,  0, "If Condenser Type=Water Cooled, CW Loop is required & must be attached to Cooling Tower"
CHILLER,           4, CW-PUMP,                                                       "CW Pump", 12929, 32065, 0,  0, "Name of a Pump that serves the (dedicated) evaporator recirculation loop"
CHILLER,           4, CW-DT,                                                      "CW Delta T", 12981, 32065, 0,  2, "Design temperature change of the water flowing through the condenser"
CHILLER,           4, CW-HEAD,                                                              "", 12982, 32065, 0,  2, "Pressure drop through the condenser at the design flow rate"
CHILLER,           4, CW-STATIC-HEAD,                                                       "", 12983, 32065, 0,  2, "Static pressure drop through the condenser at the design flow rate"
CHILLER,           4, CW-FLOW-CTRL,                                                         "", 12980, 32065, 0,  2, "The type of flow through the condenser"
CHILLER,           4, CW-MIN-FLOW,                                                          "", 12984, 32065, 0,  2, "Minimum allowable flow rate through the condenser (as a fraction of the design flow rate)"
CHILLER,           4, COND-SETPT-CTRL,                                       "COND-SETPT-CTRL",     0, 32065, 0,  0, "COND-SETPT-CTRL"
CHILLER,           4, COND-FAN-CTRL,                                           "COND-FAN-CTRL",     0, 32065, 0,  0, "COND-FAN-CTRL"
CHILLER,           4, COND-SETPT-T,                                             "COND-SETPT-T",     0, 32065, 0,  1, "COND-SETPT-T"
CHILLER,           4, COND-SETPT-DT,                                           "COND-SETPT-DT",     0, 32065, 0,  2, "COND-SETPT-DT"
CHILLER,           4, MIN-COND-T,                                                 "MIN-COND-T",     0, 32065, 0,  1, "MIN-COND-T"
CHILLER,           4, COND-CAPACITY,                                           "COND-CAPACITY",     0, 32065, 0,  3, "COND-CAPACITY"
CHILLER,           4, SCT-AMB-DT,                                                 "SCT-AMB-DT",     0, 32065, 0,  2, "SCT-AMB-DT"
CHILLER,           4, COND-FAN-EIR,                                             "COND-FAN-EIR",     0, 32065, 0,  4, "COND-FAN-EIR"
CHILLER,           4, COND-PUMP-EIR,                                           "COND-PUMP-EIR",     0, 32065, 0,  4, "COND-PUMP-EIR"
CHILLER,           4, COND-CAP-FT,                                               "COND-CAP-FT",     0, 32065, 0,  0, "COND-CAP-FT"
CHILLER,           4, AMB-FRAC-FT,                                               "AMB-FRAC-FT",     0, 32065, 0,  0, "AMB-FRAC-FT"
CHILLER,           4, COND-PWR-FPLR,                                           "COND-PWR-FPLR",     0, 32065, 0,  0, "COND-PWR-FPLR"
CHILLER,           4, MAX-HTREC,                                       "Maximum Heat Recovery", 12960, 32065, 0,  2, "Maximum fraction of design condenser heat that is available for heat recovery"
CHILLER,           4, HTREC-LOOP,                                         "Heat Recovery Loop", 19114, 19114, 0,  0, "Name of the Heat Recovery Loop that this chiller rejects heat to"
CHILLER,           4, MAX-RECOVER-T,                                                        "", 13531, 32065, 0,  2, "Maximum temperature at which heat can be recovered from the chiller"
CHILLER,           4, HTREC-PUMP,                                                           "", 12998, 32065, 0,  2, "Name of pump dedicated to provide chiller's Heat Recovery Head and Heat Rec. Static Head"
CHILLER,           4, HTREC-DT,                                        "Heat Recovery Delta T", 13005, 32065, 0,  2, "Design temperature change of the water flowing through the heat-recovery condenser"
CHILLER,           4, HTREC-HEAD,                                                           "", 13001, 32065, 0,  2, "Pressure drop through the heat recovery heat exchanger at the design flow rate"
CHILLER,           4, HTREC-STATIC-HEA,                                                     "", 13002, 32065, 0,  2, "Static pressure drop through the heat recovery heat exchanger"
CHILLER,           4, HTREC-FLOW-CTRL,                                                      "", 12999, 32065, 0,  2, "The type of heat recovery water flow through the chiller"
CHILLER,           4, HTREC-MIN-FLOW,                                                       "", 13003, 32065, 0,  2, "Minimum allowable flow rate through the heat-recovery condenser"
CHILLER,           4, EVAP-HX-TD,                                                 "EVAP-HX-TD",     0, 32065, 0,  3, "EVAP-HX-TD"
CHILLER,           4, EVAP-HX-SETPT-T,                                       "EVAP-HX-SETPT-T",     0, 32065, 0,  2, "EVAP-HX-SETPT-T"
CHILLER,           4, COND-HX-TD,                                                 "COND-HX-TD",     0, 32065, 0,  3, "COND-HX-TD"
CHILLER,           4, COND-HX-SETPT-T,                                       "COND-HX-SETPT-T",     0, 32065, 0,  2, "COND-HX-SETPT-T"
CHILLER,           4, COST-DATA,                                                            "", 13799, 32065, 0,  2, "Name of a set of Materials Costs, which specifies first costs, maintenance costs, etc."
CHILLER,           4, EQUIPMENT-REPORT,                                                     "",     0, 32065, 0,  2, "Whether or not a PS-H report is created for this chiller"
CHILLER,           4, PICTURE,                                                              "",     0, 32065, 0,  2, ""
CHILLER,           4, DRAWING,                                                              "",     0, 32065, 0,  2, ""
CHILLER,           5, TYPE,                                                             "Type", 12873, 32065, 0,  0, "PowerDOE has models for nine types of chillers"
CHILLER,           5, CAPACITY,                                                     "Capacity", 13792, 32065, 0,  1, "Nominal (rated) chiller cooling capacity in MBTU/hr (e.g., 100 ton = 1.2 MBTU/hr)"
CHILLER,           5, CAPACITY-RATIO,                                         "Capactiy Ratio", 13793, 32065, 0,  1, "Capacity as fraction of max cooling load (used only if PowerDOE sizes the chiller)"
CHILLER,           5, CAPACITY-FT,                                               "Capacity FT", 12968, 32065, 0,  0, "Bi-Quadratic Curve: Capacity as function of temp of entering condenser & exiting chilled water"
CHILLER,           5, MIN-RATIO,                                               "Minimum Ratio", 12953, 32065, 0,  2, "Minimum chiller operating ratio (a fraction of the Capacity); below this, it cycles on & off"
; SAC 4/18/02 - removed CHILLER:MAX-RATIO
; CHILLER,           5, MAX-RATIO,                                               "Maximum Ratio", 12954, 32065, 0,  2, "Maximum allowable chiller operating ratio (fraction of Capacity, also called max overload ratio)"
CHILLER,           5, HGB-RATIO,                                                   "HGB Ratio", 12952, 32065, 0,  2, "Maximum allowable part-load ratio of the chiller, above which hot gas bypass occures"
CHILLER,           5, ELEC-INPUT-RATIO,                                 "Electric Input Ratio", 12879, 32065, 0,  2, "Dimensionless ratio of electric input power to nominal capacity (i.e., invers of COP)"
CHILLER,           5, EIR-FT,                                                               "", 12967, 32065, 0,  0, "Quadratic Curve Fit: EIR as a function of temp of water entering condenser & leaving chilled"
CHILLER,           5, EIR-FPLR,                                                             "", 12969, 32065, 0,  0, "Quadratic Curve Fit: Electric Input Ratio as a function of the part load ratio"
CHILLER,           5, ELEC-TO-COND,                                    "Electric To Condenser", 12957, 32065, 0,  2, "Efficiency of compressor: i.e., fraction of chiller electricity input rejected to condenser, as heat"
CHILLER,           5, HEAT-INPUT-RATIO,                                     "Heat Input Ratio", 12956, 32065, 0,  2, "Ratio of fuel heat input (in Btus) to full load cooling capacity (in Btus), as rated conditions"
CHILLER,           5, HIR-FT,                                                               "", 12964, 32065, 0,  0, "Bi-Quadratic Curve: HIR as a function of temp of entering condenser and exiting chilled water"
CHILLER,           5, HIR-FPLR,                                                             "", 12965, 32065, 0,  0, "Quadratic Curve Fit: Heat Input Ratio as a function of the part load ratio"
CHILLER,           5, HEAT-TO-COND,                                        "Heat to Condenser", 12882, 32065, 0,  2, "Fraction of fuel or heat input to chiller that is rejected to condenser, as heat"
CHILLER,           5, START-UP-TIME,                                                        "", 13644, 32065, 0,  2, "Equivalent full-load time required to start up the chiller (in hours or fraction of hours)"
CHILLER,           5, SHUT-DOWN-TIME,                                                       "", 13649, 32065, 0,  2, "Equivalent full-load time required to shut down the chiller (in hours or fraction of hours)"
CHILLER,           5, HGB-RATIO-HTREC,                                                      "", 12970, 32065, 0,  2, "The hot gas bypass ratio when the chiller is in the heat recovery mode"
CHILLER,           5, SOLUTION-PUMP-KW,                                                     "", 13650, 32065, 0,  2, "Electricity consumption of the solution pump"
CHILLER,           5, GAS-HCAP-FPLRC,                                                       "", 13787, 32065, 0,  2, "Quadratic Curve: heating capacity as a function of the cooling part load ratio"
CHILLER,           5, GAS-HW-XEFF,                                                          "", 13780, 32065, 0,  2, "The burner efficiency (when the chiller is in the heating mode)"
CHILLER,           5, GAS-DESC-XEFF,                                                        "", 13781, 32065, 0,  2, "The burner efficiency when regenerating a desiccant system"
CHILLER,           5, GAS-COMB-FAN-KW,                                                      "", 13778, 32065, 0,  2, "Electricity consumption of the combustion blower"
CHILLER,           5, GAS-HIR-FDESCT,                                                       "", 13788, 32065, 0,  2, "Quadratic Curve: Heat Input Ratio as a function of the desiccant regeneration temperature"
CHILLER,           5, GAS-QREG-FDESCT,                                                      "", 13789, 32065, 0,  2, "Quadratic Curve: available regeneration energy as a function of the required regeneration temp"
CHILLER,           5, ENG-HEAT-TO-JAC,                                                      "", 13848, 32065, 0,  2, "Fraction of design fuel consumption that is recoverable from the jacket of an engine-chiller"
CHILLER,           5, ENG-HEAT-TO-EXH,                                                      "", 13849, 32065, 0,  2, "Fraction of design fuel consumption that is recoverable from the exhaust of an engine-chiller"
CHILLER,           5, ENG-HTREJ-FT,                                                         "", 13785, 32065, 0,  2, "Quadratic Curve: the amount of recoverable heat as a function of the entering condenser temp"
CHILLER,           5, ENG-HTREJ-FPLR,                                                       "", 13784, 32065, 0,  2, "Quadratic Curve: amount of recoverable heat as a function of the cooling part load ratio"
CHILLER,           5, HEAT/COOL-CAP,                                           "HEAT/COOL-CAP",     0, 32065, 0,  3, "HEAT/COOL-CAP"
CHILLER,           5, HEAT-CAP-FT,                                               "HEAT-CAP-FT",     0, 32065, 0,  0, "HEAT-CAP-FT"
CHILLER,           5, HEAT-CAP-FT-FRST,                                     "HEAT-CAP-FT-FRST",     0, 32065, 0,  0, "HEAT-CAP-FT-FRST"
CHILLER,           5, HEAT-EIR,                                                     "HEAT-EIR",     0, 32065, 0,  3, "HEAT-EIR"
CHILLER,           5, HEAT-EIR-FT,                                               "HEAT-EIR-FT",     0, 32065, 0,  0, "HEAT-EIR-FT"
CHILLER,           5, HEAT-EIR-FT-FRST,                                     "HEAT-EIR-FT-FRST",     0, 32065, 0,  0, "HEAT-EIR-FT-FRST"
CHILLER,           5, HEAT-EIR-FPLR,                                           "HEAT-EIR-FPLR",     0, 32065, 0,  0, "HEAT-EIR-FPLR"
CHILLER,           5, AUX-KW,                                                   "Auxiliary kW", 13795, 32065, 0,  2, "Auxiliary electric power consumption of the chiler (e.g., control panels)"
CHILLER,           5, AUX-MODE,                                                             "", 12987, 32065, 0,  2, "Always=all hours;When On=If chiller on;When Off=if chiller off;Scheduled=use Aux Schedule"
CHILLER,           5, AUX-SCHEDULE,                                       "Auxiliary Schedule", 12988, 32065, 0,  2, "Schedule for Auxiliary Power consumption (set Auxiliary Mode to Scheduled to activate this)"
CHILLER,           5, AUX-METER,                                                            "", 12989, 32065, 0,  0, "Name of the Electric Meter that tallies the electricity consumption of this chiller's auxiliaries"
CHILLER,           5, ELEC-METER,                                             "Electric Meter", 12948, 32065, 0,  0, "Name of the Electric Meter that tallies the electric consumption of this chiller"
CHILLER,           5, FUEL-METER,                                                 "Fuel Meter", 12949, 32065, 0,  0, "Name of the Fuel Meter that tallies the fuel consumption of this chiller"
CHILLER,           5, CHW-LOOP,                                                     "CHW Loop", 19111, 32065, 0,  0, "Name of the primary Chiller Water Loop that this chiller serves"
CHILLER,           5, CHW-PUMP,                                                     "CHW Pump", 13800, 32065, 0,  0, "Name of a Pump that serves the chiller's chilled water loop"
CHILLER,           5, CHW-DT,                                                    "CHW Delta T", 12974, 32065, 0,  2, "Design temperature change of the chilled water through the chiller"
CHILLER,           5, CHW-HEAD,                                                             "", 12975, 32065, 0,  2, "Head loss through the chilled water piping at the design flow rate"
CHILLER,           5, CHW-STATIC-HEAD,                                                      "", 12976, 32065, 0,  2, "The static head in the chiller circuit (typically zero)"
CHILLER,           5, CHW-FLOW-CTRL,                                                        "", 12973, 32065, 0,  2, "The type of flow through the chiller evaporator"
CHILLER,           5, CHW-MIN-FLOW,                                                         "", 12977, 32065, 0,  2, "Minimum allowable fraction of the design flow rate through the evaporator"
CHILLER,           5, CHW-MAX-FLOW,                                                         "", 13491, 32065, 0,  2, "Maximum allowable fraction of the design flow rate through the evaporator"
CHILLER,           5, HW-LOOP,                                                       "HW Loop", 19117, 32065, 0,  0, "Name of HW loop that provides heat to an absorption chiller; or that a chiller/heater heats"
CHILLER,           5, HW-PUMP,                                                              "", 12991, 32065, 0,  2, "Hot Water pump: if not specified, the head requirement is passed to the primary loop"
CHILLER,           5, HW-DT,                                                      "HW Delta T", 12993, 32065, 0,  2, "Design temp change of hot water through the boiler (used to size recirculation pump)"
CHILLER,           5, HW-HEAD,                                                              "", 12994, 32065, 0,  2, "Pressure drop of the hot water through the chiller at the design flowrate"
CHILLER,           5, HW-STATIC-HEAD,                                                       "", 12995, 32065, 0,  2, "Static HW pressure drop through the chiller; use if pumping fluid at atm pressure into loop"
CHILLER,           5, HW-FLOW-CTRL,                                                         "", 12992, 32065, 0,  2, "Constant Flow = independent of the load; Variable Flow = varies linearly with load"
CHILLER,           5, HW-MIN-FLOW,                                                          "", 12996, 32065, 0,  2, "Min hot water flow rate through chiller; used only if Hot Water Flow Control = Variable Flow"
CHILLER,           5, HW-MAX-FLOW,                                                          "", 13492, 32065, 0,  2, "Max hot water flow rate through chiller; used only if Hot Water Flow Control = Variable Flow"
CHILLER,           5, CONDENSER-TYPE,                                         "Condenser Type", 12875, 32065, 0,  0, "Air Cooled=heat exchanger & condenser; Water Cooled=cooling tower & condenser loop"
CHILLER,           5, CW-LOOP,                                                       "CW Loop", 19112, 32065, 0,  0, "If Condenser Type=Water Cooled, CW Loop is required & must be attached to Cooling Tower"
CHILLER,           5, CW-PUMP,                                                       "CW Pump", 12929, 32065, 0,  0, "Name of a Pump that serves the (dedicated) evaporator recirculation loop"
CHILLER,           5, CW-DT,                                                      "CW Delta T", 12981, 32065, 0,  2, "Design temperature change of the water flowing through the condenser"
CHILLER,           5, CW-HEAD,                                                              "", 12982, 32065, 0,  2, "Pressure drop through the condenser at the design flow rate"
CHILLER,           5, CW-STATIC-HEAD,                                                       "", 12983, 32065, 0,  2, "Static pressure drop through the condenser at the design flow rate"
CHILLER,           5, CW-FLOW-CTRL,                                                         "", 12980, 32065, 0,  2, "The type of flow through the condenser"
CHILLER,           5, CW-MIN-FLOW,                                                          "", 12984, 32065, 0,  2, "Minimum allowable flow rate through the condenser (as a fraction of the design flow rate)"
CHILLER,           5, COND-SETPT-CTRL,                                       "COND-SETPT-CTRL",     0, 32065, 0,  0, "COND-SETPT-CTRL"
CHILLER,           5, COND-FAN-CTRL,                                           "COND-FAN-CTRL",     0, 32065, 0,  0, "COND-FAN-CTRL"
CHILLER,           5, COND-SETPT-T,                                             "COND-SETPT-T",     0, 32065, 0,  1, "COND-SETPT-T"
CHILLER,           5, COND-SETPT-DT,                                           "COND-SETPT-DT",     0, 32065, 0,  2, "COND-SETPT-DT"
CHILLER,           5, MIN-COND-T,                                                 "MIN-COND-T",     0, 32065, 0,  1, "MIN-COND-T"
CHILLER,           5, COND-CAPACITY,                                           "COND-CAPACITY",     0, 32065, 0,  3, "COND-CAPACITY"
CHILLER,           5, SCT-AMB-DT,                                                 "SCT-AMB-DT",     0, 32065, 0,  2, "SCT-AMB-DT"
CHILLER,           5, COND-FAN-EIR,                                             "COND-FAN-EIR",     0, 32065, 0,  4, "COND-FAN-EIR"
CHILLER,           5, COND-PUMP-EIR,                                           "COND-PUMP-EIR",     0, 32065, 0,  4, "COND-PUMP-EIR"
CHILLER,           5, COND-CAP-FT,                                               "COND-CAP-FT",     0, 32065, 0,  0, "COND-CAP-FT"
CHILLER,           5, AMB-FRAC-FT,                                               "AMB-FRAC-FT",     0, 32065, 0,  0, "AMB-FRAC-FT"
CHILLER,           5, COND-PWR-FPLR,                                           "COND-PWR-FPLR",     0, 32065, 0,  0, "COND-PWR-FPLR"
CHILLER,           5, MAX-HTREC,                                       "Maximum Heat Recovery", 12960, 32065, 0,  2, "Maximum fraction of design condenser heat that is available for heat recovery"
CHILLER,           5, HTREC-LOOP,                                         "Heat Recovery Loop", 19114, 19114, 0,  0, "Name of the Heat Recovery Loop that this chiller rejects heat to"
CHILLER,           5, MAX-RECOVER-T,                                                        "", 13531, 32065, 0,  2, "Maximum temperature at which heat can be recovered from the chiller"
CHILLER,           5, HTREC-PUMP,                                                           "", 12998, 32065, 0,  2, "Name of pump dedicated to provide chiller's Heat Recovery Head and Heat Rec. Static Head"
CHILLER,           5, HTREC-DT,                                        "Heat Recovery Delta T", 13005, 32065, 0,  2, "Design temperature change of the water flowing through the heat-recovery condenser"
CHILLER,           5, HTREC-HEAD,                                                           "", 13001, 32065, 0,  2, "Pressure drop through the heat recovery heat exchanger at the design flow rate"
CHILLER,           5, HTREC-STATIC-HEA,                                                     "", 13002, 32065, 0,  2, "Static pressure drop through the heat recovery heat exchanger"
CHILLER,           5, HTREC-FLOW-CTRL,                                                      "", 12999, 32065, 0,  2, "The type of heat recovery water flow through the chiller"
CHILLER,           5, HTREC-MIN-FLOW,                                                       "", 13003, 32065, 0,  2, "Minimum allowable flow rate through the heat-recovery condenser"
CHILLER,           5, EVAP-HX-TD,                                                 "EVAP-HX-TD",     0, 32065, 0,  3, "EVAP-HX-TD"
CHILLER,           5, EVAP-HX-SETPT-T,                                       "EVAP-HX-SETPT-T",     0, 32065, 0,  2, "EVAP-HX-SETPT-T"
CHILLER,           5, COND-HX-TD,                                                 "COND-HX-TD",     0, 32065, 0,  3, "COND-HX-TD"
CHILLER,           5, COND-HX-SETPT-T,                                       "COND-HX-SETPT-T",     0, 32065, 0,  2, "COND-HX-SETPT-T"
CHILLER,           5, COST-DATA,                                                            "", 13799, 32065, 0,  2, "Name of a set of Materials Costs, which specifies first costs, maintenance costs, etc."
CHILLER,           5, EQUIPMENT-REPORT,                                                     "",     0, 32065, 0,  2, "Whether or not a PS-H report is created for this chiller"
CHILLER,           5, PICTURE,                                                              "",     0, 32065, 0,  2, ""
CHILLER,           5, DRAWING,                                                              "",     0, 32065, 0,  2, ""
CHILLER,           6, TYPE,                                                             "Type", 12873, 32065, 0,  0, "PowerDOE has models for nine types of chillers"
CHILLER,           6, CAPACITY,                                                     "Capacity", 13792, 32065, 0,  1, "Nominal (rated) chiller cooling capacity in MBTU/hr (e.g., 100 ton = 1.2 MBTU/hr)"
CHILLER,           6, CAPACITY-RATIO,                                         "Capactiy Ratio", 13793, 32065, 0,  1, "Capacity as fraction of max cooling load (used only if PowerDOE sizes the chiller)"
CHILLER,           6, CAPACITY-FT,                                               "Capacity FT", 12968, 32065, 0,  0, "Bi-Quadratic Curve: Capacity as function of temp of entering condenser & exiting chilled water"
CHILLER,           6, MIN-RATIO,                                               "Minimum Ratio", 12953, 32065, 0,  2, "Minimum chiller operating ratio (a fraction of the Capacity); below this, it cycles on & off"
; SAC 4/18/02 - removed CHILLER:MAX-RATIO
; CHILLER,           6, MAX-RATIO,                                               "Maximum Ratio", 12954, 32065, 0,  2, "Maximum allowable chiller operating ratio (fraction of Capacity, also called max overload ratio)"
CHILLER,           6, HGB-RATIO,                                                   "HGB Ratio", 12952, 32065, 0,  2, "Maximum allowable part-load ratio of the chiller, above which hot gas bypass occures"
CHILLER,           6, ELEC-INPUT-RATIO,                                 "Electric Input Ratio", 12879, 32065, 0,  2, "Dimensionless ratio of electric input power to nominal capacity (i.e., invers of COP)"
CHILLER,           6, EIR-FT,                                                               "", 12967, 32065, 0,  0, "Quadratic Curve Fit: EIR as a function of temp of water entering condenser & leaving chilled"
CHILLER,           6, EIR-FPLR,                                                             "", 12969, 32065, 0,  0, "Quadratic Curve Fit: Electric Input Ratio as a function of the part load ratio"
CHILLER,           6, ELEC-TO-COND,                                    "Electric To Condenser", 12957, 32065, 0,  2, "Efficiency of compressor: i.e., fraction of chiller electricity input rejected to condenser, as heat"
CHILLER,           6, HEAT-INPUT-RATIO,                                     "Heat Input Ratio", 12956, 32065, 0,  2, "Ratio of fuel heat input (in Btus) to full load cooling capacity (in Btus), as rated conditions"
CHILLER,           6, HIR-FT,                                                               "", 12964, 32065, 0,  0, "Bi-Quadratic Curve: HIR as a function of temp of entering condenser and exiting chilled water"
CHILLER,           6, HIR-FPLR,                                                             "", 12965, 32065, 0,  0, "Quadratic Curve Fit: Heat Input Ratio as a function of the part load ratio"
CHILLER,           6, HEAT-TO-COND,                                        "Heat to Condenser", 12882, 32065, 0,  2, "Fraction of fuel or heat input to chiller that is rejected to condenser, as heat"
CHILLER,           6, START-UP-TIME,                                                        "", 13644, 32065, 0,  2, "Equivalent full-load time required to start up the chiller (in hours or fraction of hours)"
CHILLER,           6, SHUT-DOWN-TIME,                                                       "", 13649, 32065, 0,  2, "Equivalent full-load time required to shut down the chiller (in hours or fraction of hours)"
CHILLER,           6, HGB-RATIO-HTREC,                                                      "", 12970, 32065, 0,  2, "The hot gas bypass ratio when the chiller is in the heat recovery mode"
CHILLER,           6, SOLUTION-PUMP-KW,                                                     "", 13650, 32065, 0,  2, "Electricity consumption of the solution pump"
CHILLER,           6, GAS-HCAP-FPLRC,                                                       "", 13787, 32065, 0,  2, "Quadratic Curve: heating capacity as a function of the cooling part load ratio"
CHILLER,           6, GAS-HW-XEFF,                                                          "", 13780, 32065, 0,  2, "The burner efficiency (when the chiller is in the heating mode)"
CHILLER,           6, GAS-DESC-XEFF,                                                        "", 13781, 32065, 0,  2, "The burner efficiency when regenerating a desiccant system"
CHILLER,           6, GAS-COMB-FAN-KW,                                                      "", 13778, 32065, 0,  2, "Electricity consumption of the combustion blower"
CHILLER,           6, GAS-HIR-FDESCT,                                                       "", 13788, 32065, 0,  2, "Quadratic Curve: Heat Input Ratio as a function of the desiccant regeneration temperature"
CHILLER,           6, GAS-QREG-FDESCT,                                                      "", 13789, 32065, 0,  2, "Quadratic Curve: available regeneration energy as a function of the required regeneration temp"
CHILLER,           6, ENG-HEAT-TO-JAC,                                                      "", 13848, 32065, 0,  2, "Fraction of design fuel consumption that is recoverable from the jacket of an engine-chiller"
CHILLER,           6, ENG-HEAT-TO-EXH,                                                      "", 13849, 32065, 0,  2, "Fraction of design fuel consumption that is recoverable from the exhaust of an engine-chiller"
CHILLER,           6, ENG-HTREJ-FT,                                                         "", 13785, 32065, 0,  2, "Quadratic Curve: the amount of recoverable heat as a function of the entering condenser temp"
CHILLER,           6, ENG-HTREJ-FPLR,                                                       "", 13784, 32065, 0,  2, "Quadratic Curve: amount of recoverable heat as a function of the cooling part load ratio"
CHILLER,           6, HEAT/COOL-CAP,                                           "HEAT/COOL-CAP",     0, 32065, 0,  3, "HEAT/COOL-CAP"
CHILLER,           6, HEAT-CAP-FT,                                               "HEAT-CAP-FT",     0, 32065, 0,  0, "HEAT-CAP-FT"
CHILLER,           6, HEAT-CAP-FT-FRST,                                     "HEAT-CAP-FT-FRST",     0, 32065, 0,  0, "HEAT-CAP-FT-FRST"
CHILLER,           6, HEAT-EIR,                                                     "HEAT-EIR",     0, 32065, 0,  3, "HEAT-EIR"
CHILLER,           6, HEAT-EIR-FT,                                               "HEAT-EIR-FT",     0, 32065, 0,  0, "HEAT-EIR-FT"
CHILLER,           6, HEAT-EIR-FT-FRST,                                     "HEAT-EIR-FT-FRST",     0, 32065, 0,  0, "HEAT-EIR-FT-FRST"
CHILLER,           6, HEAT-EIR-FPLR,                                           "HEAT-EIR-FPLR",     0, 32065, 0,  0, "HEAT-EIR-FPLR"
CHILLER,           6, AUX-KW,                                                   "Auxiliary kW", 13795, 32065, 0,  2, "Auxiliary electric power consumption of the chiler (e.g., control panels)"
CHILLER,           6, AUX-MODE,                                                             "", 12987, 32065, 0,  2, "Always=all hours;When On=If chiller on;When Off=if chiller off;Scheduled=use Aux Schedule"
CHILLER,           6, AUX-SCHEDULE,                                       "Auxiliary Schedule", 12988, 32065, 0,  2, "Schedule for Auxiliary Power consumption (set Auxiliary Mode to Scheduled to activate this)"
CHILLER,           6, AUX-METER,                                                            "", 12989, 32065, 0,  0, "Name of the Electric Meter that tallies the electricity consumption of this chiller's auxiliaries"
CHILLER,           6, ELEC-METER,                                             "Electric Meter", 12948, 32065, 0,  0, "Name of the Electric Meter that tallies the electric consumption of this chiller"
CHILLER,           6, FUEL-METER,                                                 "Fuel Meter", 12949, 32065, 0,  0, "Name of the Fuel Meter that tallies the fuel consumption of this chiller"
CHILLER,           6, CHW-LOOP,                                                     "CHW Loop", 19111, 32065, 0,  0, "Name of the primary Chiller Water Loop that this chiller serves"
CHILLER,           6, CHW-PUMP,                                                     "CHW Pump", 13800, 32065, 0,  0, "Name of a Pump that serves the chiller's chilled water loop"
CHILLER,           6, CHW-DT,                                                    "CHW Delta T", 12974, 32065, 0,  2, "Design temperature change of the chilled water through the chiller"
CHILLER,           6, CHW-HEAD,                                                             "", 12975, 32065, 0,  2, "Head loss through the chilled water piping at the design flow rate"
CHILLER,           6, CHW-STATIC-HEAD,                                                      "", 12976, 32065, 0,  2, "The static head in the chiller circuit (typically zero)"
CHILLER,           6, CHW-FLOW-CTRL,                                                        "", 12973, 32065, 0,  2, "The type of flow through the chiller evaporator"
CHILLER,           6, CHW-MIN-FLOW,                                                         "", 12977, 32065, 0,  2, "Minimum allowable fraction of the design flow rate through the evaporator"
CHILLER,           6, CHW-MAX-FLOW,                                                         "", 13491, 32065, 0,  2, "Maximum allowable fraction of the design flow rate through the evaporator"
CHILLER,           6, HW-LOOP,                                                       "HW Loop", 19117, 32065, 0,  0, "Name of HW loop that provides heat to an absorption chiller; or that a chiller/heater heats"
CHILLER,           6, HW-PUMP,                                                              "", 12991, 32065, 0,  2, "Hot Water pump: if not specified, the head requirement is passed to the primary loop"
CHILLER,           6, HW-DT,                                                      "HW Delta T", 12993, 32065, 0,  2, "Design temp change of hot water through the boiler (used to size recirculation pump)"
CHILLER,           6, HW-HEAD,                                                              "", 12994, 32065, 0,  2, "Pressure drop of the hot water through the chiller at the design flowrate"
CHILLER,           6, HW-STATIC-HEAD,                                                       "", 12995, 32065, 0,  2, "Static HW pressure drop through the chiller; use if pumping fluid at atm pressure into loop"
CHILLER,           6, HW-FLOW-CTRL,                                                         "", 12992, 32065, 0,  2, "Constant Flow = independent of the load; Variable Flow = varies linearly with load"
CHILLER,           6, HW-MIN-FLOW,                                                          "", 12996, 32065, 0,  2, "Min hot water flow rate through chiller; used only if Hot Water Flow Control = Variable Flow"
CHILLER,           6, HW-MAX-FLOW,                                                          "", 13492, 32065, 0,  2, "Max hot water flow rate through chiller; used only if Hot Water Flow Control = Variable Flow"
CHILLER,           6, CONDENSER-TYPE,                                         "Condenser Type", 12875, 32065, 0,  0, "Air Cooled=heat exchanger & condenser; Water Cooled=cooling tower & condenser loop"
CHILLER,           6, CW-LOOP,                                                       "CW Loop", 19112, 32065, 0,  0, "If Condenser Type=Water Cooled, CW Loop is required & must be attached to Cooling Tower"
CHILLER,           6, CW-PUMP,                                                       "CW Pump", 12929, 32065, 0,  0, "Name of a Pump that serves the (dedicated) evaporator recirculation loop"
CHILLER,           6, CW-DT,                                                      "CW Delta T", 12981, 32065, 0,  2, "Design temperature change of the water flowing through the condenser"
CHILLER,           6, CW-HEAD,                                                              "", 12982, 32065, 0,  2, "Pressure drop through the condenser at the design flow rate"
CHILLER,           6, CW-STATIC-HEAD,                                                       "", 12983, 32065, 0,  2, "Static pressure drop through the condenser at the design flow rate"
CHILLER,           6, CW-FLOW-CTRL,                                                         "", 12980, 32065, 0,  2, "The type of flow through the condenser"
CHILLER,           6, CW-MIN-FLOW,                                                          "", 12984, 32065, 0,  2, "Minimum allowable flow rate through the condenser (as a fraction of the design flow rate)"
CHILLER,           6, COND-SETPT-CTRL,                                       "COND-SETPT-CTRL",     0, 32065, 0,  0, "COND-SETPT-CTRL"
CHILLER,           6, COND-FAN-CTRL,                                           "COND-FAN-CTRL",     0, 32065, 0,  0, "COND-FAN-CTRL"
CHILLER,           6, COND-SETPT-T,                                             "COND-SETPT-T",     0, 32065, 0,  1, "COND-SETPT-T"
CHILLER,           6, COND-SETPT-DT,                                           "COND-SETPT-DT",     0, 32065, 0,  2, "COND-SETPT-DT"
CHILLER,           6, MIN-COND-T,                                                 "MIN-COND-T",     0, 32065, 0,  1, "MIN-COND-T"
CHILLER,           6, COND-CAPACITY,                                           "COND-CAPACITY",     0, 32065, 0,  3, "COND-CAPACITY"
CHILLER,           6, SCT-AMB-DT,                                                 "SCT-AMB-DT",     0, 32065, 0,  2, "SCT-AMB-DT"
CHILLER,           6, COND-FAN-EIR,                                             "COND-FAN-EIR",     0, 32065, 0,  4, "COND-FAN-EIR"
CHILLER,           6, COND-PUMP-EIR,                                           "COND-PUMP-EIR",     0, 32065, 0,  4, "COND-PUMP-EIR"
CHILLER,           6, COND-CAP-FT,                                               "COND-CAP-FT",     0, 32065, 0,  0, "COND-CAP-FT"
CHILLER,           6, AMB-FRAC-FT,                                               "AMB-FRAC-FT",     0, 32065, 0,  0, "AMB-FRAC-FT"
CHILLER,           6, COND-PWR-FPLR,                                           "COND-PWR-FPLR",     0, 32065, 0,  0, "COND-PWR-FPLR"
CHILLER,           6, MAX-HTREC,                                       "Maximum Heat Recovery", 12960, 32065, 0,  2, "Maximum fraction of design condenser heat that is available for heat recovery"
CHILLER,           6, HTREC-LOOP,                                         "Heat Recovery Loop", 19114, 19114, 0,  0, "Name of the Heat Recovery Loop that this chiller rejects heat to"
CHILLER,           6, MAX-RECOVER-T,                                                        "", 13531, 32065, 0,  2, "Maximum temperature at which heat can be recovered from the chiller"
CHILLER,           6, HTREC-PUMP,                                                           "", 12998, 32065, 0,  2, "Name of pump dedicated to provide chiller's Heat Recovery Head and Heat Rec. Static Head"
CHILLER,           6, HTREC-DT,                                        "Heat Recovery Delta T", 13005, 32065, 0,  2, "Design temperature change of the water flowing through the heat-recovery condenser"
CHILLER,           6, HTREC-HEAD,                                                           "", 13001, 32065, 0,  2, "Pressure drop through the heat recovery heat exchanger at the design flow rate"
CHILLER,           6, HTREC-STATIC-HEA,                                                     "", 13002, 32065, 0,  2, "Static pressure drop through the heat recovery heat exchanger"
CHILLER,           6, HTREC-FLOW-CTRL,                                                      "", 12999, 32065, 0,  2, "The type of heat recovery water flow through the chiller"
CHILLER,           6, HTREC-MIN-FLOW,                                                       "", 13003, 32065, 0,  2, "Minimum allowable flow rate through the heat-recovery condenser"
CHILLER,           6, EVAP-HX-TD,                                                 "EVAP-HX-TD",     0, 32065, 0,  3, "EVAP-HX-TD"
CHILLER,           6, EVAP-HX-SETPT-T,                                       "EVAP-HX-SETPT-T",     0, 32065, 0,  2, "EVAP-HX-SETPT-T"
CHILLER,           6, COND-HX-TD,                                                 "COND-HX-TD",     0, 32065, 0,  3, "COND-HX-TD"
CHILLER,           6, COND-HX-SETPT-T,                                       "COND-HX-SETPT-T",     0, 32065, 0,  2, "COND-HX-SETPT-T"
CHILLER,           6, COST-DATA,                                                            "", 13799, 32065, 0,  2, "Name of a set of Materials Costs, which specifies first costs, maintenance costs, etc."
CHILLER,           6, EQUIPMENT-REPORT,                                                     "",     0, 32065, 0,  2, "Whether or not a PS-H report is created for this chiller"
CHILLER,           6, PICTURE,                                                              "",     0, 32065, 0,  2, ""
CHILLER,           6, DRAWING,                                                              "",     0, 32065, 0,  2, ""
CHILLER,           7, TYPE,                                                             "Type", 12873, 32065, 0,  0, "PowerDOE has models for nine types of chillers"
CHILLER,           7, CAPACITY,                                                     "Capacity", 13792, 32065, 0,  1, "Nominal (rated) chiller cooling capacity in MBTU/hr (e.g., 100 ton = 1.2 MBTU/hr)"
CHILLER,           7, CAPACITY-RATIO,                                         "Capactiy Ratio", 13793, 32065, 0,  1, "Capacity as fraction of max cooling load (used only if PowerDOE sizes the chiller)"
CHILLER,           7, CAPACITY-FT,                                               "Capacity FT", 12968, 32065, 0,  0, "Bi-Quadratic Curve: Capacity as function of temp of entering condenser & exiting chilled water"
CHILLER,           7, MIN-RATIO,                                               "Minimum Ratio", 12953, 32065, 0,  2, "Minimum chiller operating ratio (a fraction of the Capacity); below this, it cycles on & off"
; SAC 4/18/02 - removed CHILLER:MAX-RATIO
; CHILLER,           7, MAX-RATIO,                                               "Maximum Ratio", 12954, 32065, 0,  2, "Maximum allowable chiller operating ratio (fraction of Capacity, also called max overload ratio)"
CHILLER,           7, HGB-RATIO,                                                   "HGB Ratio", 12952, 32065, 0,  2, "Maximum allowable part-load ratio of the chiller, above which hot gas bypass occures"
CHILLER,           7, ELEC-INPUT-RATIO,                                 "Electric Input Ratio", 12879, 32065, 0,  2, "Dimensionless ratio of electric input power to nominal capacity (i.e., invers of COP)"
CHILLER,           7, EIR-FT,                                                               "", 12967, 32065, 0,  0, "Quadratic Curve Fit: EIR as a function of temp of water entering condenser & leaving chilled"
CHILLER,           7, EIR-FPLR,                                                             "", 12969, 32065, 0,  0, "Quadratic Curve Fit: Electric Input Ratio as a function of the part load ratio"
CHILLER,           7, ELEC-TO-COND,                                    "Electric To Condenser", 12957, 32065, 0,  2, "Efficiency of compressor: i.e., fraction of chiller electricity input rejected to condenser, as heat"
CHILLER,           7, HEAT-INPUT-RATIO,                                     "Heat Input Ratio", 12956, 32065, 0,  2, "Ratio of fuel heat input (in Btus) to full load cooling capacity (in Btus), as rated conditions"
CHILLER,           7, HIR-FT,                                                               "", 12964, 32065, 0,  0, "Bi-Quadratic Curve: HIR as a function of temp of entering condenser and exiting chilled water"
CHILLER,           7, HIR-FPLR,                                                             "", 12965, 32065, 0,  0, "Quadratic Curve Fit: Heat Input Ratio as a function of the part load ratio"
CHILLER,           7, HEAT-TO-COND,                                        "Heat to Condenser", 12882, 32065, 0,  2, "Fraction of fuel or heat input to chiller that is rejected to condenser, as heat"
CHILLER,           7, START-UP-TIME,                                                        "", 13644, 32065, 0,  2, "Equivalent full-load time required to start up the chiller (in hours or fraction of hours)"
CHILLER,           7, SHUT-DOWN-TIME,                                                       "", 13649, 32065, 0,  2, "Equivalent full-load time required to shut down the chiller (in hours or fraction of hours)"
CHILLER,           7, HGB-RATIO-HTREC,                                                      "", 12970, 32065, 0,  2, "The hot gas bypass ratio when the chiller is in the heat recovery mode"
CHILLER,           7, SOLUTION-PUMP-KW,                                                     "", 13650, 32065, 0,  2, "Electricity consumption of the solution pump"
CHILLER,           7, GAS-HCAP-FPLRC,                                                       "", 13787, 32065, 0,  2, "Quadratic Curve: heating capacity as a function of the cooling part load ratio"
CHILLER,           7, GAS-HW-XEFF,                                                          "", 13780, 32065, 0,  2, "The burner efficiency (when the chiller is in the heating mode)"
CHILLER,           7, GAS-DESC-XEFF,                                                        "", 13781, 32065, 0,  2, "The burner efficiency when regenerating a desiccant system"
CHILLER,           7, GAS-COMB-FAN-KW,                                                      "", 13778, 32065, 0,  2, "Electricity consumption of the combustion blower"
CHILLER,           7, GAS-HIR-FDESCT,                                                       "", 13788, 32065, 0,  2, "Quadratic Curve: Heat Input Ratio as a function of the desiccant regeneration temperature"
CHILLER,           7, GAS-QREG-FDESCT,                                                      "", 13789, 32065, 0,  2, "Quadratic Curve: available regeneration energy as a function of the required regeneration temp"
CHILLER,           7, ENG-HEAT-TO-JAC,                                                      "", 13848, 32065, 0,  2, "Fraction of design fuel consumption that is recoverable from the jacket of an engine-chiller"
CHILLER,           7, ENG-HEAT-TO-EXH,                                                      "", 13849, 32065, 0,  2, "Fraction of design fuel consumption that is recoverable from the exhaust of an engine-chiller"
CHILLER,           7, ENG-HTREJ-FT,                                                         "", 13785, 32065, 0,  2, "Quadratic Curve: the amount of recoverable heat as a function of the entering condenser temp"
CHILLER,           7, ENG-HTREJ-FPLR,                                                       "", 13784, 32065, 0,  2, "Quadratic Curve: amount of recoverable heat as a function of the cooling part load ratio"
CHILLER,           7, HEAT/COOL-CAP,                                           "HEAT/COOL-CAP",     0, 32065, 0,  3, "HEAT/COOL-CAP"
CHILLER,           7, HEAT-CAP-FT,                                               "HEAT-CAP-FT",     0, 32065, 0,  0, "HEAT-CAP-FT"
CHILLER,           7, HEAT-CAP-FT-FRST,                                     "HEAT-CAP-FT-FRST",     0, 32065, 0,  0, "HEAT-CAP-FT-FRST"
CHILLER,           7, HEAT-EIR,                                                     "HEAT-EIR",     0, 32065, 0,  3, "HEAT-EIR"
CHILLER,           7, HEAT-EIR-FT,                                               "HEAT-EIR-FT",     0, 32065, 0,  0, "HEAT-EIR-FT"
CHILLER,           7, HEAT-EIR-FT-FRST,                                     "HEAT-EIR-FT-FRST",     0, 32065, 0,  0, "HEAT-EIR-FT-FRST"
CHILLER,           7, HEAT-EIR-FPLR,                                           "HEAT-EIR-FPLR",     0, 32065, 0,  0, "HEAT-EIR-FPLR"
CHILLER,           7, AUX-KW,                                                   "Auxiliary kW", 13795, 32065, 0,  2, "Auxiliary electric power consumption of the chiler (e.g., control panels)"
CHILLER,           7, AUX-MODE,                                                             "", 12987, 32065, 0,  2, "Always=all hours;When On=If chiller on;When Off=if chiller off;Scheduled=use Aux Schedule"
CHILLER,           7, AUX-SCHEDULE,                                       "Auxiliary Schedule", 12988, 32065, 0,  2, "Schedule for Auxiliary Power consumption (set Auxiliary Mode to Scheduled to activate this)"
CHILLER,           7, AUX-METER,                                                            "", 12989, 32065, 0,  0, "Name of the Electric Meter that tallies the electricity consumption of this chiller's auxiliaries"
CHILLER,           7, ELEC-METER,                                             "Electric Meter", 12948, 32065, 0,  0, "Name of the Electric Meter that tallies the electric consumption of this chiller"
CHILLER,           7, FUEL-METER,                                                 "Fuel Meter", 12949, 32065, 0,  0, "Name of the Fuel Meter that tallies the fuel consumption of this chiller"
CHILLER,           7, CHW-LOOP,                                                     "CHW Loop", 19111, 32065, 0,  0, "Name of the primary Chiller Water Loop that this chiller serves"
CHILLER,           7, CHW-PUMP,                                                     "CHW Pump", 13800, 32065, 0,  0, "Name of a Pump that serves the chiller's chilled water loop"
CHILLER,           7, CHW-DT,                                                    "CHW Delta T", 12974, 32065, 0,  2, "Design temperature change of the chilled water through the chiller"
CHILLER,           7, CHW-HEAD,                                                             "", 12975, 32065, 0,  2, "Head loss through the chilled water piping at the design flow rate"
CHILLER,           7, CHW-STATIC-HEAD,                                                      "", 12976, 32065, 0,  2, "The static head in the chiller circuit (typically zero)"
CHILLER,           7, CHW-FLOW-CTRL,                                                        "", 12973, 32065, 0,  2, "The type of flow through the chiller evaporator"
CHILLER,           7, CHW-MIN-FLOW,                                                         "", 12977, 32065, 0,  2, "Minimum allowable fraction of the design flow rate through the evaporator"
CHILLER,           7, CHW-MAX-FLOW,                                                         "", 13491, 32065, 0,  2, "Maximum allowable fraction of the design flow rate through the evaporator"
CHILLER,           7, HW-LOOP,                                                       "HW Loop", 19117, 32065, 0,  0, "Name of HW loop that provides heat to an absorption chiller; or that a chiller/heater heats"
CHILLER,           7, HW-PUMP,                                                              "", 12991, 32065, 0,  2, "Hot Water pump: if not specified, the head requirement is passed to the primary loop"
CHILLER,           7, HW-DT,                                                      "HW Delta T", 12993, 32065, 0,  2, "Design temp change of hot water through the boiler (used to size recirculation pump)"
CHILLER,           7, HW-HEAD,                                                              "", 12994, 32065, 0,  2, "Pressure drop of the hot water through the chiller at the design flowrate"
CHILLER,           7, HW-STATIC-HEAD,                                                       "", 12995, 32065, 0,  2, "Static HW pressure drop through the chiller; use if pumping fluid at atm pressure into loop"
CHILLER,           7, HW-FLOW-CTRL,                                                         "", 12992, 32065, 0,  2, "Constant Flow = independent of the load; Variable Flow = varies linearly with load"
CHILLER,           7, HW-MIN-FLOW,                                                          "", 12996, 32065, 0,  2, "Min hot water flow rate through chiller; used only if Hot Water Flow Control = Variable Flow"
CHILLER,           7, HW-MAX-FLOW,                                                          "", 13492, 32065, 0,  2, "Max hot water flow rate through chiller; used only if Hot Water Flow Control = Variable Flow"
CHILLER,           7, CONDENSER-TYPE,                                         "Condenser Type", 12875, 32065, 0,  0, "Air Cooled=heat exchanger & condenser; Water Cooled=cooling tower & condenser loop"
CHILLER,           7, CW-LOOP,                                                       "CW Loop", 19112, 32065, 0,  0, "If Condenser Type=Water Cooled, CW Loop is required & must be attached to Cooling Tower"
CHILLER,           7, CW-PUMP,                                                       "CW Pump", 12929, 32065, 0,  0, "Name of a Pump that serves the (dedicated) evaporator recirculation loop"
CHILLER,           7, CW-DT,                                                      "CW Delta T", 12981, 32065, 0,  2, "Design temperature change of the water flowing through the condenser"
CHILLER,           7, CW-HEAD,                                                              "", 12982, 32065, 0,  2, "Pressure drop through the condenser at the design flow rate"
CHILLER,           7, CW-STATIC-HEAD,                                                       "", 12983, 32065, 0,  2, "Static pressure drop through the condenser at the design flow rate"
CHILLER,           7, CW-FLOW-CTRL,                                                         "", 12980, 32065, 0,  2, "The type of flow through the condenser"
CHILLER,           7, CW-MIN-FLOW,                                                          "", 12984, 32065, 0,  2, "Minimum allowable flow rate through the condenser (as a fraction of the design flow rate)"
CHILLER,           7, COND-SETPT-CTRL,                                       "COND-SETPT-CTRL",     0, 32065, 0,  0, "COND-SETPT-CTRL"
CHILLER,           7, COND-FAN-CTRL,                                           "COND-FAN-CTRL",     0, 32065, 0,  0, "COND-FAN-CTRL"
CHILLER,           7, COND-SETPT-T,                                             "COND-SETPT-T",     0, 32065, 0,  1, "COND-SETPT-T"
CHILLER,           7, COND-SETPT-DT,                                           "COND-SETPT-DT",     0, 32065, 0,  2, "COND-SETPT-DT"
CHILLER,           7, MIN-COND-T,                                                 "MIN-COND-T",     0, 32065, 0,  1, "MIN-COND-T"
CHILLER,           7, COND-CAPACITY,                                           "COND-CAPACITY",     0, 32065, 0,  3, "COND-CAPACITY"
CHILLER,           7, SCT-AMB-DT,                                                 "SCT-AMB-DT",     0, 32065, 0,  2, "SCT-AMB-DT"
CHILLER,           7, COND-FAN-EIR,                                             "COND-FAN-EIR",     0, 32065, 0,  4, "COND-FAN-EIR"
CHILLER,           7, COND-PUMP-EIR,                                           "COND-PUMP-EIR",     0, 32065, 0,  4, "COND-PUMP-EIR"
CHILLER,           7, COND-CAP-FT,                                               "COND-CAP-FT",     0, 32065, 0,  0, "COND-CAP-FT"
CHILLER,           7, AMB-FRAC-FT,                                               "AMB-FRAC-FT",     0, 32065, 0,  0, "AMB-FRAC-FT"
CHILLER,           7, COND-PWR-FPLR,                                           "COND-PWR-FPLR",     0, 32065, 0,  0, "COND-PWR-FPLR"
CHILLER,           7, MAX-HTREC,                                       "Maximum Heat Recovery", 12960, 32065, 0,  2, "Maximum fraction of design condenser heat that is available for heat recovery"
CHILLER,           7, HTREC-LOOP,                                         "Heat Recovery Loop", 19114, 19114, 0,  0, "Name of the Heat Recovery Loop that this chiller rejects heat to"
CHILLER,           7, MAX-RECOVER-T,                                                        "", 13531, 32065, 0,  2, "Maximum temperature at which heat can be recovered from the chiller"
CHILLER,           7, HTREC-PUMP,                                                           "", 12998, 32065, 0,  2, "Name of pump dedicated to provide chiller's Heat Recovery Head and Heat Rec. Static Head"
CHILLER,           7, HTREC-DT,                                        "Heat Recovery Delta T", 13005, 32065, 0,  2, "Design temperature change of the water flowing through the heat-recovery condenser"
CHILLER,           7, HTREC-HEAD,                                                           "", 13001, 32065, 0,  2, "Pressure drop through the heat recovery heat exchanger at the design flow rate"
CHILLER,           7, HTREC-STATIC-HEA,                                                     "", 13002, 32065, 0,  2, "Static pressure drop through the heat recovery heat exchanger"
CHILLER,           7, HTREC-FLOW-CTRL,                                                      "", 12999, 32065, 0,  2, "The type of heat recovery water flow through the chiller"
CHILLER,           7, HTREC-MIN-FLOW,                                                       "", 13003, 32065, 0,  2, "Minimum allowable flow rate through the heat-recovery condenser"
CHILLER,           7, EVAP-HX-TD,                                                 "EVAP-HX-TD",     0, 32065, 0,  3, "EVAP-HX-TD"
CHILLER,           7, EVAP-HX-SETPT-T,                                       "EVAP-HX-SETPT-T",     0, 32065, 0,  2, "EVAP-HX-SETPT-T"
CHILLER,           7, COND-HX-TD,                                                 "COND-HX-TD",     0, 32065, 0,  3, "COND-HX-TD"
CHILLER,           7, COND-HX-SETPT-T,                                       "COND-HX-SETPT-T",     0, 32065, 0,  2, "COND-HX-SETPT-T"
CHILLER,           7, COST-DATA,                                                            "", 13799, 32065, 0,  2, "Name of a set of Materials Costs, which specifies first costs, maintenance costs, etc."
CHILLER,           7, EQUIPMENT-REPORT,                                                     "",     0, 32065, 0,  2, "Whether or not a PS-H report is created for this chiller"
CHILLER,           7, PICTURE,                                                              "",     0, 32065, 0,  2, ""
CHILLER,           7, DRAWING,                                                              "",     0, 32065, 0,  2, ""
CHILLER,           8, TYPE,                                                             "Type", 12873, 32065, 0,  0, "PowerDOE has models for nine types of chillers"
CHILLER,           8, CAPACITY,                                                     "Capacity", 13792, 32065, 0,  1, "Nominal (rated) chiller cooling capacity in MBTU/hr (e.g., 100 ton = 1.2 MBTU/hr)"
CHILLER,           8, CAPACITY-RATIO,                                         "Capactiy Ratio", 13793, 32065, 0,  1, "Capacity as fraction of max cooling load (used only if PowerDOE sizes the chiller)"
CHILLER,           8, CAPACITY-FT,                                               "Capacity FT", 12968, 32065, 0,  0, "Bi-Quadratic Curve: Capacity as function of temp of entering condenser & exiting chilled water"
CHILLER,           8, MIN-RATIO,                                               "Minimum Ratio", 12953, 32065, 0,  2, "Minimum chiller operating ratio (a fraction of the Capacity); below this, it cycles on & off"
; SAC 4/18/02 - removed CHILLER:MAX-RATIO
; CHILLER,           8, MAX-RATIO,                                               "Maximum Ratio", 12954, 32065, 0,  2, "Maximum allowable chiller operating ratio (fraction of Capacity, also called max overload ratio)"
CHILLER,           8, HGB-RATIO,                                                   "HGB Ratio", 12952, 32065, 0,  2, "Maximum allowable part-load ratio of the chiller, above which hot gas bypass occures"
CHILLER,           8, ELEC-INPUT-RATIO,                                 "Electric Input Ratio", 12879, 32065, 0,  2, "Dimensionless ratio of electric input power to nominal capacity (i.e., invers of COP)"
CHILLER,           8, EIR-FT,                                                               "", 12967, 32065, 0,  0, "Quadratic Curve Fit: EIR as a function of temp of water entering condenser & leaving chilled"
CHILLER,           8, EIR-FPLR,                                                             "", 12969, 32065, 0,  0, "Quadratic Curve Fit: Electric Input Ratio as a function of the part load ratio"
CHILLER,           8, ELEC-TO-COND,                                    "Electric To Condenser", 12957, 32065, 0,  2, "Efficiency of compressor: i.e., fraction of chiller electricity input rejected to condenser, as heat"
CHILLER,           8, HEAT-INPUT-RATIO,                                     "Heat Input Ratio", 12956, 32065, 0,  2, "Ratio of fuel heat input (in Btus) to full load cooling capacity (in Btus), as rated conditions"
CHILLER,           8, HIR-FT,                                                               "", 12964, 32065, 0,  0, "Bi-Quadratic Curve: HIR as a function of temp of entering condenser and exiting chilled water"
CHILLER,           8, HIR-FPLR,                                                             "", 12965, 32065, 0,  0, "Quadratic Curve Fit: Heat Input Ratio as a function of the part load ratio"
CHILLER,           8, HEAT-TO-COND,                                        "Heat to Condenser", 12882, 32065, 0,  2, "Fraction of fuel or heat input to chiller that is rejected to condenser, as heat"
CHILLER,           8, START-UP-TIME,                                                        "", 13644, 32065, 0,  2, "Equivalent full-load time required to start up the chiller (in hours or fraction of hours)"
CHILLER,           8, SHUT-DOWN-TIME,                                                       "", 13649, 32065, 0,  2, "Equivalent full-load time required to shut down the chiller (in hours or fraction of hours)"
CHILLER,           8, HGB-RATIO-HTREC,                                                      "", 12970, 32065, 0,  2, "The hot gas bypass ratio when the chiller is in the heat recovery mode"
CHILLER,           8, SOLUTION-PUMP-KW,                                                     "", 13650, 32065, 0,  2, "Electricity consumption of the solution pump"
CHILLER,           8, GAS-HCAP-FPLRC,                                                       "", 13787, 32065, 0,  2, "Quadratic Curve: heating capacity as a function of the cooling part load ratio"
CHILLER,           8, GAS-HW-XEFF,                                                          "", 13780, 32065, 0,  2, "The burner efficiency (when the chiller is in the heating mode)"
CHILLER,           8, GAS-DESC-XEFF,                                                        "", 13781, 32065, 0,  2, "The burner efficiency when regenerating a desiccant system"
CHILLER,           8, GAS-COMB-FAN-KW,                                                      "", 13778, 32065, 0,  2, "Electricity consumption of the combustion blower"
CHILLER,           8, GAS-HIR-FDESCT,                                                       "", 13788, 32065, 0,  2, "Quadratic Curve: Heat Input Ratio as a function of the desiccant regeneration temperature"
CHILLER,           8, GAS-QREG-FDESCT,                                                      "", 13789, 32065, 0,  2, "Quadratic Curve: available regeneration energy as a function of the required regeneration temp"
CHILLER,           8, ENG-HEAT-TO-JAC,                                                      "", 13848, 32065, 0,  2, "Fraction of design fuel consumption that is recoverable from the jacket of an engine-chiller"
CHILLER,           8, ENG-HEAT-TO-EXH,                                                      "", 13849, 32065, 0,  2, "Fraction of design fuel consumption that is recoverable from the exhaust of an engine-chiller"
CHILLER,           8, ENG-HTREJ-FT,                                                         "", 13785, 32065, 0,  2, "Quadratic Curve: the amount of recoverable heat as a function of the entering condenser temp"
CHILLER,           8, ENG-HTREJ-FPLR,                                                       "", 13784, 32065, 0,  2, "Quadratic Curve: amount of recoverable heat as a function of the cooling part load ratio"
CHILLER,           8, HEAT/COOL-CAP,                                           "HEAT/COOL-CAP",     0, 32065, 0,  3, "HEAT/COOL-CAP"
CHILLER,           8, HEAT-CAP-FT,                                               "HEAT-CAP-FT",     0, 32065, 0,  0, "HEAT-CAP-FT"
CHILLER,           8, HEAT-CAP-FT-FRST,                                     "HEAT-CAP-FT-FRST",     0, 32065, 0,  0, "HEAT-CAP-FT-FRST"
CHILLER,           8, HEAT-EIR,                                                     "HEAT-EIR",     0, 32065, 0,  3, "HEAT-EIR"
CHILLER,           8, HEAT-EIR-FT,                                               "HEAT-EIR-FT",     0, 32065, 0,  0, "HEAT-EIR-FT"
CHILLER,           8, HEAT-EIR-FT-FRST,                                     "HEAT-EIR-FT-FRST",     0, 32065, 0,  0, "HEAT-EIR-FT-FRST"
CHILLER,           8, HEAT-EIR-FPLR,                                           "HEAT-EIR-FPLR",     0, 32065, 0,  0, "HEAT-EIR-FPLR"
CHILLER,           8, AUX-KW,                                                   "Auxiliary kW", 13795, 32065, 0,  2, "Auxiliary electric power consumption of the chiler (e.g., control panels)"
CHILLER,           8, AUX-MODE,                                                             "", 12987, 32065, 0,  2, "Always=all hours;When On=If chiller on;When Off=if chiller off;Scheduled=use Aux Schedule"
CHILLER,           8, AUX-SCHEDULE,                                       "Auxiliary Schedule", 12988, 32065, 0,  2, "Schedule for Auxiliary Power consumption (set Auxiliary Mode to Scheduled to activate this)"
CHILLER,           8, AUX-METER,                                                            "", 12989, 32065, 0,  0, "Name of the Electric Meter that tallies the electricity consumption of this chiller's auxiliaries"
CHILLER,           8, ELEC-METER,                                             "Electric Meter", 12948, 32065, 0,  0, "Name of the Electric Meter that tallies the electric consumption of this chiller"
CHILLER,           8, FUEL-METER,                                                 "Fuel Meter", 12949, 32065, 0,  0, "Name of the Fuel Meter that tallies the fuel consumption of this chiller"
CHILLER,           8, CHW-LOOP,                                                     "CHW Loop", 19111, 32065, 0,  0, "Name of the primary Chiller Water Loop that this chiller serves"
CHILLER,           8, CHW-PUMP,                                                     "CHW Pump", 13800, 32065, 0,  0, "Name of a Pump that serves the chiller's chilled water loop"
CHILLER,           8, CHW-DT,                                                    "CHW Delta T", 12974, 32065, 0,  2, "Design temperature change of the chilled water through the chiller"
CHILLER,           8, CHW-HEAD,                                                             "", 12975, 32065, 0,  2, "Head loss through the chilled water piping at the design flow rate"
CHILLER,           8, CHW-STATIC-HEAD,                                                      "", 12976, 32065, 0,  2, "The static head in the chiller circuit (typically zero)"
CHILLER,           8, CHW-FLOW-CTRL,                                                        "", 12973, 32065, 0,  2, "The type of flow through the chiller evaporator"
CHILLER,           8, CHW-MIN-FLOW,                                                         "", 12977, 32065, 0,  2, "Minimum allowable fraction of the design flow rate through the evaporator"
CHILLER,           8, CHW-MAX-FLOW,                                                         "", 13491, 32065, 0,  2, "Maximum allowable fraction of the design flow rate through the evaporator"
CHILLER,           8, HW-LOOP,                                                       "HW Loop", 19117, 32065, 0,  0, "Name of HW loop that provides heat to an absorption chiller; or that a chiller/heater heats"
CHILLER,           8, HW-PUMP,                                                              "", 12991, 32065, 0,  2, "Hot Water pump: if not specified, the head requirement is passed to the primary loop"
CHILLER,           8, HW-DT,                                                      "HW Delta T", 12993, 32065, 0,  2, "Design temp change of hot water through the boiler (used to size recirculation pump)"
CHILLER,           8, HW-HEAD,                                                              "", 12994, 32065, 0,  2, "Pressure drop of the hot water through the chiller at the design flowrate"
CHILLER,           8, HW-STATIC-HEAD,                                                       "", 12995, 32065, 0,  2, "Static HW pressure drop through the chiller; use if pumping fluid at atm pressure into loop"
CHILLER,           8, HW-FLOW-CTRL,                                                         "", 12992, 32065, 0,  2, "Constant Flow = independent of the load; Variable Flow = varies linearly with load"
CHILLER,           8, HW-MIN-FLOW,                                                          "", 12996, 32065, 0,  2, "Min hot water flow rate through chiller; used only if Hot Water Flow Control = Variable Flow"
CHILLER,           8, HW-MAX-FLOW,                                                          "", 13492, 32065, 0,  2, "Max hot water flow rate through chiller; used only if Hot Water Flow Control = Variable Flow"
CHILLER,           8, CONDENSER-TYPE,                                         "Condenser Type", 12875, 32065, 0,  0, "Air Cooled=heat exchanger & condenser; Water Cooled=cooling tower & condenser loop"
CHILLER,           8, CW-LOOP,                                                       "CW Loop", 19112, 32065, 0,  0, "If Condenser Type=Water Cooled, CW Loop is required & must be attached to Cooling Tower"
CHILLER,           8, CW-PUMP,                                                       "CW Pump", 12929, 32065, 0,  0, "Name of a Pump that serves the (dedicated) evaporator recirculation loop"
CHILLER,           8, CW-DT,                                                      "CW Delta T", 12981, 32065, 0,  2, "Design temperature change of the water flowing through the condenser"
CHILLER,           8, CW-HEAD,                                                              "", 12982, 32065, 0,  2, "Pressure drop through the condenser at the design flow rate"
CHILLER,           8, CW-STATIC-HEAD,                                                       "", 12983, 32065, 0,  2, "Static pressure drop through the condenser at the design flow rate"
CHILLER,           8, CW-FLOW-CTRL,                                                         "", 12980, 32065, 0,  2, "The type of flow through the condenser"
CHILLER,           8, CW-MIN-FLOW,                                                          "", 12984, 32065, 0,  2, "Minimum allowable flow rate through the condenser (as a fraction of the design flow rate)"
CHILLER,           8, COND-SETPT-CTRL,                                       "COND-SETPT-CTRL",     0, 32065, 0,  0, "COND-SETPT-CTRL"
CHILLER,           8, COND-FAN-CTRL,                                           "COND-FAN-CTRL",     0, 32065, 0,  0, "COND-FAN-CTRL"
CHILLER,           8, COND-SETPT-T,                                             "COND-SETPT-T",     0, 32065, 0,  1, "COND-SETPT-T"
CHILLER,           8, COND-SETPT-DT,                                           "COND-SETPT-DT",     0, 32065, 0,  2, "COND-SETPT-DT"
CHILLER,           8, MIN-COND-T,                                                 "MIN-COND-T",     0, 32065, 0,  1, "MIN-COND-T"
CHILLER,           8, COND-CAPACITY,                                           "COND-CAPACITY",     0, 32065, 0,  3, "COND-CAPACITY"
CHILLER,           8, SCT-AMB-DT,                                                 "SCT-AMB-DT",     0, 32065, 0,  2, "SCT-AMB-DT"
CHILLER,           8, COND-FAN-EIR,                                             "COND-FAN-EIR",     0, 32065, 0,  4, "COND-FAN-EIR"
CHILLER,           8, COND-PUMP-EIR,                                           "COND-PUMP-EIR",     0, 32065, 0,  4, "COND-PUMP-EIR"
CHILLER,           8, COND-CAP-FT,                                               "COND-CAP-FT",     0, 32065, 0,  0, "COND-CAP-FT"
CHILLER,           8, AMB-FRAC-FT,                                               "AMB-FRAC-FT",     0, 32065, 0,  0, "AMB-FRAC-FT"
CHILLER,           8, COND-PWR-FPLR,                                           "COND-PWR-FPLR",     0, 32065, 0,  0, "COND-PWR-FPLR"
CHILLER,           8, MAX-HTREC,                                       "Maximum Heat Recovery", 12960, 32065, 0,  2, "Maximum fraction of design condenser heat that is available for heat recovery"
CHILLER,           8, HTREC-LOOP,                                         "Heat Recovery Loop", 19114, 19114, 0,  0, "Name of the Heat Recovery Loop that this chiller rejects heat to"
CHILLER,           8, MAX-RECOVER-T,                                                        "", 13531, 32065, 0,  2, "Maximum temperature at which heat can be recovered from the chiller"
CHILLER,           8, HTREC-PUMP,                                                           "", 12998, 32065, 0,  2, "Name of pump dedicated to provide chiller's Heat Recovery Head and Heat Rec. Static Head"
CHILLER,           8, HTREC-DT,                                        "Heat Recovery Delta T", 13005, 32065, 0,  2, "Design temperature change of the water flowing through the heat-recovery condenser"
CHILLER,           8, HTREC-HEAD,                                                           "", 13001, 32065, 0,  2, "Pressure drop through the heat recovery heat exchanger at the design flow rate"
CHILLER,           8, HTREC-STATIC-HEA,                                                     "", 13002, 32065, 0,  2, "Static pressure drop through the heat recovery heat exchanger"
CHILLER,           8, HTREC-FLOW-CTRL,                                                      "", 12999, 32065, 0,  2, "The type of heat recovery water flow through the chiller"
CHILLER,           8, HTREC-MIN-FLOW,                                                       "", 13003, 32065, 0,  2, "Minimum allowable flow rate through the heat-recovery condenser"
CHILLER,           8, EVAP-HX-TD,                                                 "EVAP-HX-TD",     0, 32065, 0,  3, "EVAP-HX-TD"
CHILLER,           8, EVAP-HX-SETPT-T,                                       "EVAP-HX-SETPT-T",     0, 32065, 0,  2, "EVAP-HX-SETPT-T"
CHILLER,           8, COND-HX-TD,                                                 "COND-HX-TD",     0, 32065, 0,  3, "COND-HX-TD"
CHILLER,           8, COND-HX-SETPT-T,                                       "COND-HX-SETPT-T",     0, 32065, 0,  2, "COND-HX-SETPT-T"
CHILLER,           8, COST-DATA,                                                            "", 13799, 32065, 0,  2, "Name of a set of Materials Costs, which specifies first costs, maintenance costs, etc."
CHILLER,           8, EQUIPMENT-REPORT,                                                     "",     0, 32065, 0,  2, "Whether or not a PS-H report is created for this chiller"
CHILLER,           8, PICTURE,                                                              "",     0, 32065, 0,  2, ""
CHILLER,           8, DRAWING,                                                              "",     0, 32065, 0,  2, ""
CHILLER,           9, TYPE,                                                             "Type", 12873, 32065, 0,  0, "PowerDOE has models for nine types of chillers"
CHILLER,           9, CAPACITY,                                                     "Capacity", 13792, 32065, 0,  1, "Nominal (rated) chiller cooling capacity in MBTU/hr (e.g., 100 ton = 1.2 MBTU/hr)"
CHILLER,           9, CAPACITY-RATIO,                                         "Capactiy Ratio", 13793, 32065, 0,  1, "Capacity as fraction of max cooling load (used only if PowerDOE sizes the chiller)"
CHILLER,           9, CAPACITY-FT,                                               "Capacity FT", 12968, 32065, 0,  0, "Bi-Quadratic Curve: Capacity as function of temp of entering condenser & exiting chilled water"
CHILLER,           9, MIN-RATIO,                                               "Minimum Ratio", 12953, 32065, 0,  2, "Minimum chiller operating ratio (a fraction of the Capacity); below this, it cycles on & off"
; SAC 4/18/02 - removed CHILLER:MAX-RATIO
; CHILLER,           9, MAX-RATIO,                                               "Maximum Ratio", 12954, 32065, 0,  2, "Maximum allowable chiller operating ratio (fraction of Capacity, also called max overload ratio)"
CHILLER,           9, HGB-RATIO,                                                   "HGB Ratio", 12952, 32065, 0,  2, "Maximum allowable part-load ratio of the chiller, above which hot gas bypass occures"
CHILLER,           9, ELEC-INPUT-RATIO,                                 "Electric Input Ratio", 12879, 32065, 0,  2, "Dimensionless ratio of electric input power to nominal capacity (i.e., invers of COP)"
CHILLER,           9, EIR-FT,                                                               "", 12967, 32065, 0,  0, "Quadratic Curve Fit: EIR as a function of temp of water entering condenser & leaving chilled"
CHILLER,           9, EIR-FPLR,                                                             "", 12969, 32065, 0,  0, "Quadratic Curve Fit: Electric Input Ratio as a function of the part load ratio"
CHILLER,           9, ELEC-TO-COND,                                    "Electric To Condenser", 12957, 32065, 0,  2, "Efficiency of compressor: i.e., fraction of chiller electricity input rejected to condenser, as heat"
CHILLER,           9, HEAT-INPUT-RATIO,                                     "Heat Input Ratio", 12956, 32065, 0,  2, "Ratio of fuel heat input (in Btus) to full load cooling capacity (in Btus), as rated conditions"
CHILLER,           9, HIR-FT,                                                               "", 12964, 32065, 0,  0, "Bi-Quadratic Curve: HIR as a function of temp of entering condenser and exiting chilled water"
CHILLER,           9, HIR-FPLR,                                                             "", 12965, 32065, 0,  0, "Quadratic Curve Fit: Heat Input Ratio as a function of the part load ratio"
CHILLER,           9, HEAT-TO-COND,                                        "Heat to Condenser", 12882, 32065, 0,  2, "Fraction of fuel or heat input to chiller that is rejected to condenser, as heat"
CHILLER,           9, START-UP-TIME,                                                        "", 13644, 32065, 0,  2, "Equivalent full-load time required to start up the chiller (in hours or fraction of hours)"
CHILLER,           9, SHUT-DOWN-TIME,                                                       "", 13649, 32065, 0,  2, "Equivalent full-load time required to shut down the chiller (in hours or fraction of hours)"
CHILLER,           9, HGB-RATIO-HTREC,                                                      "", 12970, 32065, 0,  2, "The hot gas bypass ratio when the chiller is in the heat recovery mode"
CHILLER,           9, SOLUTION-PUMP-KW,                                                     "", 13650, 32065, 0,  2, "Electricity consumption of the solution pump"
CHILLER,           9, GAS-HCAP-FPLRC,                                                       "", 13787, 32065, 0,  2, "Quadratic Curve: heating capacity as a function of the cooling part load ratio"
CHILLER,           9, GAS-HW-XEFF,                                                          "", 13780, 32065, 0,  2, "The burner efficiency (when the chiller is in the heating mode)"
CHILLER,           9, GAS-DESC-XEFF,                                                        "", 13781, 32065, 0,  2, "The burner efficiency when regenerating a desiccant system"
CHILLER,           9, GAS-COMB-FAN-KW,                                                      "", 13778, 32065, 0,  2, "Electricity consumption of the combustion blower"
CHILLER,           9, GAS-HIR-FDESCT,                                                       "", 13788, 32065, 0,  2, "Quadratic Curve: Heat Input Ratio as a function of the desiccant regeneration temperature"
CHILLER,           9, GAS-QREG-FDESCT,                                                      "", 13789, 32065, 0,  2, "Quadratic Curve: available regeneration energy as a function of the required regeneration temp"
CHILLER,           9, ENG-HEAT-TO-JAC,                                                      "", 13848, 32065, 0,  2, "Fraction of design fuel consumption that is recoverable from the jacket of an engine-chiller"
CHILLER,           9, ENG-HEAT-TO-EXH,                                                      "", 13849, 32065, 0,  2, "Fraction of design fuel consumption that is recoverable from the exhaust of an engine-chiller"
CHILLER,           9, ENG-HTREJ-FT,                                                         "", 13785, 32065, 0,  2, "Quadratic Curve: the amount of recoverable heat as a function of the entering condenser temp"
CHILLER,           9, ENG-HTREJ-FPLR,                                                       "", 13784, 32065, 0,  2, "Quadratic Curve: amount of recoverable heat as a function of the cooling part load ratio"
CHILLER,           9, HEAT/COOL-CAP,                                           "HEAT/COOL-CAP",     0, 32065, 0,  3, "HEAT/COOL-CAP"
CHILLER,           9, HEAT-CAP-FT,                                               "HEAT-CAP-FT",     0, 32065, 0,  0, "HEAT-CAP-FT"
CHILLER,           9, HEAT-CAP-FT-FRST,                                     "HEAT-CAP-FT-FRST",     0, 32065, 0,  0, "HEAT-CAP-FT-FRST"
CHILLER,           9, HEAT-EIR,                                                     "HEAT-EIR",     0, 32065, 0,  3, "HEAT-EIR"
CHILLER,           9, HEAT-EIR-FT,                                               "HEAT-EIR-FT",     0, 32065, 0,  0, "HEAT-EIR-FT"
CHILLER,           9, HEAT-EIR-FT-FRST,                                     "HEAT-EIR-FT-FRST",     0, 32065, 0,  0, "HEAT-EIR-FT-FRST"
CHILLER,           9, HEAT-EIR-FPLR,                                           "HEAT-EIR-FPLR",     0, 32065, 0,  0, "HEAT-EIR-FPLR"
CHILLER,           9, AUX-KW,                                                   "Auxiliary kW", 13795, 32065, 0,  2, "Auxiliary electric power consumption of the chiler (e.g., control panels)"
CHILLER,           9, AUX-MODE,                                                             "", 12987, 32065, 0,  2, "Always=all hours;When On=If chiller on;When Off=if chiller off;Scheduled=use Aux Schedule"
CHILLER,           9, AUX-SCHEDULE,                                       "Auxiliary Schedule", 12988, 32065, 0,  2, "Schedule for Auxiliary Power consumption (set Auxiliary Mode to Scheduled to activate this)"
CHILLER,           9, AUX-METER,                                                            "", 12989, 32065, 0,  0, "Name of the Electric Meter that tallies the electricity consumption of this chiller's auxiliaries"
CHILLER,           9, ELEC-METER,                                             "Electric Meter", 12948, 32065, 0,  0, "Name of the Electric Meter that tallies the electric consumption of this chiller"
CHILLER,           9, FUEL-METER,                                                 "Fuel Meter", 12949, 32065, 0,  0, "Name of the Fuel Meter that tallies the fuel consumption of this chiller"
CHILLER,           9, CHW-LOOP,                                                     "CHW Loop", 19111, 32065, 0,  0, "Name of the primary Chiller Water Loop that this chiller serves"
CHILLER,           9, CHW-PUMP,                                                     "CHW Pump", 13800, 32065, 0,  0, "Name of a Pump that serves the chiller's chilled water loop"
CHILLER,           9, CHW-DT,                                                    "CHW Delta T", 12974, 32065, 0,  2, "Design temperature change of the chilled water through the chiller"
CHILLER,           9, CHW-HEAD,                                                             "", 12975, 32065, 0,  2, "Head loss through the chilled water piping at the design flow rate"
CHILLER,           9, CHW-STATIC-HEAD,                                                      "", 12976, 32065, 0,  2, "The static head in the chiller circuit (typically zero)"
CHILLER,           9, CHW-FLOW-CTRL,                                                        "", 12973, 32065, 0,  2, "The type of flow through the chiller evaporator"
CHILLER,           9, CHW-MIN-FLOW,                                                         "", 12977, 32065, 0,  2, "Minimum allowable fraction of the design flow rate through the evaporator"
CHILLER,           9, CHW-MAX-FLOW,                                                         "", 13491, 32065, 0,  2, "Maximum allowable fraction of the design flow rate through the evaporator"
CHILLER,           9, HW-LOOP,                                                       "HW Loop", 19117, 32065, 0,  0, "Name of HW loop that provides heat to an absorption chiller; or that a chiller/heater heats"
CHILLER,           9, HW-PUMP,                                                              "", 12991, 32065, 0,  2, "Hot Water pump: if not specified, the head requirement is passed to the primary loop"
CHILLER,           9, HW-DT,                                                      "HW Delta T", 12993, 32065, 0,  2, "Design temp change of hot water through the boiler (used to size recirculation pump)"
CHILLER,           9, HW-HEAD,                                                              "", 12994, 32065, 0,  2, "Pressure drop of the hot water through the chiller at the design flowrate"
CHILLER,           9, HW-STATIC-HEAD,                                                       "", 12995, 32065, 0,  2, "Static HW pressure drop through the chiller; use if pumping fluid at atm pressure into loop"
CHILLER,           9, HW-FLOW-CTRL,                                                         "", 12992, 32065, 0,  2, "Constant Flow = independent of the load; Variable Flow = varies linearly with load"
CHILLER,           9, HW-MIN-FLOW,                                                          "", 12996, 32065, 0,  2, "Min hot water flow rate through chiller; used only if Hot Water Flow Control = Variable Flow"
CHILLER,           9, HW-MAX-FLOW,                                                          "", 13492, 32065, 0,  2, "Max hot water flow rate through chiller; used only if Hot Water Flow Control = Variable Flow"
CHILLER,           9, CONDENSER-TYPE,                                         "Condenser Type", 12875, 32065, 0,  0, "Air Cooled=heat exchanger & condenser; Water Cooled=cooling tower & condenser loop"
CHILLER,           9, CW-LOOP,                                                       "CW Loop", 19112, 32065, 0,  0, "If Condenser Type=Water Cooled, CW Loop is required & must be attached to Cooling Tower"
CHILLER,           9, CW-PUMP,                                                       "CW Pump", 12929, 32065, 0,  0, "Name of a Pump that serves the (dedicated) evaporator recirculation loop"
CHILLER,           9, CW-DT,                                                      "CW Delta T", 12981, 32065, 0,  2, "Design temperature change of the water flowing through the condenser"
CHILLER,           9, CW-HEAD,                                                              "", 12982, 32065, 0,  2, "Pressure drop through the condenser at the design flow rate"
CHILLER,           9, CW-STATIC-HEAD,                                                       "", 12983, 32065, 0,  2, "Static pressure drop through the condenser at the design flow rate"
CHILLER,           9, CW-FLOW-CTRL,                                                         "", 12980, 32065, 0,  2, "The type of flow through the condenser"
CHILLER,           9, CW-MIN-FLOW,                                                          "", 12984, 32065, 0,  2, "Minimum allowable flow rate through the condenser (as a fraction of the design flow rate)"
CHILLER,           9, COND-SETPT-CTRL,                                       "COND-SETPT-CTRL",     0, 32065, 0,  0, "COND-SETPT-CTRL"
CHILLER,           9, COND-FAN-CTRL,                                           "COND-FAN-CTRL",     0, 32065, 0,  0, "COND-FAN-CTRL"
CHILLER,           9, COND-SETPT-T,                                             "COND-SETPT-T",     0, 32065, 0,  1, "COND-SETPT-T"
CHILLER,           9, COND-SETPT-DT,                                           "COND-SETPT-DT",     0, 32065, 0,  2, "COND-SETPT-DT"
CHILLER,           9, MIN-COND-T,                                                 "MIN-COND-T",     0, 32065, 0,  1, "MIN-COND-T"
CHILLER,           9, COND-CAPACITY,                                           "COND-CAPACITY",     0, 32065, 0,  3, "COND-CAPACITY"
CHILLER,           9, SCT-AMB-DT,                                                 "SCT-AMB-DT",     0, 32065, 0,  2, "SCT-AMB-DT"
CHILLER,           9, COND-FAN-EIR,                                             "COND-FAN-EIR",     0, 32065, 0,  4, "COND-FAN-EIR"
CHILLER,           9, COND-PUMP-EIR,                                           "COND-PUMP-EIR",     0, 32065, 0,  4, "COND-PUMP-EIR"
CHILLER,           9, COND-CAP-FT,                                               "COND-CAP-FT",     0, 32065, 0,  0, "COND-CAP-FT"
CHILLER,           9, AMB-FRAC-FT,                                               "AMB-FRAC-FT",     0, 32065, 0,  0, "AMB-FRAC-FT"
CHILLER,           9, COND-PWR-FPLR,                                           "COND-PWR-FPLR",     0, 32065, 0,  0, "COND-PWR-FPLR"
CHILLER,           9, MAX-HTREC,                                       "Maximum Heat Recovery", 12960, 32065, 0,  2, "Maximum fraction of design condenser heat that is available for heat recovery"
CHILLER,           9, HTREC-LOOP,                                         "Heat Recovery Loop", 19114, 19114, 0,  0, "Name of the Heat Recovery Loop that this chiller rejects heat to"
CHILLER,           9, MAX-RECOVER-T,                                                        "", 13531, 32065, 0,  2, "Maximum temperature at which heat can be recovered from the chiller"
CHILLER,           9, HTREC-PUMP,                                                           "", 12998, 32065, 0,  2, "Name of pump dedicated to provide chiller's Heat Recovery Head and Heat Rec. Static Head"
CHILLER,           9, HTREC-DT,                                        "Heat Recovery Delta T", 13005, 32065, 0,  2, "Design temperature change of the water flowing through the heat-recovery condenser"
CHILLER,           9, HTREC-HEAD,                                                           "", 13001, 32065, 0,  2, "Pressure drop through the heat recovery heat exchanger at the design flow rate"
CHILLER,           9, HTREC-STATIC-HEA,                                                     "", 13002, 32065, 0,  2, "Static pressure drop through the heat recovery heat exchanger"
CHILLER,           9, HTREC-FLOW-CTRL,                                                      "", 12999, 32065, 0,  2, "The type of heat recovery water flow through the chiller"
CHILLER,           9, HTREC-MIN-FLOW,                                                       "", 13003, 32065, 0,  2, "Minimum allowable flow rate through the heat-recovery condenser"
CHILLER,           9, EVAP-HX-TD,                                                 "EVAP-HX-TD",     0, 32065, 0,  3, "EVAP-HX-TD"
CHILLER,           9, EVAP-HX-SETPT-T,                                       "EVAP-HX-SETPT-T",     0, 32065, 0,  2, "EVAP-HX-SETPT-T"
CHILLER,           9, COND-HX-TD,                                                 "COND-HX-TD",     0, 32065, 0,  3, "COND-HX-TD"
CHILLER,           9, COND-HX-SETPT-T,                                       "COND-HX-SETPT-T",     0, 32065, 0,  2, "COND-HX-SETPT-T"
CHILLER,           9, COST-DATA,                                                            "", 13799, 32065, 0,  2, "Name of a set of Materials Costs, which specifies first costs, maintenance costs, etc."
CHILLER,           9, EQUIPMENT-REPORT,                                                     "",     0, 32065, 0,  2, "Whether or not a PS-H report is created for this chiller"
CHILLER,           9, PICTURE,                                                              "",     0, 32065, 0,  2, ""
CHILLER,           9, DRAWING,                                                              "",     0, 32065, 0,  2, ""
CHILLER,          10, TYPE,                                                             "Type", 12873, 32065, 0,  0, "PowerDOE has models for nine types of chillers"
CHILLER,          10, CAPACITY,                                                     "Capacity", 13792, 32065, 0,  1, "Nominal (rated) chiller cooling capacity in MBTU/hr (e.g., 100 ton = 1.2 MBTU/hr)"
CHILLER,          10, CAPACITY-RATIO,                                         "Capactiy Ratio", 13793, 32065, 0,  1, "Capacity as fraction of max cooling load (used only if PowerDOE sizes the chiller)"
CHILLER,          10, CAPACITY-FT,                                               "Capacity FT", 12968, 32065, 0,  0, "Bi-Quadratic Curve: Capacity as function of temp of entering condenser & exiting chilled water"
CHILLER,          10, MIN-RATIO,                                               "Minimum Ratio", 12953, 32065, 0,  2, "Minimum chiller operating ratio (a fraction of the Capacity); below this, it cycles on & off"
; SAC 4/18/02 - removed CHILLER:MAX-RATIO
; CHILLER,          10, MAX-RATIO,                                               "Maximum Ratio", 12954, 32065, 0,  2, "Maximum allowable chiller operating ratio (fraction of Capacity, also called max overload ratio)"
CHILLER,          10, HGB-RATIO,                                                   "HGB Ratio", 12952, 32065, 0,  2, "Maximum allowable part-load ratio of the chiller, above which hot gas bypass occures"
CHILLER,          10, ELEC-INPUT-RATIO,                                 "Electric Input Ratio", 12879, 32065, 0,  2, "Dimensionless ratio of electric input power to nominal capacity (i.e., invers of COP)"
CHILLER,          10, EIR-FT,                                                               "", 12967, 32065, 0,  0, "Quadratic Curve Fit: EIR as a function of temp of water entering condenser & leaving chilled"
CHILLER,          10, EIR-FPLR,                                                             "", 12969, 32065, 0,  0, "Quadratic Curve Fit: Electric Input Ratio as a function of the part load ratio"
CHILLER,          10, ELEC-TO-COND,                                    "Electric To Condenser", 12957, 32065, 0,  2, "Efficiency of compressor: i.e., fraction of chiller electricity input rejected to condenser, as heat"
CHILLER,          10, HEAT-INPUT-RATIO,                                     "Heat Input Ratio", 12956, 32065, 0,  2, "Ratio of fuel heat input (in Btus) to full load cooling capacity (in Btus), as rated conditions"
CHILLER,          10, HIR-FT,                                                               "", 12964, 32065, 0,  0, "Bi-Quadratic Curve: HIR as a function of temp of entering condenser and exiting chilled water"
CHILLER,          10, HIR-FPLR,                                                             "", 12965, 32065, 0,  0, "Quadratic Curve Fit: Heat Input Ratio as a function of the part load ratio"
CHILLER,          10, HEAT-TO-COND,                                        "Heat to Condenser", 12882, 32065, 0,  2, "Fraction of fuel or heat input to chiller that is rejected to condenser, as heat"
CHILLER,          10, START-UP-TIME,                                                        "", 13644, 32065, 0,  2, "Equivalent full-load time required to start up the chiller (in hours or fraction of hours)"
CHILLER,          10, SHUT-DOWN-TIME,                                                       "", 13649, 32065, 0,  2, "Equivalent full-load time required to shut down the chiller (in hours or fraction of hours)"
CHILLER,          10, HGB-RATIO-HTREC,                                                      "", 12970, 32065, 0,  2, "The hot gas bypass ratio when the chiller is in the heat recovery mode"
CHILLER,          10, SOLUTION-PUMP-KW,                                                     "", 13650, 32065, 0,  2, "Electricity consumption of the solution pump"
CHILLER,          10, GAS-HCAP-FPLRC,                                                       "", 13787, 32065, 0,  2, "Quadratic Curve: heating capacity as a function of the cooling part load ratio"
CHILLER,          10, GAS-HW-XEFF,                                                          "", 13780, 32065, 0,  2, "The burner efficiency (when the chiller is in the heating mode)"
CHILLER,          10, GAS-DESC-XEFF,                                                        "", 13781, 32065, 0,  2, "The burner efficiency when regenerating a desiccant system"
CHILLER,          10, GAS-COMB-FAN-KW,                                                      "", 13778, 32065, 0,  2, "Electricity consumption of the combustion blower"
CHILLER,          10, GAS-HIR-FDESCT,                                                       "", 13788, 32065, 0,  2, "Quadratic Curve: Heat Input Ratio as a function of the desiccant regeneration temperature"
CHILLER,          10, GAS-QREG-FDESCT,                                                      "", 13789, 32065, 0,  2, "Quadratic Curve: available regeneration energy as a function of the required regeneration temp"
CHILLER,          10, ENG-HEAT-TO-JAC,                                                      "", 13848, 32065, 0,  2, "Fraction of design fuel consumption that is recoverable from the jacket of an engine-chiller"
CHILLER,          10, ENG-HEAT-TO-EXH,                                                      "", 13849, 32065, 0,  2, "Fraction of design fuel consumption that is recoverable from the exhaust of an engine-chiller"
CHILLER,          10, ENG-HTREJ-FT,                                                         "", 13785, 32065, 0,  2, "Quadratic Curve: the amount of recoverable heat as a function of the entering condenser temp"
CHILLER,          10, ENG-HTREJ-FPLR,                                                       "", 13784, 32065, 0,  2, "Quadratic Curve: amount of recoverable heat as a function of the cooling part load ratio"
CHILLER,          10, HEAT/COOL-CAP,                                           "HEAT/COOL-CAP",     0, 32065, 0,  3, "HEAT/COOL-CAP"
CHILLER,          10, HEAT-CAP-FT,                                               "HEAT-CAP-FT",     0, 32065, 0,  0, "HEAT-CAP-FT"
CHILLER,          10, HEAT-CAP-FT-FRST,                                     "HEAT-CAP-FT-FRST",     0, 32065, 0,  0, "HEAT-CAP-FT-FRST"
CHILLER,          10, HEAT-EIR,                                                     "HEAT-EIR",     0, 32065, 0,  3, "HEAT-EIR"
CHILLER,          10, HEAT-EIR-FT,                                               "HEAT-EIR-FT",     0, 32065, 0,  0, "HEAT-EIR-FT"
CHILLER,          10, HEAT-EIR-FT-FRST,                                     "HEAT-EIR-FT-FRST",     0, 32065, 0,  0, "HEAT-EIR-FT-FRST"
CHILLER,          10, HEAT-EIR-FPLR,                                           "HEAT-EIR-FPLR",     0, 32065, 0,  0, "HEAT-EIR-FPLR"
CHILLER,          10, AUX-KW,                                                   "Auxiliary kW", 13795, 32065, 0,  2, "Auxiliary electric power consumption of the chiler (e.g., control panels)"
CHILLER,          10, AUX-MODE,                                                             "", 12987, 32065, 0,  2, "Always=all hours;When On=If chiller on;When Off=if chiller off;Scheduled=use Aux Schedule"
CHILLER,          10, AUX-SCHEDULE,                                       "Auxiliary Schedule", 12988, 32065, 0,  2, "Schedule for Auxiliary Power consumption (set Auxiliary Mode to Scheduled to activate this)"
CHILLER,          10, AUX-METER,                                                            "", 12989, 32065, 0,  0, "Name of the Electric Meter that tallies the electricity consumption of this chiller's auxiliaries"
CHILLER,          10, ELEC-METER,                                             "Electric Meter", 12948, 32065, 0,  0, "Name of the Electric Meter that tallies the electric consumption of this chiller"
CHILLER,          10, FUEL-METER,                                                 "Fuel Meter", 12949, 32065, 0,  0, "Name of the Fuel Meter that tallies the fuel consumption of this chiller"
CHILLER,          10, CHW-LOOP,                                                     "CHW Loop", 19111, 32065, 0,  0, "Name of the primary Chiller Water Loop that this chiller serves"
CHILLER,          10, CHW-PUMP,                                                     "CHW Pump", 13800, 32065, 0,  0, "Name of a Pump that serves the chiller's chilled water loop"
CHILLER,          10, CHW-DT,                                                    "CHW Delta T", 12974, 32065, 0,  2, "Design temperature change of the chilled water through the chiller"
CHILLER,          10, CHW-HEAD,                                                             "", 12975, 32065, 0,  2, "Head loss through the chilled water piping at the design flow rate"
CHILLER,          10, CHW-STATIC-HEAD,                                                      "", 12976, 32065, 0,  2, "The static head in the chiller circuit (typically zero)"
CHILLER,          10, CHW-FLOW-CTRL,                                                        "", 12973, 32065, 0,  2, "The type of flow through the chiller evaporator"
CHILLER,          10, CHW-MIN-FLOW,                                                         "", 12977, 32065, 0,  2, "Minimum allowable fraction of the design flow rate through the evaporator"
CHILLER,          10, CHW-MAX-FLOW,                                                         "", 13491, 32065, 0,  2, "Maximum allowable fraction of the design flow rate through the evaporator"
CHILLER,          10, HW-LOOP,                                                       "HW Loop", 19117, 32065, 0,  0, "Name of HW loop that provides heat to an absorption chiller; or that a chiller/heater heats"
CHILLER,          10, HW-PUMP,                                                              "", 12991, 32065, 0,  2, "Hot Water pump: if not specified, the head requirement is passed to the primary loop"
CHILLER,          10, HW-DT,                                                      "HW Delta T", 12993, 32065, 0,  2, "Design temp change of hot water through the boiler (used to size recirculation pump)"
CHILLER,          10, HW-HEAD,                                                              "", 12994, 32065, 0,  2, "Pressure drop of the hot water through the chiller at the design flowrate"
CHILLER,          10, HW-STATIC-HEAD,                                                       "", 12995, 32065, 0,  2, "Static HW pressure drop through the chiller; use if pumping fluid at atm pressure into loop"
CHILLER,          10, HW-FLOW-CTRL,                                                         "", 12992, 32065, 0,  2, "Constant Flow = independent of the load; Variable Flow = varies linearly with load"
CHILLER,          10, HW-MIN-FLOW,                                                          "", 12996, 32065, 0,  2, "Min hot water flow rate through chiller; used only if Hot Water Flow Control = Variable Flow"
CHILLER,          10, HW-MAX-FLOW,                                                          "", 13492, 32065, 0,  2, "Max hot water flow rate through chiller; used only if Hot Water Flow Control = Variable Flow"
CHILLER,          10, CONDENSER-TYPE,                                         "Condenser Type", 12875, 32065, 0,  0, "Air Cooled=heat exchanger & condenser; Water Cooled=cooling tower & condenser loop"
CHILLER,          10, CW-LOOP,                                                       "CW Loop", 19112, 32065, 0,  0, "If Condenser Type=Water Cooled, CW Loop is required & must be attached to Cooling Tower"
CHILLER,          10, CW-PUMP,                                                       "CW Pump", 12929, 32065, 0,  0, "Name of a Pump that serves the (dedicated) evaporator recirculation loop"
CHILLER,          10, CW-DT,                                                      "CW Delta T", 12981, 32065, 0,  2, "Design temperature change of the water flowing through the condenser"
CHILLER,          10, CW-HEAD,                                                              "", 12982, 32065, 0,  2, "Pressure drop through the condenser at the design flow rate"
CHILLER,          10, CW-STATIC-HEAD,                                                       "", 12983, 32065, 0,  2, "Static pressure drop through the condenser at the design flow rate"
CHILLER,          10, CW-FLOW-CTRL,                                                         "", 12980, 32065, 0,  2, "The type of flow through the condenser"
CHILLER,          10, CW-MIN-FLOW,                                                          "", 12984, 32065, 0,  2, "Minimum allowable flow rate through the condenser (as a fraction of the design flow rate)"
CHILLER,          10, COND-SETPT-CTRL,                                       "COND-SETPT-CTRL",     0, 32065, 0,  0, "COND-SETPT-CTRL"
CHILLER,          10, COND-FAN-CTRL,                                           "COND-FAN-CTRL",     0, 32065, 0,  0, "COND-FAN-CTRL"
CHILLER,          10, COND-SETPT-T,                                             "COND-SETPT-T",     0, 32065, 0,  1, "COND-SETPT-T"
CHILLER,          10, COND-SETPT-DT,                                           "COND-SETPT-DT",     0, 32065, 0,  2, "COND-SETPT-DT"
CHILLER,          10, MIN-COND-T,                                                 "MIN-COND-T",     0, 32065, 0,  1, "MIN-COND-T"
CHILLER,          10, COND-CAPACITY,                                           "COND-CAPACITY",     0, 32065, 0,  3, "COND-CAPACITY"
CHILLER,          10, SCT-AMB-DT,                                                 "SCT-AMB-DT",     0, 32065, 0,  2, "SCT-AMB-DT"
CHILLER,          10, COND-FAN-EIR,                                             "COND-FAN-EIR",     0, 32065, 0,  4, "COND-FAN-EIR"
CHILLER,          10, COND-PUMP-EIR,                                           "COND-PUMP-EIR",     0, 32065, 0,  4, "COND-PUMP-EIR"
CHILLER,          10, COND-CAP-FT,                                               "COND-CAP-FT",     0, 32065, 0,  0, "COND-CAP-FT"
CHILLER,          10, AMB-FRAC-FT,                                               "AMB-FRAC-FT",     0, 32065, 0,  0, "AMB-FRAC-FT"
CHILLER,          10, COND-PWR-FPLR,                                           "COND-PWR-FPLR",     0, 32065, 0,  0, "COND-PWR-FPLR"
CHILLER,          10, MAX-HTREC,                                       "Maximum Heat Recovery", 12960, 32065, 0,  2, "Maximum fraction of design condenser heat that is available for heat recovery"
CHILLER,          10, HTREC-LOOP,                                         "Heat Recovery Loop", 19114, 19114, 0,  0, "Name of the Heat Recovery Loop that this chiller rejects heat to"
CHILLER,          10, MAX-RECOVER-T,                                                        "", 13531, 32065, 0,  2, "Maximum temperature at which heat can be recovered from the chiller"
CHILLER,          10, HTREC-PUMP,                                                           "", 12998, 32065, 0,  2, "Name of pump dedicated to provide chiller's Heat Recovery Head and Heat Rec. Static Head"
CHILLER,          10, HTREC-DT,                                        "Heat Recovery Delta T", 13005, 32065, 0,  2, "Design temperature change of the water flowing through the heat-recovery condenser"
CHILLER,          10, HTREC-HEAD,                                                           "", 13001, 32065, 0,  2, "Pressure drop through the heat recovery heat exchanger at the design flow rate"
CHILLER,          10, HTREC-STATIC-HEA,                                                     "", 13002, 32065, 0,  2, "Static pressure drop through the heat recovery heat exchanger"
CHILLER,          10, HTREC-FLOW-CTRL,                                                      "", 12999, 32065, 0,  2, "The type of heat recovery water flow through the chiller"
CHILLER,          10, HTREC-MIN-FLOW,                                                       "", 13003, 32065, 0,  2, "Minimum allowable flow rate through the heat-recovery condenser"
CHILLER,          10, EVAP-HX-TD,                                                 "EVAP-HX-TD",     0, 32065, 0,  3, "EVAP-HX-TD"
CHILLER,          10, EVAP-HX-SETPT-T,                                       "EVAP-HX-SETPT-T",     0, 32065, 0,  2, "EVAP-HX-SETPT-T"
CHILLER,          10, COND-HX-TD,                                                 "COND-HX-TD",     0, 32065, 0,  3, "COND-HX-TD"
CHILLER,          10, COND-HX-SETPT-T,                                       "COND-HX-SETPT-T",     0, 32065, 0,  2, "COND-HX-SETPT-T"
CHILLER,          10, COST-DATA,                                                            "", 13799, 32065, 0,  2, "Name of a set of Materials Costs, which specifies first costs, maintenance costs, etc."
CHILLER,          10, EQUIPMENT-REPORT,                                                     "",     0, 32065, 0,  2, "Whether or not a PS-H report is created for this chiller"
CHILLER,          10, PICTURE,                                                              "",     0, 32065, 0,  2, ""
CHILLER,          10, DRAWING,                                                              "",     0, 32065, 0,  2, ""
CHILLER,          11, TYPE,                                                             "Type", 12873, 32065, 0,  0, "PowerDOE has models for nine types of chillers"
CHILLER,          11, CAPACITY,                                                     "Capacity", 13792, 32065, 0,  1, "Nominal (rated) chiller cooling capacity in MBTU/hr (e.g., 100 ton = 1.2 MBTU/hr)"
CHILLER,          11, CAPACITY-RATIO,                                         "Capactiy Ratio", 13793, 32065, 0,  1, "Capacity as fraction of max cooling load (used only if PowerDOE sizes the chiller)"
CHILLER,          11, CAPACITY-FT,                                               "Capacity FT", 12968, 32065, 0,  0, "Bi-Quadratic Curve: Capacity as function of temp of entering condenser & exiting chilled water"
CHILLER,          11, MIN-RATIO,                                               "Minimum Ratio", 12953, 32065, 0,  2, "Minimum chiller operating ratio (a fraction of the Capacity); below this, it cycles on & off"
; SAC 4/18/02 - removed CHILLER:MAX-RATIO
; CHILLER,          11, MAX-RATIO,                                               "Maximum Ratio", 12954, 32065, 0,  2, "Maximum allowable chiller operating ratio (fraction of Capacity, also called max overload ratio)"
CHILLER,          11, HGB-RATIO,                                                   "HGB Ratio", 12952, 32065, 0,  2, "Maximum allowable part-load ratio of the chiller, above which hot gas bypass occures"
CHILLER,          11, ELEC-INPUT-RATIO,                                 "Electric Input Ratio", 12879, 32065, 0,  2, "Dimensionless ratio of electric input power to nominal capacity (i.e., invers of COP)"
CHILLER,          11, EIR-FT,                                                               "", 12967, 32065, 0,  0, "Quadratic Curve Fit: EIR as a function of temp of water entering condenser & leaving chilled"
CHILLER,          11, EIR-FPLR,                                                             "", 12969, 32065, 0,  0, "Quadratic Curve Fit: Electric Input Ratio as a function of the part load ratio"
CHILLER,          11, ELEC-TO-COND,                                    "Electric To Condenser", 12957, 32065, 0,  2, "Efficiency of compressor: i.e., fraction of chiller electricity input rejected to condenser, as heat"
CHILLER,          11, HEAT-INPUT-RATIO,                                     "Heat Input Ratio", 12956, 32065, 0,  2, "Ratio of fuel heat input (in Btus) to full load cooling capacity (in Btus), as rated conditions"
CHILLER,          11, HIR-FT,                                                               "", 12964, 32065, 0,  0, "Bi-Quadratic Curve: HIR as a function of temp of entering condenser and exiting chilled water"
CHILLER,          11, HIR-FPLR,                                                             "", 12965, 32065, 0,  0, "Quadratic Curve Fit: Heat Input Ratio as a function of the part load ratio"
CHILLER,          11, HEAT-TO-COND,                                        "Heat to Condenser", 12882, 32065, 0,  2, "Fraction of fuel or heat input to chiller that is rejected to condenser, as heat"
CHILLER,          11, START-UP-TIME,                                                        "", 13644, 32065, 0,  2, "Equivalent full-load time required to start up the chiller (in hours or fraction of hours)"
CHILLER,          11, SHUT-DOWN-TIME,                                                       "", 13649, 32065, 0,  2, "Equivalent full-load time required to shut down the chiller (in hours or fraction of hours)"
CHILLER,          11, HGB-RATIO-HTREC,                                                      "", 12970, 32065, 0,  2, "The hot gas bypass ratio when the chiller is in the heat recovery mode"
CHILLER,          11, SOLUTION-PUMP-KW,                                                     "", 13650, 32065, 0,  2, "Electricity consumption of the solution pump"
CHILLER,          11, GAS-HCAP-FPLRC,                                                       "", 13787, 32065, 0,  2, "Quadratic Curve: heating capacity as a function of the cooling part load ratio"
CHILLER,          11, GAS-HW-XEFF,                                                          "", 13780, 32065, 0,  2, "The burner efficiency (when the chiller is in the heating mode)"
CHILLER,          11, GAS-DESC-XEFF,                                                        "", 13781, 32065, 0,  2, "The burner efficiency when regenerating a desiccant system"
CHILLER,          11, GAS-COMB-FAN-KW,                                                      "", 13778, 32065, 0,  2, "Electricity consumption of the combustion blower"
CHILLER,          11, GAS-HIR-FDESCT,                                                       "", 13788, 32065, 0,  2, "Quadratic Curve: Heat Input Ratio as a function of the desiccant regeneration temperature"
CHILLER,          11, GAS-QREG-FDESCT,                                                      "", 13789, 32065, 0,  2, "Quadratic Curve: available regeneration energy as a function of the required regeneration temp"
CHILLER,          11, ENG-HEAT-TO-JAC,                                                      "", 13848, 32065, 0,  2, "Fraction of design fuel consumption that is recoverable from the jacket of an engine-chiller"
CHILLER,          11, ENG-HEAT-TO-EXH,                                                      "", 13849, 32065, 0,  2, "Fraction of design fuel consumption that is recoverable from the exhaust of an engine-chiller"
CHILLER,          11, ENG-HTREJ-FT,                                                         "", 13785, 32065, 0,  2, "Quadratic Curve: the amount of recoverable heat as a function of the entering condenser temp"
CHILLER,          11, ENG-HTREJ-FPLR,                                                       "", 13784, 32065, 0,  2, "Quadratic Curve: amount of recoverable heat as a function of the cooling part load ratio"
CHILLER,          11, HEAT/COOL-CAP,                                           "HEAT/COOL-CAP",     0, 32065, 0,  3, "HEAT/COOL-CAP"
CHILLER,          11, HEAT-CAP-FT,                                               "HEAT-CAP-FT",     0, 32065, 0,  0, "HEAT-CAP-FT"
CHILLER,          11, HEAT-CAP-FT-FRST,                                     "HEAT-CAP-FT-FRST",     0, 32065, 0,  0, "HEAT-CAP-FT-FRST"
CHILLER,          11, HEAT-EIR,                                                     "HEAT-EIR",     0, 32065, 0,  3, "HEAT-EIR"
CHILLER,          11, HEAT-EIR-FT,                                               "HEAT-EIR-FT",     0, 32065, 0,  0, "HEAT-EIR-FT"
CHILLER,          11, HEAT-EIR-FT-FRST,                                     "HEAT-EIR-FT-FRST",     0, 32065, 0,  0, "HEAT-EIR-FT-FRST"
CHILLER,          11, HEAT-EIR-FPLR,                                           "HEAT-EIR-FPLR",     0, 32065, 0,  0, "HEAT-EIR-FPLR"
CHILLER,          11, AUX-KW,                                                   "Auxiliary kW", 13795, 32065, 0,  2, "Auxiliary electric power consumption of the chiler (e.g., control panels)"
CHILLER,          11, AUX-MODE,                                                             "", 12987, 32065, 0,  2, "Always=all hours;When On=If chiller on;When Off=if chiller off;Scheduled=use Aux Schedule"
CHILLER,          11, AUX-SCHEDULE,                                       "Auxiliary Schedule", 12988, 32065, 0,  2, "Schedule for Auxiliary Power consumption (set Auxiliary Mode to Scheduled to activate this)"
CHILLER,          11, AUX-METER,                                                            "", 12989, 32065, 0,  0, "Name of the Electric Meter that tallies the electricity consumption of this chiller's auxiliaries"
CHILLER,          11, ELEC-METER,                                             "Electric Meter", 12948, 32065, 0,  0, "Name of the Electric Meter that tallies the electric consumption of this chiller"
CHILLER,          11, FUEL-METER,                                                 "Fuel Meter", 12949, 32065, 0,  0, "Name of the Fuel Meter that tallies the fuel consumption of this chiller"
CHILLER,          11, CHW-LOOP,                                                     "CHW Loop", 19111, 32065, 0,  0, "Name of the primary Chiller Water Loop that this chiller serves"
CHILLER,          11, CHW-PUMP,                                                     "CHW Pump", 13800, 32065, 0,  0, "Name of a Pump that serves the chiller's chilled water loop"
CHILLER,          11, CHW-DT,                                                    "CHW Delta T", 12974, 32065, 0,  2, "Design temperature change of the chilled water through the chiller"
CHILLER,          11, CHW-HEAD,                                                             "", 12975, 32065, 0,  2, "Head loss through the chilled water piping at the design flow rate"
CHILLER,          11, CHW-STATIC-HEAD,                                                      "", 12976, 32065, 0,  2, "The static head in the chiller circuit (typically zero)"
CHILLER,          11, CHW-FLOW-CTRL,                                                        "", 12973, 32065, 0,  2, "The type of flow through the chiller evaporator"
CHILLER,          11, CHW-MIN-FLOW,                                                         "", 12977, 32065, 0,  2, "Minimum allowable fraction of the design flow rate through the evaporator"
CHILLER,          11, CHW-MAX-FLOW,                                                         "", 13491, 32065, 0,  2, "Maximum allowable fraction of the design flow rate through the evaporator"
CHILLER,          11, HW-LOOP,                                                       "HW Loop", 19117, 32065, 0,  0, "Name of HW loop that provides heat to an absorption chiller; or that a chiller/heater heats"
CHILLER,          11, HW-PUMP,                                                              "", 12991, 32065, 0,  2, "Hot Water pump: if not specified, the head requirement is passed to the primary loop"
CHILLER,          11, HW-DT,                                                      "HW Delta T", 12993, 32065, 0,  2, "Design temp change of hot water through the boiler (used to size recirculation pump)"
CHILLER,          11, HW-HEAD,                                                              "", 12994, 32065, 0,  2, "Pressure drop of the hot water through the chiller at the design flowrate"
CHILLER,          11, HW-STATIC-HEAD,                                                       "", 12995, 32065, 0,  2, "Static HW pressure drop through the chiller; use if pumping fluid at atm pressure into loop"
CHILLER,          11, HW-FLOW-CTRL,                                                         "", 12992, 32065, 0,  2, "Constant Flow = independent of the load; Variable Flow = varies linearly with load"
CHILLER,          11, HW-MIN-FLOW,                                                          "", 12996, 32065, 0,  2, "Min hot water flow rate through chiller; used only if Hot Water Flow Control = Variable Flow"
CHILLER,          11, HW-MAX-FLOW,                                                          "", 13492, 32065, 0,  2, "Max hot water flow rate through chiller; used only if Hot Water Flow Control = Variable Flow"
CHILLER,          11, CONDENSER-TYPE,                                         "Condenser Type", 12875, 32065, 0,  0, "Air Cooled=heat exchanger & condenser; Water Cooled=cooling tower & condenser loop"
CHILLER,          11, CW-LOOP,                                                       "CW Loop", 19112, 32065, 0,  0, "If Condenser Type=Water Cooled, CW Loop is required & must be attached to Cooling Tower"
CHILLER,          11, CW-PUMP,                                                       "CW Pump", 12929, 32065, 0,  0, "Name of a Pump that serves the (dedicated) evaporator recirculation loop"
CHILLER,          11, CW-DT,                                                      "CW Delta T", 12981, 32065, 0,  2, "Design temperature change of the water flowing through the condenser"
CHILLER,          11, CW-HEAD,                                                              "", 12982, 32065, 0,  2, "Pressure drop through the condenser at the design flow rate"
CHILLER,          11, CW-STATIC-HEAD,                                                       "", 12983, 32065, 0,  2, "Static pressure drop through the condenser at the design flow rate"
CHILLER,          11, CW-FLOW-CTRL,                                                         "", 12980, 32065, 0,  2, "The type of flow through the condenser"
CHILLER,          11, CW-MIN-FLOW,                                                          "", 12984, 32065, 0,  2, "Minimum allowable flow rate through the condenser (as a fraction of the design flow rate)"
CHILLER,          11, COND-SETPT-CTRL,                                       "COND-SETPT-CTRL",     0, 32065, 0,  0, "COND-SETPT-CTRL"
CHILLER,          11, COND-FAN-CTRL,                                           "COND-FAN-CTRL",     0, 32065, 0,  0, "COND-FAN-CTRL"
CHILLER,          11, COND-SETPT-T,                                             "COND-SETPT-T",     0, 32065, 0,  1, "COND-SETPT-T"
CHILLER,          11, COND-SETPT-DT,                                           "COND-SETPT-DT",     0, 32065, 0,  2, "COND-SETPT-DT"
CHILLER,          11, MIN-COND-T,                                                 "MIN-COND-T",     0, 32065, 0,  1, "MIN-COND-T"
CHILLER,          11, COND-CAPACITY,                                           "COND-CAPACITY",     0, 32065, 0,  3, "COND-CAPACITY"
CHILLER,          11, SCT-AMB-DT,                                                 "SCT-AMB-DT",     0, 32065, 0,  2, "SCT-AMB-DT"
CHILLER,          11, COND-FAN-EIR,                                             "COND-FAN-EIR",     0, 32065, 0,  4, "COND-FAN-EIR"
CHILLER,          11, COND-PUMP-EIR,                                           "COND-PUMP-EIR",     0, 32065, 0,  4, "COND-PUMP-EIR"
CHILLER,          11, COND-CAP-FT,                                               "COND-CAP-FT",     0, 32065, 0,  0, "COND-CAP-FT"
CHILLER,          11, AMB-FRAC-FT,                                               "AMB-FRAC-FT",     0, 32065, 0,  0, "AMB-FRAC-FT"
CHILLER,          11, COND-PWR-FPLR,                                           "COND-PWR-FPLR",     0, 32065, 0,  0, "COND-PWR-FPLR"
CHILLER,          11, MAX-HTREC,                                       "Maximum Heat Recovery", 12960, 32065, 0,  2, "Maximum fraction of design condenser heat that is available for heat recovery"
CHILLER,          11, HTREC-LOOP,                                         "Heat Recovery Loop", 19114, 19114, 0,  0, "Name of the Heat Recovery Loop that this chiller rejects heat to"
CHILLER,          11, MAX-RECOVER-T,                                                        "", 13531, 32065, 0,  2, "Maximum temperature at which heat can be recovered from the chiller"
CHILLER,          11, HTREC-PUMP,                                                           "", 12998, 32065, 0,  2, "Name of pump dedicated to provide chiller's Heat Recovery Head and Heat Rec. Static Head"
CHILLER,          11, HTREC-DT,                                        "Heat Recovery Delta T", 13005, 32065, 0,  2, "Design temperature change of the water flowing through the heat-recovery condenser"
CHILLER,          11, HTREC-HEAD,                                                           "", 13001, 32065, 0,  2, "Pressure drop through the heat recovery heat exchanger at the design flow rate"
CHILLER,          11, HTREC-STATIC-HEA,                                                     "", 13002, 32065, 0,  2, "Static pressure drop through the heat recovery heat exchanger"
CHILLER,          11, HTREC-FLOW-CTRL,                                                      "", 12999, 32065, 0,  2, "The type of heat recovery water flow through the chiller"
CHILLER,          11, HTREC-MIN-FLOW,                                                       "", 13003, 32065, 0,  2, "Minimum allowable flow rate through the heat-recovery condenser"
CHILLER,          11, EVAP-HX-TD,                                                 "EVAP-HX-TD",     0, 32065, 0,  3, "EVAP-HX-TD"
CHILLER,          11, EVAP-HX-SETPT-T,                                       "EVAP-HX-SETPT-T",     0, 32065, 0,  2, "EVAP-HX-SETPT-T"
CHILLER,          11, COND-HX-TD,                                                 "COND-HX-TD",     0, 32065, 0,  3, "COND-HX-TD"
CHILLER,          11, COND-HX-SETPT-T,                                       "COND-HX-SETPT-T",     0, 32065, 0,  2, "COND-HX-SETPT-T"
CHILLER,          11, COST-DATA,                                                            "", 13799, 32065, 0,  2, "Name of a set of Materials Costs, which specifies first costs, maintenance costs, etc."
CHILLER,          11, EQUIPMENT-REPORT,                                                     "",     0, 32065, 0,  2, "Whether or not a PS-H report is created for this chiller"
CHILLER,          11, PICTURE,                                                              "",     0, 32065, 0,  2, ""
CHILLER,          11, DRAWING,                                                              "",     0, 32065, 0,  2, ""
BOILER,            0, TYPE,                                                             "Type", 12792, 32066, 0,  0, "Can be fuel or electric, hot water or steam, and with or without draft fans"
BOILER,            0, CAPACITY,                                                     "Capacity", 12796, 32066, 0,  1, "Nominal (rated) heating capacity of the boiler (in millions of BTU's per hour)"
BOILER,            0, CAPACITY-RATIO,                                         "Capacity Ratio", 12797, 32066, 0,  1, "Capacity as fraction of max heating load (used only if PowerDOE sizes the boiler)"
BOILER,            0, CAPACITY-FT,                                               "Capacity FT", 12176, 32066, 0,  1, "Bi-Quadratic Curve: Capacity as a function of the temp of entering and exiting water"
BOILER,            0, MIN-RATIO,                                               "Minimum Ratio", 12141, 32066, 0,  2, "Minimum boiler operating ratio (a fraction of the Capacity); below this, it cycles on & off"
BOILER,            0, MAX-RATIO,                                               "Maximum Ratio", 12145, 32066, 0,  2, "Maximum allowable boiler operating ratio (a fraction of the Capacity)"
BOILER,            0, ELEC-INPUT-RATIO,                                 "Electric Input Ratio", 12799, 32066, 0,  2, "Dimensionless ratio of electric input power to nominal capacity (at rated conditions)"
BOILER,            0, EIR-FPLR,                                                             "", 12175, 32066, 0,  0, "Quadratic Curve Fit: Electric Input Ratio as a function of the part load ratio"
BOILER,            0, HEAT-INPUT-RATIO,                                     "Heat Input Ratio", 12798, 32066, 0,  2, "Dimensionless ratio of fuel heat input to boiler output at full load (at rated conditions)"
BOILER,            0, HIR-FT,                                                               "", 12174, 32066, 0,  0, "Bi-Quadratic Curve: the HIR as a function of the temp of entering and exiting water"
BOILER,            0, HIR-FPLR,                                                             "", 12172, 32066, 0,  0, "Quadratic Curve Fit: Heat Input Ratio as a function of the part load ratio"
BOILER,            0, LOCATION,                                                             "", 12758, 32066, 0,  0, "Outdoors=heat lost to environment; Zone=heat lost to the Boiler Zone"
BOILER,            0, ZONE-NAME,                                                 "Boiler Zone", 12087, 32066, 0,  0, "Name of zone that the boiler is in (draws combustion air from here)"
BOILER,            0, START-UP-TIME,                                                        "",   684, 32066, 0,  0, "Equivalent full-load time (in hours) required to bring the boiler on-line"
BOILER,            0, AUX-KW,                                                   "Auxiliary kW", 12807, 32066, 0,  0, "Auxiliary electric power consumption of the boiler (e.g., control panels)"
BOILER,            0, AUX-MODE,                                               "Auxiliary Mode", 12198, 32066, 0,  0, "Always=all hours;When On=If boiler on;When Off=if boiler off;Scheduled=use Aux Schedule"
BOILER,            0, AUX-SCHEDULE,                                       "Auxiliary Schedule", 12199, 32066, 0,  0, "Schedule for Auxiliary Power consumption (set Auxiliary Mode to Scheduled to activate this)"
BOILER,            0, AUX-METER,                                            "Auxililary Meter", 12200, 32066, 0,  0, "Name of the Electric Meter that tallies the electricity consumption of this boiler's auxiliaries"
BOILER,            0, ELEC-METER,                                             "Electric Meter", 12810, 32066, 0,  0, "Name of the Electric Meter that tallies the electricity consumption of this boiler"
BOILER,            0, FUEL-METER,                                                 "Fuel Meter", 12809, 32066, 0,  0, "Name of the Fuel Meter that tallies the fuel consumption of this boiler"
BOILER,            0, AQUASTAT-SETPT-T,                                                     "", 13186, 32066, 0,  0, "The setpoint of the boiler's internal aquastat"
BOILER,            0, HW-LOOP,                                                       "HW Loop", 19129, 32066, 0,  0, "Name of the loop that the boiler serves (Loop Type must be Hot Water, Two Pipe, or WLHP)"
BOILER,            0, HW-PUMP,                                                       "HW Pump", 12897, 32066, 0,  0, "Hot Water pump: if not specified, the head requirement is passed to the primary loop"
BOILER,            0, HW-DT,                                                      "HW Delta T", 12182, 32066, 0,  1, "Design temp change of hot water through the boiler (used to size recirculation pump, if present)"
BOILER,            0, HW-HEAD,                                                       "HW Head", 12184, 32066, 0,  1, "Pressure drop through the boiler at the design flowrate"
BOILER,            0, HW-STATIC-HEAD,                                         "HW Static Head", 12186, 32066, 0,  2, "Static pressure drop through the boiler; use if pumping fluid at atm pressure into loop"
BOILER,            0, HW-FLOW-CTRL,                                          "HW Flow Control", 12180, 32066, 0,  0, "Constant Flow = independent of the load; Variable Flow = varies linearly with load"
BOILER,            0, HW-MIN-FLOW,                                           "HW Minimum Flow", 12187, 32066, 0,  1, "Min flow rate through the boiler; used only if Hot Water Flow Control = Variable Flow"
BOILER,            0, HW-MAX-FLOW,                                           "HW Maximum Flow", 12121, 32066, 0,  1, "Max flow rate through the boiler; used only if Hot Water Flow Control = Variable Flow"
BOILER,            0, *HW-ISOLATION,                                            "HW Isolation", 12188, 32066, 0,  0, "Whether the boiler has an isolation valve that closes when the boiler is not being used"
BOILER,            0, COST-DATA,                                                        "Cost", 12795, 32066, 0,  0, "Name of a set of Materials Costs, which specifies first costs, maintenance costs, etc."
BOILER,            0, EQUIPMENT-REPORT,                                                     "",  1551, 32066, 0,  2, "Whether or not a PS-H report is created for this boiler"
BOILER,            0, PICTURE,                                                              "",     0, 32066, 0,  2, ""
BOILER,            0, DRAWING,                                                              "",     0, 32066, 0,  2, ""
DW-HEATER,         0, TYPE,                                                             "Type", 13187, 32067, 0,  0, "Type of DHW heater: gas, electric or heat pump"
DW-HEATER,         0, TANK-VOLUME,                                                          "", 13189, 32067, 0,  2, "Volume of the DHW storage tank"
DW-HEATER,         0, CAPACITY,                                                             "",   802, 32067, 0,  2, "Nominal (rated) heating capacity of the water heater (in millions of BTU's per hour)"
DW-HEATER,         0, CAPACITY-RATIO,                                                       "",   803, 32067, 0,  2, "Capacity as fraction of max heating load (used only if PowerDOE sizes the water heater)"
DW-HEATER,         0, CAPACITY-FT,                                                          "", 13201, 32067, 0,  2, "Bi-Quadratic Curve: Capacity as a function of the temp of entering and exiting water"
DW-HEATER,         0, ELEC-INPUT-RATIO,                                                     "",   805, 32067, 0,  2, "Dimensionless ratio of electric input power to nominal capacity (at rated conditions)"
DW-HEATER,         0, EIR-FT,                                                               "", 13199, 32067, 0,  2, "Quadratic Curve Fit: Electric Input Ratio as a function of temperature entering & leaving water"
DW-HEATER,         0, EIR-FPLR,                    "Electric Input Ratio = f(Part Load Ratio)", 13198, 32067, 0,  0, "Quadratic Curve Fit: Electric Input Ratio as a function of the part load ratio"
DW-HEATER,         0, HEAT-INPUT-RATIO,                                                     "",   804, 32067, 0,  2, "Dimensionless ratio of fuel heat input to DHW heater output at full load (at rated conditions)"
DW-HEATER,         0, HIR-FT,                                                               "", 13197, 32067, 0,  0, "Bi-Quadratic Curve: the HIR as a function of the temp of entering and exiting water"
DW-HEATER,         0, HIR-FPLR,                        "Heat Input Ratio = f(Part Load Ratio)", 13195, 32067, 0,  0, "Quadratic Curve Fit: Heat Input Ratio as a function of the part load ratio"
DW-HEATER,         0, TANK-UA,                                                              "", 12757, 32067, 0,  2, "Thermal conductivity of the DHW storage tank"
DW-HEATER,         0, LOCATION,                                                             "",   801, 32067, 0,  2, "For DHW storage tank: Outdoors=heat lost to environment; Zone=heat lost to the DHW Zone"
DW-HEATER,         0, ZONE-NAME,                                                        "Zone", 12755, 32067, 0,  2, "Name of zone that the DHW storage tank is in)"
DW-HEATER,         0, AUX-KW,                                                               "",   806, 32067, 0,  2, "Auxiliary electric power consumption of the DHW water heater (e.g., control panels)"
DW-HEATER,         0, AUX-MODE,                                                             "", 13209, 32067, 0,  2, "Always=all hours;When On=If heater on;When Off=if heater off;Scheduled=use Aux Schedule"
DW-HEATER,         0, AUX-SCHEDULE,                                             "Aux Schedule", 13210, 32067, 0,  2, "Schedule for Auxiliary Power consumption (set Auxiliary Mode to Scheduled to activate this)"
DW-HEATER,         0, AUX-METER,                                                            "", 13241, 32067, 0,  2, "Name of the Electric Meter that tallies the electricity consumption of this heater's auxiliaries"
DW-HEATER,         0, ELEC-METER,                                                           "",   809, 32067, 0,  2, "Name of the Electric Meter that tallies the electricity consumption of this DHW heater"
DW-HEATER,         0, FUEL-METER,                                                           "",   808, 32067, 0,  2, "Name of the Fuel Meter that tallies the fuel consumption of this DHW heater"
DW-HEATER,         0, AQUASTAT-SETPT-T,                                                     "",   808, 32067, 0,  2, "DHW heater tank temperature setpoint"
DW-HEATER,         0, DHW-LOOP,                                                     "DHW Loop",   800, 32067, 0,  2, "Name of the Domestic Hot Water loop that this heater serves"
DW-HEATER,         0, DHW-PUMP,                                           "Recirculation Pump", 12751, 32067, 0,  2, "Hot Water pump: if not specified, the head requirement is passed to the primary loop"
DW-HEATER,         0, DHW-HEAD,                                                             "", 12752, 32067, 0,  2, "Pressure drop through the DHW heater at the design flowrate"
DW-HEATER,         0, DHW-STATIC-HEAD,                                                      "", 12756, 32067, 0,  2, "Static pressure drop through the heater; use if pumping fluid at atm pressure into loop"
DW-HEATER,         0, DW-MIN-FLOW,                                                          "", 13206, 32067, 0,  2, "Minimum flow rate through the DHW heater"
DW-HEATER,         0, DW-MAX-FLOW,                                                          "", 13207, 32067, 0,  2, "Maximum flow rate through the DHW heater"
DW-HEATER,         0, HP-SUPP-CAPACITY,                                                     "", 13185, 32067, 0,  2, "The capacity of the backup immersion heater"
DW-HEATER,         0, MAX-HP-TANK-T,                                                        "", 13194, 32067, 0,  2, "The maximum water temperature that the heat pump can provide"
DW-HEATER,         0, MAX-HTREC-RATE,                                                       "",   807,   696, 0,  2, "Maximum hourly rate at which heat can be recovered by the DHW Heater"
DW-HEATER,         0, COST-DATA,                                                            "", 12750, 32067, 0,  2, "Name of a set of Materials Costs, which specifies first costs, maintenance costs, etc."
DW-HEATER,         0, EQUIPMENT-REPORT,                                                     "",   898, 32067, 0,  2, "Whether or not a PS-H report is created for this DHW heater"
DW-HEATER,         0, PICTURE,                                                              "",     0, 32067, 0,  2, ""
DW-HEATER,         0, DRAWING,                                                              "",     0, 32067, 0,  2, ""
HEAT-REJECTION,    0, TYPE,                                                             "Type", 12900, 32068, 0,  0, "Open Tower=Direct evap cool;Open Tower & HX=heat exchanger transfers heat between fluids"
HEAT-REJECTION,    0, CAPACITY,                                                     "Capacity", 12190, 32068, 0,  1, "Nominal (rated) cooling capacity in MBTU/hr (e.g., 100 ton = 1.2 MBTU/hr)"
HEAT-REJECTION,    0, CAPACITY-RATIO,                                         "Capacity Ratio", 12201, 32068, 0,  1, "Capacity as fraction of max cooling load (used only if PowerDOE sizes the tower)"
HEAT-REJECTION,    0, NUMBER-OF-CELLS,                                       "Number of Cells", 12202, 32068, 0,  0, "Total number of cells in the cooling tower"
HEAT-REJECTION,    0, ELEC-INPUT-RATIO,                                 "Electric Input Ratio", 12206, 32068, 0,  2, "Dimensionless ratio of electric input power to nominal tower capacity"
HEAT-REJECTION,    0, FAN-KW/CELL,                                           "Fan kW per Cell", 12207, 32068, 0,  1, "Power consumption of the cooling tower fan (per cell), at the rated flow rate"
HEAT-REJECTION,    0, CAPACITY-CTRL,                                        "Capacity Control", 12122, 32068, 0,  0, "1SpdFan=cycles on/off;Fluid Bypass=via valve;2SpdFan=cycles off/low/on;Var. Fan modulates"
HEAT-REJECTION,    0, CELL-CTRL,                                                "Cell Control", 12131, 32068, 0,  0, "Min Cells=maximise flow through each cell;Max Cells =minimize flow through each cell"
HEAT-REJECTION,    0, CAP-FAPP&WB,                                                          "", 12530, 32068, 0,  0, "Bi-Quadratic Equation used to determine Capacity - use of the default is highly recommended"
HEAT-REJECTION,    0, CAP-FRNG&WB,                                                          "", 14279, 32068, 0,  0, "Bi-Quadratic Equation used to determine Capacity - use of the default is highly recommended"
HEAT-REJECTION,    0, MAX-RANGE,                                                            "", 14281, 32068, 0,  2, "Max allowable value of Design Range for which the Capacity f(range, wetbulb) curve is valid"
HEAT-REJECTION,    0, CAP-FAIRFLOW,                                                         "", 14533, 32068, 0,  2, "Quadratic eqn: flow capacity as a function of the airflow through the heat rejector"
HEAT-REJECTION,    0, FAN-KW-FSPEED,                                                        "", 14278, 32068, 0,  2, "Cubic eqn: fan power consumption as a function of fan speed"
HEAT-REJECTION,    0, FAN-KW-FDAMPER,                                                       "", 12529, 32068, 0,  2, "Cubic eqn: fan power consumption as a function of fan air flow rate"
HEAT-REJECTION,    0, PAN-LOSS,                                                             "", 14304, 32068, 0,  2, "The thermal loss of the pan at the design pan fluid T, ambient T and wind speed"
HEAT-REJECTION,    0, PAN-LOSS-RATIO,                                                       "", 14305, 32068, 0,  2, "Ratio of the design pan losses to the design heat rejection capacity (at CTI rating conditions)"
HEAT-REJECTION,    0, PAN-FLUID-T,                                                          "", 14306, 32068, 0,  2, "Temperature of the fluid in the pan that corresponds to the design Pan Loss"
HEAT-REJECTION,    0, PAN-AMBIENT-T,                                                        "", 14307, 32068, 0,  2, "Ambient air temperature that corresponds to the design Pan Loss"
HEAT-REJECTION,    0, PAN-WINDSPEED,                                                        "", 14308, 32068, 0,  2, "The (design) wind speed that corresponds to the design Pan Loss"
HEAT-REJECTION,    0, PAN-HEATER-TYPE,                                                      "", 14303, 32068, 0,  2, "Type of pan heater used for freeze protection when the heat rejection device is not operating"
HEAT-REJECTION,    0, PAN-HEATER-LOOP,                                       "Pan Heater Loop", 14309, 32068, 0,  2, "Name of a heating-type loop used for freeze protection"
HEAT-REJECTION,    0, PAN-HEATER-HEAD,                                                      "", 14311, 32068, 0,  2, "The friction loss of the pan heater coil"
HEAT-REJECTION,    0, PAN-VALVE-TYPE,                                                       "", 14310, 32068, 0,  2, "The type of valve that modulates the flow through the pan heater coil"
HEAT-REJECTION,    0, PAN-HEATER-DT,                                                        "", 14312, 32068, 0,  2, "Design temperature drop through the pan heater coil"
HEAT-REJECTION,    0, COIL-LOSS,                                                            "", 14340, 32068, 0,  2, "Thermal loss of the fluid cooler at the winter design conditions"
HEAT-REJECTION,    0, COIL-LOSS-RATIO,                                                      "", 14341, 32068, 0,  2, "Ratio of design fluid cooler losses to design heat rejection capacity (at CTI rating conditions)"
HEAT-REJECTION,    0, COIL-FLUID-T,                                                         "", 14342, 32068, 0,  2, "Design temperature of fluid in the coil (corresponding to the design Coil Loss)"
HEAT-REJECTION,    0, COIL-AMBIENT-T,                                                       "", 14343, 32068, 0,  2, "Design ambient air temperature (corresponding to the design Coil Loss)"
HEAT-REJECTION,    0, COIL-WINDSPEED,                                                       "", 14344, 32068, 0,  2, "Design wind speed (corresponding to the design Coil Loss)"
HEAT-REJECTION,    0, WET-COIL-SCH,                                                         "", 14335, 32068, 0,  2, "Name of an On\Off\Temp schedule that defines when the coil in the fluid cooler runs wet"
HEAT-REJECTION,    0, DRY-INLET-DT,                                                         "", 14274, 32068, 0,  2, "Delta T across the dry coil that is necessary to achieve the design heat rejection capacity"
HEAT-REJECTION,    0, DRY-AIR-RATIO,                                                        "", 14336, 32068, 0,  2, "The increase in airflow when running with a dry coil (applies to Fluid Coolers only)"
HEAT-REJECTION,    0, DRY-HX,                                                    "Dry Coil HX", 14273, 32068, 0,  2, "Name of HX when running dry"
HEAT-REJECTION,    0, AIR-TO-FLUID-FLO,                                                     "", 14334, 32068, 0,  2, "Ratio of air flow through the cooler to fluid flow (at design conditions)"
HEAT-REJECTION,    0, HX-DT,                                           "Heat Exchange Delta T", 12208, 32068, 0,  1, "Delta T between loop fluid leaving heat exchanger, and tower fluid entering heat exchanger"
HEAT-REJECTION,    0, HX-HEAD,                                         "Heat Exchange Delta P", 14268, 32068, 0,  1, "Pressure drop through the heat exchanger"
HEAT-REJECTION,    0, DESIGN-RANGE,                                             "Design Range", 12212, 32068, 0,  1, "Fluid DT through cooling tower; used to calc design flowrate; applies to Open Tower & HX only"
HEAT-REJECTION,    0, DESIGN-APPROACH,                                       "Design Approach", 12211, 32068, 0,  1, "Difference between temperature of fluid leaving tower, and ambient air wetbulb temperature"
HEAT-REJECTION,    0, DESIGN-WETBULB,                                         "Design Wetbulb", 12210, 32068, 0,  1, "The wet-bulb temperatureused in the heat rejector design calculations"
HEAT-REJECTION,    0, MAX-FLOW/CELL,                                       "Cell Maximum Flow", 12465, 32068, 0,  2, "Largest allowable ratio of actual flow rate to design flow rate (for each cell)"
HEAT-REJECTION,    0, MIN-FLOW/CELL,                                       "Cell Minimum Flow", 12466, 32068, 0,  2, "Smallest allowable ratio of actual flow rate to design flow rate (for each cell)"
HEAT-REJECTION,    0, FAN-OFF-AIR-FLOW,                                         "Fan Off Flow", 12468, 32068, 0,  2, "Ratio of airflow through tower due to natural convection (fans off), to flow at design fan speed"
HEAT-REJECTION,    0, FAN-LOW-AIR-FLOW,                                         "Fan Low Flow", 12474, 32068, 0,  2, "For 2 speed fans: ratio of power consumption when fans at low speed to that at design speed"
HEAT-REJECTION,    0, FAN-LOW-KW,                                           "Fan Low Electric", 12476, 32068, 0,  2, "For 2 speed fans: ratio of power consumption when fans at low speed to that at design speed"
HEAT-REJECTION,    0, MIN-VFD-SPEED,                                       "Minimum Fan Speed", 12478, 32068, 0,  2, "For varaible speed fans: ratio of minimum allowable speed to nominal fan speed"
HEAT-REJECTION,    0, MIN-RESET-PLR,                                                        "", 14276, 32068, 0,  2, "Part load ratio corresponding to Minimum Fan Speed (below this PLR, fan doesn't modulate)"
HEAT-REJECTION,    0, MAX-RESET-SPEED,                                                      "", 14277, 32068, 0,  2, "Max allowable speed of a variable-speed cooling tower fan during Load Reset operation"
HEAT-REJECTION,    0, AUX-KW,                                                   "Auxiliary kW", 12706, 32068, 0,  1, "Auxiliary electric power consumption of the cooling tower (e.g., control panels)"
HEAT-REJECTION,    0, AUX-MODE,                                               "Auxiliary Mode", 12901, 32068, 0,  0, "Always=all hours;When On=If tower on;When Off=if tower off;Scheduled=use Aux Schedule"
HEAT-REJECTION,    0, AUX-SCHEDULE,                                       "Auxiliary Schedule", 12902, 32068, 0,  0, "Schedule for Auxiliary Power consumption (set Auxiliary Mode to Scheduled to activate this)"
HEAT-REJECTION,    0, AUX-METER,                                             "Auxiliary Meter", 12804, 32068, 0,  0, "Name of the Electric Meter that tallies the electricity consumption of this tower's auxiliaries"
HEAT-REJECTION,    0, ELEC-METER,                                             "Electric Meter", 12209, 32068, 0,  0, "Name of the Electric Meter that tallies the electric consumption of this tower"
HEAT-REJECTION,    0, CW-LOOP,                                                       "CW Loop", 19133, 32068, 0,  0, "Name of the condenser water (or heat pump) Loop that this Cooling Tower serves"
HEAT-REJECTION,    0, CW-PUMP,                                                       "CW Pump", 12532, 32068, 0,  0, "Name of Pump that serves the tower fluid; required if tower Type is Open Tower & HX"
HEAT-REJECTION,    0, CW-DT,                                                      "CW Delta T", 12563, 32068, 0,  1, "Design temperature drop of the fluid through the tower"
HEAT-REJECTION,    0, CW-HEAD,                                                       "CW Head", 12564, 32068, 0,  1, "Design delta P through tower due to friction (not including any Static Head); for HX towers only"
HEAT-REJECTION,    0, CW-STATIC-HEAD,                                         "CW Static Head", 12565, 32068, 0,  1, "Tower static head: equal to distance between spray nozzles and water level in the sump"
HEAT-REJECTION,    0, CW-FLOW-CTRL,                                          "CW Flow Control", 12551, 32068, 0,  0, "Applies only if there is a condenser water pump; otherwise defaults to Loop Flow Control"
HEAT-REJECTION,    0, CW-MIN-FLOW,                                           "CW Minimum Flow", 12585, 32068, 0,  1, "Minimum fluid flow rate through the tower; below this, tower pump cycles on & off"
HEAT-REJECTION,    0, *CW-ISOLATION,                                            "CW Isolation", 12590, 32068, 0,  0, "Whether an isolation valve exists to shunt the fluid flow; if no tower Pump, fluid always flows"
HEAT-REJECTION,    0, CW-HX,                                               "CW Heat Exchanger", 14269, 32068, 0,  2, "Max allowable speed of a variable-speed cooling tower fan during Load Reset operation"
HEAT-REJECTION,    0, SPRAY-KW/CELL,                                                        "", 14270, 32068, 0,  2, "The power consumption of the spray pump (per cell)"
HEAT-REJECTION,    0, SPRAY-KW/FLOW,                                                        "", 14271, 32068, 0,  2, "Power consumption of spray pump, per flow (at the design flow and the CTI rating conditions)"
HEAT-REJECTION,    0, SPRAY-PUMP-CTRL,                                                      "", 14272, 32068, 0,  2, "The control method that regulates the operation of the spray pump and the fan"
HEAT-REJECTION,    0, COST-DATA,                                                        "Cost", 12240, 32068, 0,  0, "Name of a set of Materials Costs, which specifies first costs, maintenance costs, etc."
HEAT-REJECTION,    0, EQUIPMENT-REPORT,                                                     "",  1555, 32068, 0,  2, "Whether or not a PS-H report is created for this tower"
HEAT-REJECTION,    0, PICTURE,                                                              "",     0, 32068, 0,  2, ""
HEAT-REJECTION,    0, DRAWING,                                                              "",     0, 32068, 0,  2, ""
; SAC 3/30/03 - Modified some decimal precision values to be consistent w/ screen mods from MSA
; SAC 10/25/03 - Updated and added various items to be consistent w/ new PV algorithm improvements
PV-MODULE,         0, TYPE,                                                             "Type",     0,     0, 0,  0, "Photovoltaic module type"
PV-MODULE,         0, SIM-ALGORITHM,                                                        "",     0,     0, 0,  0, "Simulation algorithm"
PV-MODULE,         0, HEIGHT,                                                         "Height",     0,     0, 0,  1, "Height of photovoltaic module"
PV-MODULE,         0, WIDTH,                                                           "Width",     0,     0, 0,  1, "Width of photovoltaic module"
PV-MODULE,         0, GLAZING-TYPE,                                                         "",     0,     0, 0,  0, "GLAZING-TYPE"
PV-MODULE,         0, IRRADIANCE-FAM,  "Irradiance f(effective air mass between module & sun)",     0,     0, 0,  0, "Irradiance as a function of the effective air mass between module and the sun"
PV-MODULE,         0, IRRADIANCE-FAOI,                "Irradiance f(sun's angle of incidence)",     0,     0, 0,  0, "Irradiance as a function of the sun's angle of incidence"
PV-MODULE,         0, CELL-BACK-DT,                                   "Cell - Back Surface dT",     0,     0, 0,  1, "Differential between cell temperature and back surface temperature"
PV-MODULE,         0, VOLTS-OPEN-CKT,                              "Open Circuit Voltage, Voc",     0,     0, 0,  2, "Open circuit voltage at 1000 W/m2, 25°C and 1.5 air mass"
PV-MODULE,         0, VOLTS/T-OPEN-CKT,                           "Voc Temperature Coef, BVoc",     0,     0, 0,  4, "The rate at which Voc changes with temperature"
PV-MODULE,         0, AMPS-SHORT-CKT,                             "Short Circuit Current, Isc",     0,     0, 0,  2, "Short circuit current at 1000 W/m2, 25°C and 1.5 air mass"
PV-MODULE,         0, AMPS/T-SHORT-CKT,                           "Isc Temperature Coef, aIsc",     0,     0, 0,  5, "The rate at which Isc changes with temperature"
PV-MODULE,         0, VOLTS-MAX-PWR,                                  "Max Power Voltage, Vmp",     0,     0, 0,  2, "Maximum power voltage at 1000 W/m2, 25°C and 1.5 air mass"
PV-MODULE,         0, VOLTS/T-MAX-PWR,                            "Vmp Temperature Coef, BVmp",     0,     0, 0,  4, "The rate at which Vmp changes with temperature"
PV-MODULE,         0, VOLTS/E-MAX-PWR,                            "Vmp Irradiance Coef, mBVmp",     0,     0, 0,  4, "The rate at which Vmp changes with irradiance"
PV-MODULE,         0, AMPS-MAX-PWR,                                   "Max Power Current, Imp",     0,     0, 0,  2, "Maximum power current at 1000 W/m2, 25°C and 1.5 air mass"
PV-MODULE,         0, AMPS/T-MAX-PWR,                             "Imp Temperature Coef, aImp",     0,     0, 0,  4, "The rate at which Imp changes with temperature"
PV-MODULE,         0, CELLS-SERIES,                                "Number of Cells in Series",     0,     0, 0,  0, "CELLS-SERIES"
PV-MODULE,         0, C0,                                    "C0 Coefficient of King Equation",     0,     0, 0,  2, "C0"
PV-MODULE,         0, C1,                                    "C1 Coefficient of King Equation",     0,     0, 0,  2, "C1"
PV-MODULE,         0, C2,                                    "C2 Coefficient of King Equation",     0,     0, 0,  2, "C2"
PV-MODULE,         0, C3,                                    "C3 Coefficient of King Equation",     0,     0, 0,  2, "C3"
PV-MODULE,         0, FDIODE,                                 "Diode-Effect Coef. of King Eq.",     0,     0, 0,  2, "FDIODE"
PV-MODULE,         0, A0-A4,                                             "Air Mass Polynomial",     0,     0, 0, 10, "4th-order polynomial modifying irradiance as a function of air mass"
PV-MODULE,         0, B0-B5,                                       "Incident Angle Polynomial",     0,     0, 0, 10, "5th-order polynomial modifying irradiance transmission for incident angle"
PV-MODULE,         0, COST-DATA,                                                            "",     0,     0, 0,  0, "COST-DATA"
PV-MODULE,         0, EQUIPMENT-REPORT,                                                     "",     0,     0, 0,  0, "EQUIPMENT-REPORT"
PV-MODULE,         0, PICTURE,                                                              "",     0,     0, 0,  0, "PICTURE"
PV-MODULE,         0, DRAWING,                                                              "",     0,     0, 0,  0, "DRAWING"
PV-MODULE,         0, AREA,                                                                 "",     0,     0, 0,  2, "AREA"
PV-MODULE,         0, CAPACITY,                                                             "",     0,     0, 0,  5, "CAPACITY"
PV-MODULE,         0, EFFICIENCY,                                                           "",     0,     0, 0,  3, "EFFICIENCY"
PV-MODULE,         0, NOM-OPER-CELL-T,                                        "no longer used",     0,     0, 0,  1, "NOM-OPER-CELL-T"
PV-MODULE,         0, NOCT-AMBIENT,                                           "no longer used",     0,     0, 0,  1, "NOCT-AMBIENT"
PV-MODULE,         0, NOCT-IRRADIANCE,                                        "no longer used",     0,     0, 0,  1, "NOCT-IRRADIANCE"
PV-MODULE,         0, NOCT-WINDSPEED,                                         "no longer used",     0,     0, 0,  2, "NOCT-WINDSPEED"
PV-MODULE,         0, REF-IRRADIANCE,                                         "no longer used",     0,     0, 0,  1, "REF-IRRADIANCE"
; SAC 3/30/03 - Added several PV-module-related keywords and modified some decimal precision values to be consistent w/ screen mods from MSA
; SAC 10/25/03 - Updated and added various items to be consistent w/ new PV algorithm improvements
ELEC-GENERATOR,    0, TYPE,                                                             "Type", 32070, 32070, 0,  0, ""
ELEC-GENERATOR,    0, CAPACITY,                                                     "Capacity", 32070, 32070, 0,  3, "Nominal (rated) capacity"
ELEC-GENERATOR,    0, CAPACITY-FT,                                               "Capacity FT", 32070, 32070, 0,  0, "Bi-Quadratic Curve: Capacity as a function of the temp of entering and exiting water"
ELEC-GENERATOR,    0, MIN-RATIO,                                                            "", 32070, 32070, 0,  2, "Minimum generator operating ratio (a fraction of the Capacity); below this, it cycles on & off"
ELEC-GENERATOR,    0, MAX-RATIO,                                                            "", 32070, 32070, 0,  2, "Maximum allowable generator operating ratio (a fraction of the Capacity)"
ELEC-GENERATOR,    0, ELEC-INPUT-RATIO,                                                     "", 32070, 32070, 0,  4, "the ratio of direct-current input power to alternating-current output power"
ELEC-GENERATOR,    0, EIR-FPLR,                                "Elec Input Ratio f(part load)", 32070, 32070, 0,  0, "Linear or Quadratic Curve Fit: Electric Input Ratio as a function of the part load ratio"
ELEC-GENERATOR,    0, HEAT-INPUT-RATIO,                                                     "", 32070, 32070, 0,  2, "Dimensionless ratio of fuel heat input to output at full load (at rated conditions)"
ELEC-GENERATOR,    0, HIR-FT,                                            "Heat Input Ratio FT", 32070, 32070, 0,  0, "Bi-Quadratic Curve: the HIR as a function of the temp of entering and exiting water"
ELEC-GENERATOR,    0, HIR-FPLR,                                                             "", 32070, 32070, 0,  2, "Quadratic Curve Fit: Heat Input Ratio as a function of the part load ratio"
ELEC-GENERATOR,    0, START-UP-TIME,                                                        "", 32070, 32070, 0,  2, ""
ELEC-GENERATOR,    0, AUX-KW,                                                               "", 32070, 32070, 0,  3, "Auxiliary electric power consumption of the generator (e.g., control panels)"
ELEC-GENERATOR,    0, AUX-MODE,                                                             "", 32070, 32070, 0,  2, "Always=all hours;When On=If gen. on;When Off=if gen. off;Scheduled=use Aux Schedule"
ELEC-GENERATOR,    0, AUX-SCHEDULE,                                       "Auxiliary Schedule", 32070, 32070, 0,  2, "Schedule for Auxiliary Power consumption (set Auxiliary Mode to Scheduled to activate this)"
ELEC-GENERATOR,    0, AUX-METER,                                                            "", 32070, 32070, 0,  2, "Name of Electric Meter that tallies the electricity consumption of this generator's auxiliaries"
ELEC-GENERATOR,    0, ELEC-METER,                                                           "", 32070, 32070, 0,  2, "Name of the Electric Meter that tallies the electricity consumption"
ELEC-GENERATOR,    0, SURPLUS-METER,                                                        "", 32070, 32070, 0,  2, ""
ELEC-GENERATOR,    0, FUEL-METER,                                                           "", 32070, 32070, 0,  2, "Name of the Fuel Meter that tallies the fuel consumption of this generator"
ELEC-GENERATOR,    0, EXH-LOOP,                                                             "", 32070, 32070, 0,  2, ""
ELEC-GENERATOR,    0, EXH-RCVR,                                                             "", 32070, 32070, 0,  2, ""
ELEC-GENERATOR,    0, EXH-RCVR-FPLR,                                                        "", 32070, 32070, 0,  2, ""
ELEC-GENERATOR,    0, JAC-LOOP,                                                             "", 32070, 32070, 0,  2, ""
ELEC-GENERATOR,    0, JAC-RCVR,                                                             "", 32070, 32070, 0,  2, ""
ELEC-GENERATOR,    0, JAC-RCVR-FPLR,                                                        "", 32070, 32070, 0,  2, ""
ELEC-GENERATOR,    0, RCVR-TRACK-LOOP,                                                       "", 32070, 32070, 0,  2, ""
ELEC-GENERATOR,    0, CW-LOOP,                                                              "", 32070, 32070, 0,  2, "If Condenser Type=Water Cooled, CW Loop is required & must be attached to Cooling Tower"
ELEC-GENERATOR,    0, CW-DT,                                                      "CW Delta T", 32070, 32070, 0,  2, ""
ELEC-GENERATOR,    0, CW-HEAD,                                                              "", 32070, 32070, 0,  2, ""
ELEC-GENERATOR,    0, CW-FLOW-CTRL,                                                         "", 32070, 32070, 0,  2, ""
ELEC-GENERATOR,    0, STEAM-LOOP,                                                           "", 32070, 32070, 0,  2, ""
ELEC-GENERATOR,    0, STEAM-ENT-PRES,                                                       "", 32070, 32070, 0,  2, ""
ELEC-GENERATOR,    0, STEAM-SUPER-T,                                                        "", 32070, 32070, 0,  2, ""
ELEC-GENERATOR,    0, STEAM-EXH-PRES,                                                       "", 32070, 32070, 0,  2, ""
ELEC-GENERATOR,    0, STEAM-ENTH-FP&P,                                                      "", 32070, 32070, 0,  2, ""
ELEC-GENERATOR,    0, STEAM-CONDENSATE,                                                     "", 32070, 32070, 0,  2, ""
ELEC-GENERATOR,    0, MECH-EFF,                                                             "", 32070, 32070, 0,  2, ""
ELEC-GENERATOR,    0, NUM-INVERTERS,                                     "Number of Inverters", 32070, 32070, 0,  0, "the number of inverters that operate in parallel"
ELEC-GENERATOR,    0, INVERTER-CTRL,                                        "Inverter Control", 32070, 32070, 0,  0, "the staging control mechanism as the load varies (only when more than one inverter is present)"
ELEC-GENERATOR,    0, MIN-OPER-VOLTS,                                    "Minimum Input Volts", 32070, 32070, 0,  2, "the minimim input voltage below which the inverter will shut down"
ELEC-GENERATOR,    0, MIN-TRACK-VOLTS,                                "Minimun Tracking Volts", 32070, 32070, 0,  2, "the minimum input tracking voltage at which the inverter can operate efficiently"
ELEC-GENERATOR,    0, MAX-TRACK-VOLTS,                                "Maximum Tracking Volts", 32070, 32070, 0,  2, "the maximum input tracking voltage at which the inverter can operate efficiently"
ELEC-GENERATOR,    0, PV-MODULE,                                                   "PV Module", 32070, 32070, 0,  0, "the photovoltaic module that comprises the array"
ELEC-GENERATOR,    0, MODULES-SERIES,                               "Number of Series Modules", 32070, 32070, 0,  0, "the number of photovoltaic modules wired in series"
ELEC-GENERATOR,    0, MODULES-PARALLEL,                           "Number of Parallel Modules", 32070, 32070, 0,  0, "the number of photovoltaic modules wired in parallel"
ELEC-GENERATOR,    0, MOUNT-TYPE,                                                 "Mount Type", 32070, 32070, 0,  0, "the mounting configuration of the photovoltaic array"
ELEC-GENERATOR,    0, BUILDING-SHADE,                                         "Building Shade", 32070, 32070, 0,  0, "the shading surface on which the photovoltaic module(s) are mounted"
ELEC-GENERATOR,    0, EXTERIOR-WALL,                                           "Exterior Wall", 32070, 32070, 0,  0, "the exterior wall surface on which the photovoltaic module(s) are mounted"
ELEC-GENERATOR,    0, EXTERIOR-ROOF,                                                    "Roof", 32070, 32070, 0,  0, "the roof surface on which the photovoltaic module(s) are mounted"
ELEC-GENERATOR,    0, ARRAY-FRACTION,                                         "Array Fraction", 32070, 32070, 0,  3, "the fraction of the shade, wall or roof surface that is covered by photovoltaic modules"
ELEC-GENERATOR,    0, MOUNT-HEIGHT,                                             "Mount Height", 32070, 32070, 0,  3, "the average distance between the back of the array and the surface to which it is mounted"
ELEC-GENERATOR,    0, MOUNT-AZIMUTH,                                           "Mount Azimuth", 32070, 32070, 0,  2, "the azimuth of the array rack, where 180° is due south, relative to the building coordinate system"
ELEC-GENERATOR,    0, MOUNT-TILT,                                                 "Mount Tilt", 32070, 32070, 0,  2, "the tilt of the array rack, where 0° is horizontal (surface outward normal pointing straight up)"
ELEC-GENERATOR,    0, GND-REFLECTANCE,                                    "Ground Reflectance", 32070, 32070, 0,  3, "the ground reflectance on the array rack"
ELEC-GENERATOR,    0, WIND-COEF-A,                                      "Wind Coefficient 'A'", 32070, 32070, 0,  4, "Coefficient determining upper temperature limit at low wind speeds"
ELEC-GENERATOR,    0, WIND-COEF-B,                                      "Wind Coefficient 'B'", 32070, 32070, 0,  4, "Coefficient determining the rate that module T drops as wind increases"
ELEC-GENERATOR,    0, COST-DATA,                                                            "", 32070, 32070, 0,  2, "Name of a set of Materials Costs, which specifies first costs, maintenance costs, etc."
ELEC-GENERATOR,    0, EQUIPMENT-REPORT,                                                     "", 32070, 32070, 0,  2, "Whether or not a PS-H report is created for this generator"
ELEC-GENERATOR,    0, PICTURE,                                                              "", 32070, 32070, 0,  2, ""
ELEC-GENERATOR,    0, DRAWING,                                                              "", 32070, 32070, 0,  2, ""
ELEC-GENERATOR,    0, WIND-COEF,                           "Wind Coefficient - no longer used", 32070, 32070, 0,  4, "the wind coefficient for the photovoltaic array"
ELEC-GENERATOR,    0, OFFSET-T,                          "Offset Temperature - no longer used", 32070, 32070, 0,  2, "the offset temperature for the photovoltaic array"
ELEC-GENERATOR,    0, CELL-T-COEF,                   "Cell Temperature Coeff - no longer used", 32070, 32070, 0,  4, "the coefficient that modifies the hourly operating cell temperature as a function of the irradiance, ambient temperature, and wind speed"
THERMAL-STORAGE,   1, TYPE,                                                             "Type", 12075, 32071, 0,  0, "Whether a hot or cold water storage tank"
THERMAL-STORAGE,   1, CAPACITY,                                                             "", 12876, 32071, 0,  2, "Net thermal storage capacity of the tank"
THERMAL-STORAGE,   1, CAPACITY-RATIO,                                                       "", 12944, 32071, 0,  2, "Tank is sized to meet this multiplied by 1 hour's design loop load (if Capacity not specified)"
THERMAL-STORAGE,   1, BASE-T,                                                               "", 12945, 32071, 0,  2, "When tank reaches this temperature, no more storage is possible"
THERMAL-STORAGE,   1, T-RANGE,                                                              "", 12946, 32071, 0,  2, "Temperature range between the fully charged and fully discharged state"
THERMAL-STORAGE,   1, CHRG-LOOP,                                                 "Charge Loop", 12528, 32071, 0,  0, "Name of the loop that charges the tank (more than one storage tank per loop is allowed)"
THERMAL-STORAGE,   1, CHRG-T,                                                               "", 12947, 32071, 0,  2, "Temperature at which the tank is fully charged (may force loop to exceed its setpoint temp)"
THERMAL-STORAGE,   1, CHRG-T-FHOURS,                                                        "", 14050, 32071, 0,  2, "Quadratic Curve Fit: charge temp as function of length of time tank has been charged"
THERMAL-STORAGE,   1, MAX-CHRG-RATE,                                                        "", 12666, 32071, 0,  2, "Maximum rate at which the storage tank can charge"
THERMAL-STORAGE,   1, CHRG-RATE-FHOURS,                                                     "", 14049, 32071, 0,  2, "Quadratic Curve Fit: charge temp as function of length of time tank has been charging"
THERMAL-STORAGE,   1, CHRG-SCH,                                              "Charge Schedule", 12079, 32071, 0,  2, "Name of an on/off schedule that defines when the tank is allowed to be charged"
THERMAL-STORAGE,   1, DELAY-CHRG-HOUR,                                                      "", 13357, 32071, 0,  2, "The latest hour (while Charge Schedule is ON) by which the tank should be fully charged"
THERMAL-STORAGE,   1, INITIAL-CHRG,                                                         "", 13358, 32071, 0,  2, "Fraction of the tank's Capacity that is stored at the start of the simulation"
THERMAL-STORAGE,   1, DCHRG-LOOP,                                             "Discharge Loop", 12076, 32071, 0,  0, "Name of the loop the tank discharges to (only one tank can dicharge to any particular loop)"
THERMAL-STORAGE,   1, MAX-DCHRG-RATE,                                                       "", 12078, 32071, 0,  2, "maximum rate at which the storage tank can discharge (i.e., supply the loop)"
THERMAL-STORAGE,   1, DCHRG-RATE-FHOUR,                                                     "", 14021, 32071, 0,  2, "Quadratic Curve Fit: discharge rate as function of length of time tank has been discharging"
THERMAL-STORAGE,   1, LOSS-COEFICIENT,                                                      "", 13268, 13268, 0,  2, "Thermal losses of the tank, per degree temperature difference between tank and its Location"
THERMAL-STORAGE,   1, LOCATION,                                                             "", 12793, 32071, 0,  2, "Outdoor=Losses based on ouside air drybulb; Zone=Losses based on temp of Zone Name"
THERMAL-STORAGE,   1, ZONE-NAME,                                                            "", 12874, 32071, 0,  2, "Name of the space the storage tank is in (used only if Location = Zone)"
THERMAL-STORAGE,   1, FREEZE-T,                                                             "", 13681, 32071, 0,  2, "Temperature at which the tank storage medium freezes"
THERMAL-STORAGE,   1, FREEZE-LOOP,                                               "Freeze Loop", 19142, 32071, 0,  2, "Name of Hot Water or Two Pipe loop that heats a Cold Water Tank to prevent freezing"
THERMAL-STORAGE,   1, AUX-KW,                                                               "", 13033, 32071, 0,  2, "Auxiliary electric power consumption of the thermal storage device (e.g., control panels)"
THERMAL-STORAGE,   1, AUX-MODE,                                                             "", 13057, 32071, 0,  2, "Always=all hours;When On=If on;When Off=if off;Scheduled=use Aux Schedule"
THERMAL-STORAGE,   1, AUX-SCHEDULE,                                       "Auxiliary Schedule", 13037, 32071, 0,  2, "Schedule for Auxiliary Power consumption (set Auxiliary Mode to Scheduled to activate this)"
THERMAL-STORAGE,   1, AUX-METER,                                                            "", 13062, 32071, 0,  2, "Name of the Electric Meter that tallies the electricity consumption of the auxiliaries"
THERMAL-STORAGE,   1, COST-DATA,                                                            "", 12077, 32071, 0,  2, "Name of a set of Materials Costs, which specifies first costs, maintenance costs, etc."
THERMAL-STORAGE,   1, EQUIPMENT-REPORT,                                                     "",     0, 32071, 0,  2, "Whether or not a PS-H report is created for this thermal storage device"
THERMAL-STORAGE,   1, PICTURE,                                                              "",     0, 32071, 0,  2, "Temperature range between the fully charged and fully discharged state"
THERMAL-STORAGE,   1, DRAWING,                                                              "",     0, 32071, 0,  2, ""
THERMAL-STORAGE,   2, TYPE,                                                             "Type", 12075, 32071, 0,  0, "Whether a hot or cold water storage tank"
THERMAL-STORAGE,   2, CAPACITY,                                                             "", 12876, 32071, 0,  2, "Net thermal storage capacity of the tank"
THERMAL-STORAGE,   2, CAPACITY-RATIO,                                                       "", 12944, 32071, 0,  2, "Tank is sized to meet this multiplied by 1 hour's design loop load (if Capacity not specified)"
THERMAL-STORAGE,   2, BASE-T,                                                               "", 12945, 32071, 0,  2, "When tank reaches this temperature, no more storage is possible"
THERMAL-STORAGE,   2, T-RANGE,                                                              "", 12946, 32071, 0,  2, "Temperature range between the fully charged and fully discharged state"
THERMAL-STORAGE,   2, CHRG-LOOP,                                                 "Charge Loop", 12528, 32071, 0,  0, "Name of the loop that charges the tank (more than one storage tank per loop is allowed)"
THERMAL-STORAGE,   2, CHRG-T,                                                               "", 12947, 32071, 0,  2, "Temperature at which the tank is fully charged (may force loop to exceed its setpoint temp)"
THERMAL-STORAGE,   2, CHRG-T-FHOURS,                                                        "", 14050, 32071, 0,  2, "Quadratic Curve Fit: charge temp as function of length of time tank has been charged"
THERMAL-STORAGE,   2, MAX-CHRG-RATE,                                                        "", 12666, 32071, 0,  2, "Maximum rate at which the storage tank can charge"
THERMAL-STORAGE,   2, CHRG-RATE-FHOURS,                                                     "", 14049, 32071, 0,  2, "Quadratic Curve Fit: charge rate as function of length of time tank has been charging"
THERMAL-STORAGE,   2, CHRG-SCH,                                              "Charge Schedule", 12079, 32071, 0,  2, "Name of an on/off schedule that defines when the tank is allowed to be charged"
THERMAL-STORAGE,   2, DELAY-CHRG-HOUR,                                                      "", 13357, 32071, 0,  2, "The latest hour (while Charge Schedule is ON) by which the tank should be fully charged"
THERMAL-STORAGE,   2, INITIAL-CHRG,                                                         "", 13358, 32071, 0,  2, "Fraction of the tank's Capacity that is stored at the start of the simulation"
THERMAL-STORAGE,   2, DCHRG-LOOP,                                             "Discharge Loop", 12076, 32071, 0,  0, "Name of the loop the tank discharges to (only one tank can dicharge to any particular loop)"
THERMAL-STORAGE,   2, MAX-DCHRG-RATE,                                                       "", 12078, 32071, 0,  2, "maximum rate at which the storage tank can discharge (i.e., supply the loop)"
THERMAL-STORAGE,   2, DCHRG-RATE-FHOUR,                                                     "", 14021, 32071, 0,  2, "Quadratic Curve Fit: discharge rate as function of length of time tank has been discharging"
THERMAL-STORAGE,   2, LOSS-COEFICIENT,                                                      "", 13268, 32071, 0,  2, "Thermal losses of the tank, per degree temperature difference between tank and its Location"
THERMAL-STORAGE,   2, LOCATION,                                                             "", 12793, 32071, 0,  2, "Outdoor=Losses based on ouside air drybulb; Zone=Losses based on temp of Zone Name"
THERMAL-STORAGE,   2, ZONE-NAME,                                                            "", 12874, 32071, 0,  2, "Name of the space the storage tank is in (used only if Location = Zone)"
THERMAL-STORAGE,   2, FREEZE-T,                                                             "", 13681, 32071, 0,  2, "Temperature at which the tank storage medium freezes"
THERMAL-STORAGE,   2, AUX-KW,                                                               "", 13033, 32071, 0,  2, "Auxiliary electric power consumption of the thermal storage device (e.g., control panels)"
THERMAL-STORAGE,   2, AUX-MODE,                                                             "", 13057, 32071, 0,  2, "Always=all hours;When On=If on;When Off=if off;Scheduled=use Aux Schedule"
THERMAL-STORAGE,   2, AUX-SCHEDULE,                                       "Auxiliary Schedule", 13037, 32071, 0,  2, "Schedule for Auxiliary Power consumption (set Auxiliary Mode to Scheduled to activate this)"
THERMAL-STORAGE,   2, AUX-METER,                                                            "", 13062, 32071, 0,  2, "Name of the Electric Meter that tallies the electricity consumption of the auxiliaries"
THERMAL-STORAGE,   2, COST-DATA,                                                            "", 12077, 32071, 0,  2, "Name of a set of Materials Costs, which specifies first costs, maintenance costs, etc."
THERMAL-STORAGE,   2, EQUIPMENT-REPORT,                                                     "",     0, 32071, 0,  2, "Whether or not a PS-H report is created for this thermal storage device"
THERMAL-STORAGE,   2, PICTURE,                                                              "",     0, 32071, 0,  2, ""
THERMAL-STORAGE,   2, DRAWING,                                                              "",     0, 32071, 0,  2, ""
HEAT-EXCHANGER,    1, TYPE,                                                             "Type", 14315, 32072, 0,  2, "The type of heat exchanger (defines both fluid types)"
HEAT-EXCHANGER,    1, CONFIGURATION,                                                        "", 14316, 32072, 0,  2, "Configuration of the heat exchanger (default varies according to Type of HX)"
HEAT-EXCHANGER,    1, CAPACITY,                                                             "", 14317, 32072, 0,  2, "Capacity of the heat exchanger at design Supply Flow, Demand Flow, and the Inlet Delta T"
HEAT-EXCHANGER,    1, UA-PRODUCT,                                                           "", 14318, 32072, 0,  2, "Overall heat transfer coefficient of the HX at design conditions (inverse of thermal resistance)"
HEAT-EXCHANGER,    1, INLETS-DT,                                                            "", 14319, 32072, 0,  2, "Design Delta T between entering supply-side fluid T and entering demand-side fluid T"
HEAT-EXCHANGER,    1, SUPPLY-FLOW,                                                          "", 14321, 32072, 0,  2, "Design fluid flow rate on the supply-side"
HEAT-EXCHANGER,    1, MAX-SUPPLY-FLOW,                                                      "", 14322, 32072, 0,  2, "Ratio of the maximum allowable supply-side flow rate to the design Flow rate"
HEAT-EXCHANGER,    1, SUPPLY-PRES-DROP,                                                     "", 14510, 32072, 0,  2, "Design pressure drop of the supply-side fluid at the design Flow rate"
HEAT-EXCHANGER,    1, SUPPLY-FILM-RES,                                                      "", 14323, 32072, 0,  2, "Fraction of overall heat exchanger resistance caused by the supply-side film resistance"
HEAT-EXCHANGER,    1, SUPPLY-FILM-EXP,                                                      "", 14324, 32072, 0,  2, "Exponential factor that modifies Film Resistance Fraction (Supply Side) as fct of fluid flow rate"
HEAT-EXCHANGER,    1, DEMAND-FLOW,                                                          "", 14326, 32072, 0,  2, "Demand-side design fluid flow rate"
HEAT-EXCHANGER,    1, MAX-DEMAND-FLOW,                                                      "", 14327, 32072, 0,  2, "Ratio of the maximum allowable demand-side flow rate to the design Flow rate"
HEAT-EXCHANGER,    1, DEMAND-PRES-DROP,                                                     "", 14511, 32072, 0,  2, "Demand-side fluid pressure drop (at the design Flow rate)"
HEAT-EXCHANGER,    1, DEMAND-FILM-RES,                                                      "", 14328, 32072, 0,  2, "Fraction of overall HX thermal resistance caused by the demand-side film resistance"
HEAT-EXCHANGER,    1, DEMAND-FILM-EXP,                                                      "", 14329, 32072, 0,  2, "Exponential factor modifies Film Resistance Fraction (Demand Side) as a fct of fluid flow rate"
HEAT-EXCHANGER,    1, MAX-ERROR,                                                            "", 14320, 32072, 0,  2, "Maximum convergence error that the algorithm must meet for an iteration to be valid"
HEAT-EXCHANGER,    1, EQUIPMENT-REPORT,                                                     "",     0, 32072, 0,  2, ""
HEAT-EXCHANGER,    1, PICTURE,                                                              "",     0, 32072, 0,  2, ""
HEAT-EXCHANGER,    1, DRAWING,                                                              "",     0, 32072, 0,  2, ""
HEAT-EXCHANGER,    2, TYPE,                                                             "Type", 14315, 32072, 0,  2, "The type of heat exchanger (defines both fluid types)"
HEAT-EXCHANGER,    2, CONFIGURATION,                                                        "", 14316, 32072, 0,  2, "Configuration of the heat exchanger (default varies according to Type of HX)"
HEAT-EXCHANGER,    2, CAPACITY,                                                             "", 14317, 32072, 0,  2, "Capacity of the heat exchanger at design Supply Flow, Demand Flow, and the Inlet Delta T"
HEAT-EXCHANGER,    2, UA-PRODUCT,                                                           "", 14318, 32072, 0,  2, "Overall heat transfer coefficient of the HX at design conditions (inverse of thermal resistance)"
HEAT-EXCHANGER,    2, INLETS-DT,                                                            "", 14319, 32072, 0,  2, "Design Delta T between entering supply-side fluid T and entering demand-side fluid T"
HEAT-EXCHANGER,    2, SUPPLY-FLOW,                                                          "", 14321, 32072, 0,  2, "Design fluid flow rate on the supply-side"
HEAT-EXCHANGER,    2, MAX-SUPPLY-FLOW,                                                      "", 14322, 32072, 0,  2, "Ratio of the maximum allowable supply-side flow rate to the design Flow rate"
HEAT-EXCHANGER,    2, SUPPLY-PRES-DROP,                                                     "", 14510, 32072, 0,  2, "Design pressure drop of the supply-side fluid at the design Flow rate"
HEAT-EXCHANGER,    2, SUPPLY-FILM-RES,                                                      "", 14323, 32072, 0,  2, "Fraction of overall heat exchanger resistance caused by the supply-side film resistance "
HEAT-EXCHANGER,    2, SUPPLY-FILM-EXP,                                                      "", 14324, 32072, 0,  2, "Exponential factor that modifies Film Resistance Fraction (Supply Side) as fct of fluid flow rate"
HEAT-EXCHANGER,    2, DEMAND-FLOW,                                                          "", 14326, 32072, 0,  2, "Demand-side design fluid flow rate"
HEAT-EXCHANGER,    2, MAX-DEMAND-FLOW,                                                      "", 14327, 32072, 0,  2, "Ratio of the maximum allowable demand-side flow rate to the design Flow rate"
HEAT-EXCHANGER,    2, DEMAND-PRES-DROP,                                                     "", 14511, 32072, 0,  2, "Demand-side fluid pressure drop (at the design Flow rate)"
HEAT-EXCHANGER,    2, DEMAND-FILM-RES,                                                      "", 14328, 32072, 0,  2, "Fraction of overall HX thermal resistance caused by the demand-side film resistance "
HEAT-EXCHANGER,    2, DEMAND-FILM-EXP,                                                      "", 14329, 32072, 0,  2, "Exponential factor modifies Film Resistance Fraction (Demand Side) as a fct of fluid flow rate"
HEAT-EXCHANGER,    2, MAX-ERROR,                                                            "", 14320, 32072, 0,  2, "Maximum convergence error that the algorithm must meet for an iteration to be valid"
HEAT-EXCHANGER,    2, EQUIPMENT-REPORT,                                                     "",     0, 32072, 0,  2, ""
HEAT-EXCHANGER,    2, PICTURE,                                                              "",     0, 32072, 0,  2, ""
HEAT-EXCHANGER,    2, DRAWING,                                                              "",     0, 32072, 0,  2, ""
HEAT-EXCHANGER,    3, TYPE,                                                             "Type", 14315, 32072, 0,  2, "The type of heat exchanger (defines both fluid types)"
HEAT-EXCHANGER,    3, CONFIGURATION,                                                        "", 14316, 32072, 0,  2, "Configuration of the heat exchanger (default varies according to Type of HX)"
HEAT-EXCHANGER,    3, CAPACITY,                                                             "", 14317, 32072, 0,  2, "Capacity of the heat exchanger at design Supply Flow, Demand Flow, and the Inlet Delta T"
HEAT-EXCHANGER,    3, UA-PRODUCT,                                                           "", 14318, 32072, 0,  2, "Overall heat transfer coefficient of the HX at design conditions (inverse of thermal resistance)"
HEAT-EXCHANGER,    3, INLETS-DT,                                                            "", 14319, 32072, 0,  2, "Design Delta T between entering supply-side fluid T and entering demand-side fluid T"
HEAT-EXCHANGER,    3, SUPPLY-FLOW,                                                          "", 14321, 32072, 0,  2, "Design fluid flow rate on the supply-side"
HEAT-EXCHANGER,    3, MAX-SUPPLY-FLOW,                                                      "", 14322, 32072, 0,  2, "Ratio of the maximum allowable supply-side flow rate to the design Flow rate"
HEAT-EXCHANGER,    3, SUPPLY-PRES-DROP,                                                     "", 14510, 32072, 0,  2, "Design pressure drop of the supply-side fluid at the design Flow rate"
HEAT-EXCHANGER,    3, SUPPLY-FILM-RES,                                                      "", 14323, 32072, 0,  2, "Fraction of overall heat exchanger resistance caused by the supply-side film resistance"
HEAT-EXCHANGER,    3, SUPPLY-FILM-EXP,                                                      "", 14324, 32072, 0,  2, "Exponential factor that modifies Film Resistance Fraction (Supply Side) as fct of fluid flow rate"
HEAT-EXCHANGER,    3, DEMAND-FLOW,                                                          "", 14326, 32072, 0,  2, "Demand-side design fluid flow rate"
HEAT-EXCHANGER,    3, MAX-DEMAND-FLOW,                                                      "", 14327, 32072, 0,  2, "Ratio of the maximum allowable demand-side flow rate to the design Flow rate"
HEAT-EXCHANGER,    3, DEMAND-PRES-DROP,                                                     "", 14511, 32072, 0,  2, "Demand-side fluid pressure drop (at the design Flow rate)"
HEAT-EXCHANGER,    3, DEMAND-FILM-RES,                                                      "", 14328, 32072, 0,  2, "Fraction of overall HX thermal resistance caused by the demand-side film resistance"
HEAT-EXCHANGER,    3, DEMAND-FILM-EXP,                                                      "", 14329, 32072, 0,  2, "Exponential factor modifies Film Resistance Fraction (Demand Side) as a fct of fluid flow rate"
HEAT-EXCHANGER,    3, MAX-ERROR,                                                            "", 14320, 32072, 0,  2, "Maximum convergence error that the algorithm must meet for an iteration to be valid"
HEAT-EXCHANGER,    3, EQUIPMENT-REPORT,                                                     "",     0, 32072, 0,  2, ""
HEAT-EXCHANGER,    3, PICTURE,                                                              "",     0, 32072, 0,  2, ""
HEAT-EXCHANGER,    3, DRAWING,                                                              "",     0, 32072, 0,  2, ""
HEAT-EXCHANGER,    4, TYPE,                                                             "Type", 14315, 32072, 0,  2, "The type of heat exchanger (defines both fluid types)"
HEAT-EXCHANGER,    4, CONFIGURATION,                                                        "", 14316, 32072, 0,  2, "Configuration of the heat exchanger (default varies according to Type of HX)"
HEAT-EXCHANGER,    4, CAPACITY,                                                             "", 14317, 32072, 0,  2, "Capacity of the heat exchanger at design Supply Flow, Demand Flow, and the Inlet Delta T"
HEAT-EXCHANGER,    4, UA-PRODUCT,                                                           "", 14318, 32072, 0,  2, "Overall heat transfer coefficient of the HX at design conditions (inverse of thermal resistance)"
HEAT-EXCHANGER,    4, INLETS-DT,                                                            "", 14319, 32072, 0,  2, "Design Delta T between entering supply-side fluid T and entering demand-side fluid T"
HEAT-EXCHANGER,    4, SUPPLY-FLOW,                                                          "", 14321, 32072, 0,  2, "Design fluid flow rate on the supply-side"
HEAT-EXCHANGER,    4, MAX-SUPPLY-FLOW,                                                      "", 14322, 32072, 0,  2, "Ratio of the maximum allowable supply-side flow rate to the design Flow rate"
HEAT-EXCHANGER,    4, SUPPLY-PRES-DROP,                                                     "", 14510, 32072, 0,  2, "Design pressure drop of the supply-side fluid at the design Flow rate"
HEAT-EXCHANGER,    4, SUPPLY-FILM-RES,                                                      "", 14323, 32072, 0,  2, "Fraction of overall heat exchanger resistance caused by the supply-side film resistance"
HEAT-EXCHANGER,    4, SUPPLY-FILM-EXP,                                                      "", 14324, 32072, 0,  2, "Exponential factor that modifies Film Resistance Fraction (Supply Side) as fct of fluid flow rate"
HEAT-EXCHANGER,    4, DEMAND-FLOW,                                                          "", 14326, 32072, 0,  2, "Demand-side design fluid flow rate"
HEAT-EXCHANGER,    4, MAX-DEMAND-FLOW,                                                      "", 14327, 32072, 0,  2, "Ratio of the maximum allowable demand-side flow rate to the design Flow rate"
HEAT-EXCHANGER,    4, DEMAND-PRES-DROP,                                                     "", 14511, 32072, 0,  2, "Demand-side fluid pressure drop (at the design Flow rate)"
HEAT-EXCHANGER,    4, DEMAND-FILM-RES,                                                      "", 14328, 32072, 0,  2, "Fraction of overall HX thermal resistance caused by the demand-side film resistance"
HEAT-EXCHANGER,    4, DEMAND-FILM-EXP,                                                      "", 14329, 32072, 0,  2, "Exponential factor modifies Film Resistance Fraction (Demand Side) as a fct of fluid flow rate"
HEAT-EXCHANGER,    4, MAX-ERROR,                                                            "", 14320, 32072, 0,  2, "Maximum convergence error that the algorithm must meet for an iteration to be valid"
HEAT-EXCHANGER,    4, EQUIPMENT-REPORT,                                                     "",     0, 32072, 0,  2, ""
HEAT-EXCHANGER,    4, PICTURE,                                                              "",     0, 32072, 0,  2, ""
HEAT-EXCHANGER,    4, DRAWING,                                                              "",     0, 32072, 0,  2, ""
EQUIP-CTRL,        1, TYPE,                                                             "Type", 14020, 32073, 0,  0, "The type of load that this Equipment Control sequence applies to"
EQUIP-CTRL,        1, CIRCULATION-LOOP,                                     "Circulation Loop", 19103, 32073, 0,  0, "Name of the Loop this Equipment Control sequence applies to"
EQUIP-CTRL,        1, LOADS-THRU-1,                                                         "", 14053, 32073, 0,  2, "The load threshold up to which the corresponding piece of equipment is used to satisfy"
EQUIP-CTRL,        1, LOADS-THRU-2,                                                         "", 14053, 32073, 0,  2, "The load threshold up to which the corresponding piece of equipment is used to satisfy"
EQUIP-CTRL,        1, LOADS-THRU-3,                                                         "", 14053, 32073, 0,  2, "The load threshold up to which the corresponding piece of equipment is used to satisfy"
EQUIP-CTRL,        1, LOADS-THRU-4,                                                         "", 14053, 32073, 0,  2, "The load threshold up to which the corresponding piece of equipment is used to satisfy"
EQUIP-CTRL,        1, LOADS-THRU-5,                                                         "", 14053, 32073, 0,  2, "The load threshold up to which the corresponding piece of equipment is used to satisfy"
EQUIP-CTRL,        1, PRORATE-LOAD,                                                         "", 14053, 32073, 0,  2, "Prorate load to all equipment (yes) or allocate by sequence number (no)"
EQUIP-CTRL,        1, CHILLERS-1,                                                           "",   719, 32073, 0,  0, "Name of the chiller that is used to match the corresponding load range"
EQUIP-CTRL,        1, CHILLERS-2,                                                           "",   719, 32073, 0,  0, "Name of the chiller that is used to match the corresponding load range"
EQUIP-CTRL,        1, CHILLERS-3,                                                           "",   719, 32073, 0,  0, "Name of the chiller that is used to match the corresponding load range"
EQUIP-CTRL,        1, CHILLERS-4,                                                           "",   719, 32073, 0,  0, "Name of the chiller that is used to match the corresponding load range"
EQUIP-CTRL,        1, CHILLERS-5,                                                           "",   719, 32073, 0,  0, "Name of the chiller that is used to match the corresponding load range"
EQUIP-CTRL,        1, CHILLERS-SEQ-1,                                                       "",   720, 32073, 0,  2, "The order in which the chillers are used to satisfy the load"
EQUIP-CTRL,        1, CHILLERS-SEQ-2,                                                       "",   720, 32073, 0,  2, "The order in which the chillers are used to satisfy the load"
EQUIP-CTRL,        1, CHILLERS-SEQ-3,                                                       "",   720, 32073, 0,  2, "The order in which the chillers are used to satisfy the load"
EQUIP-CTRL,        1, CHILLERS-SEQ-4,                                                       "",   720, 32073, 0,  2, "The order in which the chillers are used to satisfy the load"
EQUIP-CTRL,        1, CHILLERS-SEQ-5,                                                       "",   720, 32073, 0,  2, "The order in which the chillers are used to satisfy the load"
EQUIP-CTRL,        1, MAX-LOAD-1,                                                           "",   709, 32073, 0,  2, "The maximum allowable load for the corresponding equipment"
EQUIP-CTRL,        1, MAX-LOAD-2,                                                           "",   709, 32073, 0,  2, "The maximum allowable load for the corresponding equipment"
EQUIP-CTRL,        1, MAX-LOAD-3,                                                           "",   709, 32073, 0,  2, "The maximum allowable load for the corresponding equipment"
EQUIP-CTRL,        1, MAX-LOAD-4,                                                           "",   709, 32073, 0,  2, "The maximum allowable load for the corresponding equipment"
EQUIP-CTRL,        1, MAX-LOAD-5,                                                           "",   709, 32073, 0,  2, "The maximum allowable load for the corresponding equipment"
EQUIP-CTRL,        1, STORE-SEQ-1,                                                          "", 14025, 32073, 0,  2, "The order in which the thermal storage devices are used to satisfy the load"
EQUIP-CTRL,        1, STORE-SEQ-2,                                                          "", 14025, 32073, 0,  2, "The order in which the thermal storage devices are used to satisfy the load"
EQUIP-CTRL,        1, STORE-SEQ-3,                                                          "", 14025, 32073, 0,  2, "The order in which the thermal storage devices are used to satisfy the load"
EQUIP-CTRL,        1, STORE-SEQ-4,                                                          "", 14025, 32073, 0,  2, "The order in which the thermal storage devices are used to satisfy the load"
EQUIP-CTRL,        1, STORE-SEQ-5,                                                          "", 14025, 32073, 0,  2, "The order in which the thermal storage devices are used to satisfy the load"
EQUIP-CTRL,        1, STORE-MAX-LOAD-1,                                                     "", 14026, 32073, 0,  2, "The maximum allowable load for the thermal storage device"
EQUIP-CTRL,        1, STORE-MAX-LOAD-2,                                                     "", 14026, 32073, 0,  2, "The maximum allowable load for the thermal storage device"
EQUIP-CTRL,        1, STORE-MAX-LOAD-3,                                                     "", 14026, 32073, 0,  2, "The maximum allowable load for the thermal storage device"
EQUIP-CTRL,        1, STORE-MAX-LOAD-4,                                                     "", 14026, 32073, 0,  2, "The maximum allowable load for the thermal storage device"
EQUIP-CTRL,        1, STORE-MAX-LOAD-5,                                                     "", 14026, 32073, 0,  2, "The maximum allowable load for the thermal storage device"
EQUIP-CTRL,        1, METER-SEQ-1,                                                          "", 14027, 32073, 0,  2, "The order in which the meters are used to satisfy the load"
EQUIP-CTRL,        1, METER-SEQ-2,                                                          "", 14027, 32073, 0,  2, "The order in which the meters are used to satisfy the load"
EQUIP-CTRL,        1, METER-SEQ-3,                                                          "", 14027, 32073, 0,  2, "The order in which the meters are used to satisfy the load"
EQUIP-CTRL,        1, METER-SEQ-4,                                                          "", 14027, 32073, 0,  2, "The order in which the meters are used to satisfy the load"
EQUIP-CTRL,        1, METER-SEQ-5,                                                          "", 14027, 32073, 0,  2, "The order in which the meters are used to satisfy the load"
EQUIP-CTRL,        1, METER-MAX-LOAD-1,                                                     "", 14028, 32073, 0,  2, "The maximum allowable load for the meter"
EQUIP-CTRL,        1, METER-MAX-LOAD-2,                                                     "", 14028, 32073, 0,  2, "The maximum allowable load for the meter"
EQUIP-CTRL,        1, METER-MAX-LOAD-3,                                                     "", 14028, 32073, 0,  2, "The maximum allowable load for the meter"
EQUIP-CTRL,        1, METER-MAX-LOAD-4,                                                     "", 14028, 32073, 0,  2, "The maximum allowable load for the meter"
EQUIP-CTRL,        1, METER-MAX-LOAD-5,                                                     "", 14028, 32073, 0,  2, "The maximum allowable load for the meter"
EQUIP-CTRL,        2, TYPE,                                                             "Type", 14020, 32073, 0,  0, "The type of load that this Equipment Control sequence applies to"
EQUIP-CTRL,        2, CIRCULATION-LOOP,                                     "Circulation Loop", 19103, 32073, 0,  0, "Name of the Loop this Equipment Control sequence applies to"
EQUIP-CTRL,        2, LOADS-THRU-1,                                                         "", 14053, 32073, 0,  2, "The load threshold up to which the corresponding piece of equipment is used to satisfy"
EQUIP-CTRL,        2, LOADS-THRU-2,                                                         "", 14053, 32073, 0,  2, "The load threshold up to which the corresponding piece of equipment is used to satisfy"
EQUIP-CTRL,        2, LOADS-THRU-3,                                                         "", 14053, 32073, 0,  2, "The load threshold up to which the corresponding piece of equipment is used to satisfy"
EQUIP-CTRL,        2, LOADS-THRU-4,                                                         "", 14053, 32073, 0,  2, "The load threshold up to which the corresponding piece of equipment is used to satisfy"
EQUIP-CTRL,        2, LOADS-THRU-5,                                                         "", 14053, 32073, 0,  2, "The load threshold up to which the corresponding piece of equipment is used to satisfy"
EQUIP-CTRL,        2, PRORATE-LOAD,                                                         "", 14053, 32073, 0,  2, "Prorate load to all equipment (yes) or allocate by sequence number (no)"
EQUIP-CTRL,        2, BOILERS-1,                                                            "",   721, 32073, 0,  0, "Name of the boiler that is used to match the corresponding load range"
EQUIP-CTRL,        2, BOILERS-2,                                                            "",   721, 32073, 0,  0, "Name of the boiler that is used to match the corresponding load range"
EQUIP-CTRL,        2, BOILERS-3,                                                            "",   721, 32073, 0,  0, "Name of the boiler that is used to match the corresponding load range"
EQUIP-CTRL,        2, BOILERS-4,                                                            "",   721, 32073, 0,  0, "Name of the boiler that is used to match the corresponding load range"
EQUIP-CTRL,        2, BOILERS-5,                                                            "",   721, 32073, 0,  0, "Name of the boiler that is used to match the corresponding load range"
EQUIP-CTRL,        2, BOILERS-SEQ-1,                                                        "",   720, 32073, 0,  2, "The order in which the boilers are used to satisfy the load"
EQUIP-CTRL,        2, BOILERS-SEQ-2,                                                        "",   720, 32073, 0,  2, "The order in which the boilers are used to satisfy the load"
EQUIP-CTRL,        2, BOILERS-SEQ-3,                                                        "",   720, 32073, 0,  2, "The order in which the boilers are used to satisfy the load"
EQUIP-CTRL,        2, BOILERS-SEQ-4,                                                        "",   720, 32073, 0,  2, "The order in which the boilers are used to satisfy the load"
EQUIP-CTRL,        2, BOILERS-SEQ-5,                                                        "",   720, 32073, 0,  2, "The order in which the boilers are used to satisfy the load"
EQUIP-CTRL,        2, MAX-LOAD-1,                                                           "",   709, 32073, 0,  2, "The maximum allowable load for the corresponding equipment"
EQUIP-CTRL,        2, MAX-LOAD-2,                                                           "",   709, 32073, 0,  2, "The maximum allowable load for the corresponding equipment"
EQUIP-CTRL,        2, MAX-LOAD-3,                                                           "",   709, 32073, 0,  2, "The maximum allowable load for the corresponding equipment"
EQUIP-CTRL,        2, MAX-LOAD-4,                                                           "",   709, 32073, 0,  2, "The maximum allowable load for the corresponding equipment"
EQUIP-CTRL,        2, MAX-LOAD-5,                                                           "",   709, 32073, 0,  2, "The maximum allowable load for the corresponding equipment"
EQUIP-CTRL,        2, STORE-SEQ-1,                                                          "", 14025, 32073, 0,  2, "The order in which the thermal storage devices are used to satisfy the load"
EQUIP-CTRL,        2, STORE-SEQ-2,                                                          "", 14025, 32073, 0,  2, "The order in which the thermal storage devices are used to satisfy the load"
EQUIP-CTRL,        2, STORE-SEQ-3,                                                          "", 14025, 32073, 0,  2, "The order in which the thermal storage devices are used to satisfy the load"
EQUIP-CTRL,        2, STORE-SEQ-4,                                                          "", 14025, 32073, 0,  2, "The order in which the thermal storage devices are used to satisfy the load"
EQUIP-CTRL,        2, STORE-SEQ-5,                                                          "", 14025, 32073, 0,  2, "The order in which the thermal storage devices are used to satisfy the load"
EQUIP-CTRL,        2, STORE-MAX-LOAD-1,                                                     "", 14026, 32073, 0,  2, "The maximum allowable load for the thermal storage device"
EQUIP-CTRL,        2, STORE-MAX-LOAD-2,                                                     "", 14026, 32073, 0,  2, "The maximum allowable load for the thermal storage device"
EQUIP-CTRL,        2, STORE-MAX-LOAD-3,                                                     "", 14026, 32073, 0,  2, "The maximum allowable load for the thermal storage device"
EQUIP-CTRL,        2, STORE-MAX-LOAD-4,                                                     "", 14026, 32073, 0,  2, "The maximum allowable load for the thermal storage device"
EQUIP-CTRL,        2, STORE-MAX-LOAD-5,                                                     "", 14026, 32073, 0,  2, "The maximum allowable load for the thermal storage device"
EQUIP-CTRL,        2, METER-SEQ-1,                                                          "", 14027, 32073, 0,  2, "The order in which the meters are used to satisfy the load"
EQUIP-CTRL,        2, METER-SEQ-2,                                                          "", 14027, 32073, 0,  2, "The order in which the meters are used to satisfy the load"
EQUIP-CTRL,        2, METER-SEQ-3,                                                          "", 14027, 32073, 0,  2, "The order in which the meters are used to satisfy the load"
EQUIP-CTRL,        2, METER-SEQ-4,                                                          "", 14027, 32073, 0,  2, "The order in which the meters are used to satisfy the load"
EQUIP-CTRL,        2, METER-SEQ-5,                                                          "", 14027, 32073, 0,  2, "The order in which the meters are used to satisfy the load"
EQUIP-CTRL,        2, METER-MAX-LOAD-1,                                                     "", 14028, 32073, 0,  2, "The maximum allowable load for the meter"
EQUIP-CTRL,        2, METER-MAX-LOAD-2,                                                     "", 14028, 32073, 0,  2, "The maximum allowable load for the meter"
EQUIP-CTRL,        2, METER-MAX-LOAD-3,                                                     "", 14028, 32073, 0,  2, "The maximum allowable load for the meter"
EQUIP-CTRL,        2, METER-MAX-LOAD-4,                                                     "", 14028, 32073, 0,  2, "The maximum allowable load for the meter"
EQUIP-CTRL,        2, METER-MAX-LOAD-5,                                                     "", 14028, 32073, 0,  2, "The maximum allowable load for the meter"
EQUIP-CTRL,        2, CHLR/HTRS-1,                                                          "",   717, 32073, 0,  0, "Name of the chiller/heater that is used to match the corresponding load range"
EQUIP-CTRL,        2, CHLR/HTRS-2,                                                          "",   717, 32073, 0,  0, "Name of the chiller/heater that is used to match the corresponding load range"
EQUIP-CTRL,        2, CHLR/HTRS-3,                                                          "",   717, 32073, 0,  0, "Name of the chiller/heater that is used to match the corresponding load range"
EQUIP-CTRL,        2, CHLR/HTRS-4,                                                          "",   717, 32073, 0,  0, "Name of the chiller/heater that is used to match the corresponding load range"
EQUIP-CTRL,        2, CHLR/HTRS-5,                                                          "",   717, 32073, 0,  0, "Name of the chiller/heater that is used to match the corresponding load range"
EQUIP-CTRL,        2, CHLR/HTRS-SEQ-1,                                                      "",   720, 32073, 0,  2, "The order in which the chiller/heaters are used to satisfy the load"
EQUIP-CTRL,        2, CHLR/HTRS-SEQ-2,                                                      "",   720, 32073, 0,  2, "The order in which the chiller/heaters are used to satisfy the load"
EQUIP-CTRL,        2, CHLR/HTRS-SEQ-3,                                                      "",   720, 32073, 0,  2, "The order in which the chiller/heaters are used to satisfy the load"
EQUIP-CTRL,        2, CHLR/HTRS-SEQ-4,                                                      "",   720, 32073, 0,  2, "The order in which the chiller/heaters are used to satisfy the load"
EQUIP-CTRL,        2, CHLR/HTRS-SEQ-5,                                                      "",   720, 32073, 0,  2, "The order in which the chiller/heaters are used to satisfy the load"
EQUIP-CTRL,        2, CHLR/HTRS-MAX-1,                                                      "",   709, 32073, 0,  2, "The maximum allowable load for the chiller/heater"
EQUIP-CTRL,        2, CHLR/HTRS-MAX-2,                                                      "",   709, 32073, 0,  2, "The maximum allowable load for the chiller/heater"
EQUIP-CTRL,        2, CHLR/HTRS-MAX-3,                                                      "",   709, 32073, 0,  2, "The maximum allowable load for the chiller/heater"
EQUIP-CTRL,        2, CHLR/HTRS-MAX-4,                                                      "",   709, 32073, 0,  2, "The maximum allowable load for the chiller/heater"
EQUIP-CTRL,        2, CHLR/HTRS-MAX-5,                                                      "",   709, 32073, 0,  2, "The maximum allowable load for the chiller/heater"
EQUIP-CTRL,        2, GENERATORS-1,                                                         "",     0, 32073, 0,  2, ""
EQUIP-CTRL,        2, GENERATORS-2,                                                         "",     0, 32073, 0,  2, ""
EQUIP-CTRL,        2, GENERATORS-3,                                                         "",     0, 32073, 0,  2, ""
EQUIP-CTRL,        2, GENERATORS-4,                                                         "",     0, 32073, 0,  2, ""
EQUIP-CTRL,        2, GENERATORS-5,                                                         "",     0, 32073, 0,  2, ""
EQUIP-CTRL,        2, GENERATORS-SEQ-1,                                                     "",     0, 32073, 0,  2, ""
EQUIP-CTRL,        2, GENERATORS-SEQ-2,                                                     "",     0, 32073, 0,  2, ""
EQUIP-CTRL,        2, GENERATORS-SEQ-3,                                                     "",     0, 32073, 0,  2, ""
EQUIP-CTRL,        2, GENERATORS-SEQ-4,                                                     "",     0, 32073, 0,  2, ""
EQUIP-CTRL,        2, GENERATORS-SEQ-5,                                                     "",     0, 32073, 0,  2, ""
EQUIP-CTRL,        2, GENERATORS-MAX-1,                                                     "",     0, 32073, 0,  2, ""
EQUIP-CTRL,        2, GENERATORS-MAX-2,                                                     "",     0, 32073, 0,  2, ""
EQUIP-CTRL,        2, GENERATORS-MAX-3,                                                     "",     0, 32073, 0,  2, ""
EQUIP-CTRL,        2, GENERATORS-MAX-4,                                                     "",     0, 32073, 0,  2, ""
EQUIP-CTRL,        2, GENERATORS-MAX-5,                                                     "",     0, 32073, 0,  2, ""
EQUIP-CTRL,        3, TYPE,                                                             "Type", 14020, 32073, 0,  0, "The type of load that this Equipment Control sequence applies to"
EQUIP-CTRL,        3, CIRCULATION-LOOP,                                     "Circulation Loop", 19103, 32073, 0,  0, "Name of the Loop this Equipment Control sequence applies to"
EQUIP-CTRL,        3, LOADS-THRU-1,                                                         "", 14053, 32073, 0,  2, "The load threshold up to which the corresponding piece of equipment is used to satisfy"
EQUIP-CTRL,        3, LOADS-THRU-2,                                                         "", 14053, 32073, 0,  2, "The load threshold up to which the corresponding piece of equipment is used to satisfy"
EQUIP-CTRL,        3, LOADS-THRU-3,                                                         "", 14053, 32073, 0,  2, "The load threshold up to which the corresponding piece of equipment is used to satisfy"
EQUIP-CTRL,        3, LOADS-THRU-4,                                                         "", 14053, 32073, 0,  2, "The load threshold up to which the corresponding piece of equipment is used to satisfy"
EQUIP-CTRL,        3, LOADS-THRU-5,                                                         "", 14053, 32073, 0,  2, "The load threshold up to which the corresponding piece of equipment is used to satisfy"
EQUIP-CTRL,        3, PRORATE-LOAD,                                                         "", 14053, 32073, 0,  2, "Prorate load to all equipment (yes) or allocate by sequence number (no)"
EQUIP-CTRL,        3, DW-HEATERS-1,                                                         "",   714, 32073, 0,  0, "The maximum allowable load for the DHW heater"
EQUIP-CTRL,        3, DW-HEATERS-2,                                                         "",   714, 32073, 0,  0, "The maximum allowable load for the DHW heater"
EQUIP-CTRL,        3, DW-HEATERS-3,                                                         "",   714, 32073, 0,  0, "The maximum allowable load for the DHW heater"
EQUIP-CTRL,        3, DW-HEATERS-4,                                                         "",   714, 32073, 0,  0, "The maximum allowable load for the DHW heater"
EQUIP-CTRL,        3, DW-HEATERS-5,                                                         "",   714, 32073, 0,  0, "The maximum allowable load for the DHW heater"
EQUIP-CTRL,        3, DW-HEATERS-SEQ-1,                                                     "",   720, 32073, 0,  2, "The order in which the DHW heaters are used to satisfy the load"
EQUIP-CTRL,        3, DW-HEATERS-SEQ-2,                                                     "",   720, 32073, 0,  2, "The order in which the DHW heaters are used to satisfy the load"
EQUIP-CTRL,        3, DW-HEATERS-SEQ-3,                                                     "",   720, 32073, 0,  2, "The order in which the DHW heaters are used to satisfy the load"
EQUIP-CTRL,        3, DW-HEATERS-SEQ-4,                                                     "",   720, 32073, 0,  2, "The order in which the DHW heaters are used to satisfy the load"
EQUIP-CTRL,        3, DW-HEATERS-SEQ-5,                                                     "",   720, 32073, 0,  2, "The order in which the DHW heaters are used to satisfy the load"
EQUIP-CTRL,        3, MAX-LOAD-1,                                                           "",   709, 32073, 0,  2, "The maximum allowable load for the corresponding equipment"
EQUIP-CTRL,        3, MAX-LOAD-2,                                                           "",   709, 32073, 0,  2, "The maximum allowable load for the corresponding equipment"
EQUIP-CTRL,        3, MAX-LOAD-3,                                                           "",   709, 32073, 0,  2, "The maximum allowable load for the corresponding equipment"
EQUIP-CTRL,        3, MAX-LOAD-4,                                                           "",   709, 32073, 0,  2, "The maximum allowable load for the corresponding equipment"
EQUIP-CTRL,        3, MAX-LOAD-5,                                                           "",   709, 32073, 0,  2, "The maximum allowable load for the corresponding equipment"
EQUIP-CTRL,        3, METER-SEQ-1,                                                          "", 14027, 32073, 0,  2, "The order in which the meters are used to satisfy the load"
EQUIP-CTRL,        3, METER-SEQ-2,                                                          "", 14027, 32073, 0,  2, "The order in which the meters are used to satisfy the load"
EQUIP-CTRL,        3, METER-SEQ-3,                                                          "", 14027, 32073, 0,  2, "The order in which the meters are used to satisfy the load"
EQUIP-CTRL,        3, METER-SEQ-4,                                                          "", 14027, 32073, 0,  2, "The order in which the meters are used to satisfy the load"
EQUIP-CTRL,        3, METER-SEQ-5,                                                          "", 14027, 32073, 0,  2, "The order in which the meters are used to satisfy the load"
EQUIP-CTRL,        3, METER-MAX-LOAD-1,                                                     "", 14028, 32073, 0,  2, "The maximum allowable load for the meter"
EQUIP-CTRL,        3, METER-MAX-LOAD-2,                                                     "", 14028, 32073, 0,  2, "The maximum allowable load for the meter"
EQUIP-CTRL,        3, METER-MAX-LOAD-3,                                                     "", 14028, 32073, 0,  2, "The maximum allowable load for the meter"
EQUIP-CTRL,        3, METER-MAX-LOAD-4,                                                     "", 14028, 32073, 0,  2, "The maximum allowable load for the meter"
EQUIP-CTRL,        3, METER-MAX-LOAD-5,                                                     "", 14028, 32073, 0,  2, "The maximum allowable load for the meter"
EQUIP-CTRL,        3, GENERATORS-1,                                                         "",     0, 32073, 0,  2, ""
EQUIP-CTRL,        3, GENERATORS-2,                                                         "",     0, 32073, 0,  2, ""
EQUIP-CTRL,        3, GENERATORS-3,                                                         "",     0, 32073, 0,  2, ""
EQUIP-CTRL,        3, GENERATORS-4,                                                         "",     0, 32073, 0,  2, ""
EQUIP-CTRL,        3, GENERATORS-5,                                                         "",     0, 32073, 0,  2, ""
EQUIP-CTRL,        3, GENERATORS-SEQ-1,                                                     "",     0, 32073, 0,  2, ""
EQUIP-CTRL,        3, GENERATORS-SEQ-2,                                                     "",     0, 32073, 0,  2, ""
EQUIP-CTRL,        3, GENERATORS-SEQ-3,                                                     "",     0, 32073, 0,  2, ""
EQUIP-CTRL,        3, GENERATORS-SEQ-4,                                                     "",     0, 32073, 0,  2, ""
EQUIP-CTRL,        3, GENERATORS-SEQ-5,                                                     "",     0, 32073, 0,  2, ""
EQUIP-CTRL,        3, GENERATORS-MAX-1,                                                     "",     0, 32073, 0,  2, ""
EQUIP-CTRL,        3, GENERATORS-MAX-2,                                                     "",     0, 32073, 0,  2, ""
EQUIP-CTRL,        3, GENERATORS-MAX-3,                                                     "",     0, 32073, 0,  2, ""
EQUIP-CTRL,        3, GENERATORS-MAX-4,                                                     "",     0, 32073, 0,  2, ""
EQUIP-CTRL,        3, GENERATORS-MAX-5,                                                     "",     0, 32073, 0,  2, ""
EQUIP-CTRL,        4, TYPE,                                                             "Type", 14020, 32073, 0,  0, "The type of load that this Equipment Control sequence applies to"
EQUIP-CTRL,        4, CIRCULATION-LOOP,                                     "Circulation Loop", 19103, 32073, 0,  0, "Name of the Loop this Equipment Control sequence applies to"
EQUIP-CTRL,        4, FLOWS-THRU-1,                                                         "", 14022, 32073, 0,  2, "Maximum flow rate for which the Heat Rejection device is used"
EQUIP-CTRL,        4, FLOWS-THRU-2,                                                         "", 14022, 32073, 0,  2, "Maximum flow rate for which the Heat Rejection device is used"
EQUIP-CTRL,        4, FLOWS-THRU-3,                                                         "", 14022, 32073, 0,  2, "Maximum flow rate for which the Heat Rejection device is used"
EQUIP-CTRL,        4, FLOWS-THRU-4,                                                         "", 14022, 32073, 0,  2, "Maximum flow rate for which the Heat Rejection device is used"
EQUIP-CTRL,        4, FLOWS-THRU-5,                                                         "", 14022, 32073, 0,  2, "Maximum flow rate for which the Heat Rejection device is used"
EQUIP-CTRL,        4, PRORATE-LOAD,                                                         "", 14053, 32073, 0,  2, "Prorate load to all equipment (yes) or allocate by sequence number (no)"
EQUIP-CTRL,        4, HEAT-REJ-1,                                                           "",   712, 32073, 0,  0, "The maximum allowable load for the heat rejector"
EQUIP-CTRL,        4, HEAT-REJ-2,                                                           "",   712, 32073, 0,  0, "The maximum allowable load for the heat rejector"
EQUIP-CTRL,        4, HEAT-REJ-3,                                                           "",   712, 32073, 0,  0, "The maximum allowable load for the heat rejector"
EQUIP-CTRL,        4, HEAT-REJ-4,                                                           "",   712, 32073, 0,  0, "The maximum allowable load for the heat rejector"
EQUIP-CTRL,        4, HEAT-REJ-5,                                                           "",   712, 32073, 0,  0, "The maximum allowable load for the heat rejector"
EQUIP-CTRL,        4, HEAT-REJ-SEQ-1,                                                       "",   720, 32073, 0,  2, "The order in which the heat rejectors are used to satisfy the load"
EQUIP-CTRL,        4, HEAT-REJ-SEQ-2,                                                       "",   720, 32073, 0,  2, "The order in which the heat rejectors are used to satisfy the load"
EQUIP-CTRL,        4, HEAT-REJ-SEQ-3,                                                       "",   720, 32073, 0,  2, "The order in which the heat rejectors are used to satisfy the load"
EQUIP-CTRL,        4, HEAT-REJ-SEQ-4,                                                       "",   720, 32073, 0,  2, "The order in which the heat rejectors are used to satisfy the load"
EQUIP-CTRL,        4, HEAT-REJ-SEQ-5,                                                       "",   720, 32073, 0,  2, "The order in which the heat rejectors are used to satisfy the load"
EQUIP-CTRL,        4, MAX-FLOW-1,                                                           "",   710, 32073, 0,  2, "Maximum allowable flow rate that can be assigned to each Heat Rejection Device"
EQUIP-CTRL,        4, MAX-FLOW-2,                                                           "",   710, 32073, 0,  2, "Maximum allowable flow rate that can be assigned to each Heat Rejection Device"
EQUIP-CTRL,        4, MAX-FLOW-3,                                                           "",   710, 32073, 0,  2, "Maximum allowable flow rate that can be assigned to each Heat Rejection Device"
EQUIP-CTRL,        4, MAX-FLOW-4,                                                           "",   710, 32073, 0,  2, "Maximum allowable flow rate that can be assigned to each Heat Rejection Device"
EQUIP-CTRL,        4, MAX-FLOW-5,                                                           "",   710, 32073, 0,  2, "Maximum allowable flow rate that can be assigned to each Heat Rejection Device"
EQUIP-CTRL,        4, GLHX-1,                                                               "",   712, 32073, 0,  0, "Name of the ground loop HX that is used to match the corresponding load range"
EQUIP-CTRL,        4, GLHX-2,                                                               "",   712, 32073, 0,  0, "Name of the ground loop HX that is used to match the corresponding load range"
EQUIP-CTRL,        4, GLHX-3,                                                               "",   712, 32073, 0,  0, "Name of the ground loop HX that is used to match the corresponding load range"
EQUIP-CTRL,        4, GLHX-4,                                                               "",   712, 32073, 0,  0, "Name of the ground loop HX that is used to match the corresponding load range"
EQUIP-CTRL,        4, GLHX-5,                                                               "",   712, 32073, 0,  0, "Name of the ground loop HX that is used to match the corresponding load range"
EQUIP-CTRL,        4, GLHX-SEQ-1,                                                           "",   720, 32073, 0,  2, "The order in which the ground loop HXs are used to satisfy the load"
EQUIP-CTRL,        4, GLHX-SEQ-2,                                                           "",   720, 32073, 0,  2, "The order in which the ground loop HXs are used to satisfy the load"
EQUIP-CTRL,        4, GLHX-SEQ-3,                                                           "",   720, 32073, 0,  2, "The order in which the ground loop HXs are used to satisfy the load"
EQUIP-CTRL,        4, GLHX-SEQ-4,                                                           "",   720, 32073, 0,  2, "The order in which the ground loop HXs are used to satisfy the load"
EQUIP-CTRL,        4, GLHX-SEQ-5,                                                           "",   720, 32073, 0,  2, "The order in which the ground loop HXs are used to satisfy the load"
EQUIP-CTRL,        4, GLHX-MAX-1,                                                           "",   710, 32073, 0,  2, "The maximum allowable flow for the ground loop HX"
EQUIP-CTRL,        4, GLHX-MAX-2,                                                           "",   710, 32073, 0,  2, "The maximum allowable flow for the ground loop HX"
EQUIP-CTRL,        4, GLHX-MAX-3,                                                           "",   710, 32073, 0,  2, "The maximum allowable flow for the ground loop HX"
EQUIP-CTRL,        4, GLHX-MAX-4,                                                           "",   710, 32073, 0,  2, "The maximum allowable flow for the ground loop HX"
EQUIP-CTRL,        4, GLHX-MAX-5,                                                           "",   710, 32073, 0,  2, "The maximum allowable flow for the ground loop HX"
EQUIP-CTRL,        5, TYPE,                                                             "Type", 14020, 32073, 0,  0, "The type of load that this Equipment Control sequence applies to"
EQUIP-CTRL,        5, ELEC-METER,                                             "Electric Meter", 14052, 32073, 0,  0, "Name of the Electric Meter for which this control sequence controls the attached generators"
EQUIP-CTRL,        5, LOADS-THRU-1,                                                         "", 14053, 32073, 0,  2, "The load threshold up to which the corresponding piece of equipment is used to satisfy"
EQUIP-CTRL,        5, LOADS-THRU-2,                                                         "", 14053, 32073, 0,  2, "The load threshold up to which the corresponding piece of equipment is used to satisfy"
EQUIP-CTRL,        5, LOADS-THRU-3,                                                         "", 14053, 32073, 0,  2, "The load threshold up to which the corresponding piece of equipment is used to satisfy"
EQUIP-CTRL,        5, LOADS-THRU-4,                                                         "", 14053, 32073, 0,  2, "The load threshold up to which the corresponding piece of equipment is used to satisfy"
EQUIP-CTRL,        5, LOADS-THRU-5,                                                         "", 14053, 32073, 0,  2, "The load threshold up to which the corresponding piece of equipment is used to satisfy"
EQUIP-CTRL,        5, PRORATE-LOAD,                                                         "", 14053, 32073, 0,  2, "Prorate load to all equipment (yes) or allocate by sequence number (no)"
EQUIP-CTRL,        5, GENERATORS-1,                                                         "",   714, 32073, 0,  0, "The maximum allowable load for the generator"
EQUIP-CTRL,        5, GENERATORS-2,                                                         "",   714, 32073, 0,  0, "The maximum allowable load for the generator"
EQUIP-CTRL,        5, GENERATORS-3,                                                         "",   714, 32073, 0,  0, "The maximum allowable load for the generator"
EQUIP-CTRL,        5, GENERATORS-4,                                                         "",   714, 32073, 0,  0, "The maximum allowable load for the generator"
EQUIP-CTRL,        5, GENERATORS-5,                                                         "",   714, 32073, 0,  0, "The maximum allowable load for the generator"
EQUIP-CTRL,        5, GENERATORS-SEQ-1,                                                     "",   720, 32073, 0,  2, "The order in which the generators are used to satisfy the load"
EQUIP-CTRL,        5, GENERATORS-SEQ-2,                                                     "",   720, 32073, 0,  2, "The order in which the generators are used to satisfy the load"
EQUIP-CTRL,        5, GENERATORS-SEQ-3,                                                     "",   720, 32073, 0,  2, "The order in which the generators are used to satisfy the load"
EQUIP-CTRL,        5, GENERATORS-SEQ-4,                                                     "",   720, 32073, 0,  2, "The order in which the generators are used to satisfy the load"
EQUIP-CTRL,        5, GENERATORS-SEQ-5,                                                     "",   720, 32073, 0,  2, "The order in which the generators are used to satisfy the load"
EQUIP-CTRL,        5, MAX-LOAD-1,                                                           "",   709, 32073, 0,  2, "The maximum allowable load for the corresponding equipment"
EQUIP-CTRL,        5, MAX-LOAD-2,                                                           "",   709, 32073, 0,  2, "The maximum allowable load for the corresponding equipment"
EQUIP-CTRL,        5, MAX-LOAD-3,                                                           "",   709, 32073, 0,  2, "The maximum allowable load for the corresponding equipment"
EQUIP-CTRL,        5, MAX-LOAD-4,                                                           "",   709, 32073, 0,  2, "The maximum allowable load for the corresponding equipment"
EQUIP-CTRL,        5, MAX-LOAD-5,                                                           "",   709, 32073, 0,  2, "The maximum allowable load for the corresponding equipment"
EQUIP-CTRL,        5, METER-SEQ-1,                                                          "",     0, 32073, 0,  2, ""
EQUIP-CTRL,        5, METER-SEQ-2,                                                          "",     0, 32073, 0,  2, ""
EQUIP-CTRL,        5, METER-SEQ-3,                                                          "",     0, 32073, 0,  2, ""
EQUIP-CTRL,        5, METER-SEQ-4,                                                          "",     0, 32073, 0,  2, ""
EQUIP-CTRL,        5, METER-SEQ-5,                                                          "",     0, 32073, 0,  2, ""
EQUIP-CTRL,        5, METER-MAX-LOAD-1,                                                     "",     0, 32073, 0,  2, ""
EQUIP-CTRL,        5, METER-MAX-LOAD-2,                                                     "",     0, 32073, 0,  2, ""
EQUIP-CTRL,        5, METER-MAX-LOAD-3,                                                     "",     0, 32073, 0,  2, ""
EQUIP-CTRL,        5, METER-MAX-LOAD-4,                                                     "",     0, 32073, 0,  2, ""
EQUIP-CTRL,        5, METER-MAX-LOAD-5,                                                     "",     0, 32073, 0,  2, ""
LOAD-MANAGEMENT,   1, TYPE,                                                             "Type", 14287, 32074, 0,  0, "The type of control this sequence uses"
LOAD-MANAGEMENT,   1, QUAL-SCH,                                                             "", 14288, 32074, 0,  0, "A Flag schedule that defines when this Load Management sequence is active"
LOAD-MANAGEMENT,   1, QUAL-SCH-FLAG,                                     "Schedule Flag Value", 14289, 32074, 0,  2, "Value of the flag in the Qualification Schedule: specifies when this Load Mgmt is active"
LOAD-MANAGEMENT,   1, EQUIP-CTRL-SCH,                             "Equipment Control Schedule", 14290, 32074, 0,  0, "Schedule with flags that switch Equipment Control sequences and/or enable/disable loops"
LOAD-MANAGEMENT,   1, CTRL-FLAG-1,                                            "Control Flag 1", 14294, 32074, 0,  2, "Flag value corresponding to one of the flag values in the Equipment Control Schedule"
LOAD-MANAGEMENT,   1, CTRL-FLAG-2,                                                          "", 14294, 32074, 0,  2, "Flag value corresponding to one of the flag values in the Equipment Control Schedule"
LOAD-MANAGEMENT,   1, CTRL-FLAG-3,                                                          "", 14294, 32074, 0,  2, "Flag value corresponding to one of the flag values in the Equipment Control Schedule"
LOAD-MANAGEMENT,   1, CTRL-FLAG-4,                                                          "", 14294, 32074, 0,  2, "Flag value corresponding to one of the flag values in the Equipment Control Schedule"
LOAD-MANAGEMENT,   1, CTRL-FLAG-5,                                                          "", 14294, 32074, 0,  2, "Flag value corresponding to one of the flag values in the Equipment Control Schedule"
LOAD-MANAGEMENT,   1, CTRL-PRIORITY-1,                                                      "", 14366, 32074, 0,  2, "The Equipment Ctrl sequence with highest priority overrides all others when a conflict exists"
LOAD-MANAGEMENT,   1, CTRL-PRIORITY-2,                                                      "", 14366, 32074, 0,  2, "The Equipment Ctrl sequence with highest priority overrides all others when a conflict exists"
LOAD-MANAGEMENT,   1, CTRL-PRIORITY-3,                                                      "", 14366, 32074, 0,  2, "The Equipment Ctrl sequence with highest priority overrides all others when a conflict exists"
LOAD-MANAGEMENT,   1, CTRL-PRIORITY-4,                                                      "", 14366, 32074, 0,  2, "The Equipment Ctrl sequence with highest priority overrides all others when a conflict exists"
LOAD-MANAGEMENT,   1, CTRL-PRIORITY-5,                                                      "", 14366, 32074, 0,  2, "The Equipment Ctrl sequence with highest priority overrides all others when a conflict exists"
LOAD-MANAGEMENT,   1, EQUIP-CTRLS-1,                                                        "",   699, 32074, 0,  0, "Names of Equip Ctrl sequences used when Equip Ctrl Flag or Temp Through condition is true"
LOAD-MANAGEMENT,   1, EQUIP-CTRLS-2,                                                        "",   699, 32074, 0,  0, "Names of Equip Ctrl sequences used when Equip Ctrl Flag or Temp Through condition is true"
LOAD-MANAGEMENT,   1, EQUIP-CTRLS-3,                                                        "",   699, 32074, 0,  0, "Names of Equip Ctrl sequences used when Equip Ctrl Flag or Temp Through condition is true"
LOAD-MANAGEMENT,   1, EQUIP-CTRLS-4,                                                        "",   699, 32074, 0,  0, "Names of Equip Ctrl sequences used when Equip Ctrl Flag or Temp Through condition is true"
LOAD-MANAGEMENT,   1, EQUIP-CTRLS-5,                                                        "",   699, 32074, 0,  0, "Names of Equip Ctrl sequences used when Equip Ctrl Flag or Temp Through condition is true"
LOAD-MANAGEMENT,   1, LOOPS-ON-1,                                                           "",   697, 32074, 0,  0, "The loops that are forced to operate this hour"
LOAD-MANAGEMENT,   1, LOOPS-ON-2,                                                           "",   697, 32074, 0,  0, "The loops that are forced to operate this hour"
LOAD-MANAGEMENT,   1, LOOPS-ON-3,                                                           "",   697, 32074, 0,  0, "The loops that are forced to operate this hour"
LOAD-MANAGEMENT,   1, LOOPS-ON-4,                                                           "",   697, 32074, 0,  0, "The loops that are forced to operate this hour"
LOAD-MANAGEMENT,   1, LOOPS-ON-5,                                                           "",   697, 32074, 0,  0, "The loops that are forced to operate this hour"
LOAD-MANAGEMENT,   1, LOOPS-OFF-1,                                                          "",   698, 32074, 0,  0, "The loops that are forced off this hour"
LOAD-MANAGEMENT,   1, LOOPS-OFF-2,                                                          "",   698, 32074, 0,  0, "The loops that are forced off this hour"
LOAD-MANAGEMENT,   1, LOOPS-OFF-3,                                                          "",   698, 32074, 0,  0, "The loops that are forced off this hour"
LOAD-MANAGEMENT,   1, LOOPS-OFF-4,                                                          "",   698, 32074, 0,  0, "The loops that are forced off this hour"
LOAD-MANAGEMENT,   1, LOOPS-OFF-5,                                                          "",   698, 32074, 0,  0, "The loops that are forced off this hour"
LOAD-MANAGEMENT,   2, TYPE,                                                             "Type", 14287, 32074, 0,  0, "The type of control this sequence uses"
LOAD-MANAGEMENT,   2, QUAL-SCH,                                                             "", 14288, 32074, 0,  0, "A Flag schedule that defines when this Load Management sequence is active"
LOAD-MANAGEMENT,   2, QUAL-SCH-FLAG,                                                        "", 14289, 32074, 0,  2, "Value of the flag in the Qualification Schedule: specifies when this Load Mgmt is active"
LOAD-MANAGEMENT,   2, TEMPS-THRU-1,                                      "Temperatures Thru 1", 14295, 32074, 0,  2, "The maximum temperature for which this management sequence applies"
LOAD-MANAGEMENT,   2, TEMPS-THRU-2,                                                         "", 14295, 32074, 0,  2, "The maximum temperature for which this management sequence applies"
LOAD-MANAGEMENT,   2, TEMPS-THRU-3,                                                         "", 14295, 32074, 0,  2, "The maximum temperature for which this management sequence applies"
LOAD-MANAGEMENT,   2, TEMPS-THRU-4,                                                         "", 14295, 32074, 0,  2, "The maximum temperature for which this management sequence applies"
LOAD-MANAGEMENT,   2, TEMPS-THRU-5,                                                         "", 14295, 32074, 0,  2, "The maximum temperature for which this management sequence applies"
LOAD-MANAGEMENT,   2, CTRL-PRIORITY-1,                                                      "", 14366, 32074, 0,  2, "The Equipment Ctrl sequence with highest priority overrides all others when a conflict exists"
LOAD-MANAGEMENT,   2, CTRL-PRIORITY-2,                                                      "", 14366, 32074, 0,  2, "The Equipment Ctrl sequence with highest priority overrides all others when a conflict exists"
LOAD-MANAGEMENT,   2, CTRL-PRIORITY-3,                                                      "", 14366, 32074, 0,  2, "The Equipment Ctrl sequence with highest priority overrides all others when a conflict exists"
LOAD-MANAGEMENT,   2, CTRL-PRIORITY-4,                                                      "", 14366, 32074, 0,  2, "The Equipment Ctrl sequence with highest priority overrides all others when a conflict exists"
LOAD-MANAGEMENT,   2, CTRL-PRIORITY-5,                                                      "", 14366, 32074, 0,  2, "The Equipment Ctrl sequence with highest priority overrides all others when a conflict exists"
LOAD-MANAGEMENT,   2, EQUIP-CTRLS-1,                                                        "",   699, 32074, 0,  0, "Names of Equip Ctrl sequences used when Equip Ctrl Flag or Temp Through condition is true"
LOAD-MANAGEMENT,   2, EQUIP-CTRLS-2,                                                        "",   699, 32074, 0,  0, "Names of Equip Ctrl sequences used when Equip Ctrl Flag or Temp Through condition is true"
LOAD-MANAGEMENT,   2, EQUIP-CTRLS-3,                                                        "",   699, 32074, 0,  0, "Names of Equip Ctrl sequences used when Equip Ctrl Flag or Temp Through condition is true"
LOAD-MANAGEMENT,   2, EQUIP-CTRLS-4,                                                        "",   699, 32074, 0,  0, "Names of Equip Ctrl sequences used when Equip Ctrl Flag or Temp Through condition is true"
LOAD-MANAGEMENT,   2, EQUIP-CTRLS-5,                                                        "",   699, 32074, 0,  0, "Names of Equip Ctrl sequences used when Equip Ctrl Flag or Temp Through condition is true"
LOAD-MANAGEMENT,   2, LOOPS-ON-1,                                                           "",   697, 32074, 0,  0, "The loops that are forced to operate this hour"
LOAD-MANAGEMENT,   2, LOOPS-ON-2,                                                           "",   697, 32074, 0,  0, "The loops that are forced to operate this hour"
LOAD-MANAGEMENT,   2, LOOPS-ON-3,                                                           "",   697, 32074, 0,  0, "The loops that are forced to operate this hour"
LOAD-MANAGEMENT,   2, LOOPS-ON-4,                                                           "",   697, 32074, 0,  0, "The loops that are forced to operate this hour"
LOAD-MANAGEMENT,   2, LOOPS-ON-5,                                                           "",   697, 32074, 0,  0, "The loops that are forced to operate this hour"
LOAD-MANAGEMENT,   2, LOOPS-OFF-1,                                                          "",   698, 32074, 0,  0, "The loops that are forced off this hour"
LOAD-MANAGEMENT,   2, LOOPS-OFF-2,                                                          "",   698, 32074, 0,  0, "The loops that are forced off this hour"
LOAD-MANAGEMENT,   2, LOOPS-OFF-3,                                                          "",   698, 32074, 0,  0, "The loops that are forced off this hour"
LOAD-MANAGEMENT,   2, LOOPS-OFF-4,                                                          "",   698, 32074, 0,  0, "The loops that are forced off this hour"
LOAD-MANAGEMENT,   2, LOOPS-OFF-5,                                                          "",   698, 32074, 0,  0, "The loops that are forced off this hour"
LOAD-MANAGEMENT,   3, TYPE,                                                             "Type", 14287, 32074, 0,  0, "The type of control this sequence uses"
LOAD-MANAGEMENT,   3, QUAL-SCH,                                                             "", 14288, 32074, 0,  0, "A Flag schedule that defines when this Load Management sequence is active"
LOAD-MANAGEMENT,   3, QUAL-SCH-FLAG,                                                        "", 14289, 32074, 0,  2, "Value of the flag in the Qualification Schedule: specifies when this Load Mgmt is active"
LOAD-MANAGEMENT,   3, CTRL-ZONE,                                                "Control Zone", 14291, 32074, 0,  0, "Name of the Zone whose temperature is used to switch Equipment Control sequences"
LOAD-MANAGEMENT,   3, TEMPS-THRU-1,                                      "Temperatures Thru 1", 14295, 32074, 0,  2, "The maximum temperature for which this management sequence applies"
LOAD-MANAGEMENT,   3, TEMPS-THRU-2,                                                         "", 14295, 32074, 0,  2, "The maximum temperature for which this management sequence applies"
LOAD-MANAGEMENT,   3, TEMPS-THRU-3,                                                         "", 14295, 32074, 0,  2, "The maximum temperature for which this management sequence applies"
LOAD-MANAGEMENT,   3, TEMPS-THRU-4,                                                         "", 14295, 32074, 0,  2, "The maximum temperature for which this management sequence applies"
LOAD-MANAGEMENT,   3, TEMPS-THRU-5,                                                         "", 14295, 32074, 0,  2, "The maximum temperature for which this management sequence applies"
LOAD-MANAGEMENT,   3, CTRL-PRIORITY-1,                                                      "", 14366, 32074, 0,  2, "The Equipment Ctrl sequence with highest priority overrides all others when a conflict exists"
LOAD-MANAGEMENT,   3, CTRL-PRIORITY-2,                                                      "", 14366, 32074, 0,  2, "The Equipment Ctrl sequence with highest priority overrides all others when a conflict exists"
LOAD-MANAGEMENT,   3, CTRL-PRIORITY-3,                                                      "", 14366, 32074, 0,  2, "The Equipment Ctrl sequence with highest priority overrides all others when a conflict exists"
LOAD-MANAGEMENT,   3, CTRL-PRIORITY-4,                                                      "", 14366, 32074, 0,  2, "The Equipment Ctrl sequence with highest priority overrides all others when a conflict exists"
LOAD-MANAGEMENT,   3, CTRL-PRIORITY-5,                                                      "", 14366, 32074, 0,  2, "The Equipment Ctrl sequence with highest priority overrides all others when a conflict exists"
LOAD-MANAGEMENT,   3, EQUIP-CTRLS-1,                                                        "",   699, 32074, 0,  0, "Names of Equip Ctrl sequences used when Equip Ctrl Flag or Temp Through condition is true"
LOAD-MANAGEMENT,   3, EQUIP-CTRLS-2,                                                        "",   699, 32074, 0,  0, "Names of Equip Ctrl sequences used when Equip Ctrl Flag or Temp Through condition is true"
LOAD-MANAGEMENT,   3, EQUIP-CTRLS-3,                                                        "",   699, 32074, 0,  0, "Names of Equip Ctrl sequences used when Equip Ctrl Flag or Temp Through condition is true"
LOAD-MANAGEMENT,   3, EQUIP-CTRLS-4,                                                        "",   699, 32074, 0,  0, "Names of Equip Ctrl sequences used when Equip Ctrl Flag or Temp Through condition is true"
LOAD-MANAGEMENT,   3, EQUIP-CTRLS-5,                                                        "",   699, 32074, 0,  0, "Names of Equip Ctrl sequences used when Equip Ctrl Flag or Temp Through condition is true"
LOAD-MANAGEMENT,   3, LOOPS-ON-1,                                                           "",   697, 32074, 0,  0, "The loops that are forced to operate this hour"
LOAD-MANAGEMENT,   3, LOOPS-ON-2,                                                           "",   697, 32074, 0,  0, "The loops that are forced to operate this hour"
LOAD-MANAGEMENT,   3, LOOPS-ON-3,                                                           "",   697, 32074, 0,  0, "The loops that are forced to operate this hour"
LOAD-MANAGEMENT,   3, LOOPS-ON-4,                                                           "",   697, 32074, 0,  0, "The loops that are forced to operate this hour"
LOAD-MANAGEMENT,   3, LOOPS-ON-5,                                                           "",   697, 32074, 0,  0, "The loops that are forced to operate this hour"
LOAD-MANAGEMENT,   3, LOOPS-OFF-1,                                                          "",   698, 32074, 0,  0, "The loops that are forced off this hour"
LOAD-MANAGEMENT,   3, LOOPS-OFF-2,                                                          "",   698, 32074, 0,  0, "The loops that are forced off this hour"
LOAD-MANAGEMENT,   3, LOOPS-OFF-3,                                                          "",   698, 32074, 0,  0, "The loops that are forced off this hour"
LOAD-MANAGEMENT,   3, LOOPS-OFF-4,                                                          "",   698, 32074, 0,  0, "The loops that are forced off this hour"
LOAD-MANAGEMENT,   3, LOOPS-OFF-5,                                                          "",   698, 32074, 0,  0, "The loops that are forced off this hour"
LOAD-MANAGEMENT,   4, TYPE,                                                             "Type", 14287, 32074, 0,  0, "The type of control this sequence uses"
LOAD-MANAGEMENT,   4, QUAL-SCH,                                                             "", 14288, 32074, 0,  0, "A Flag schedule that defines when this Load Management sequence is active"
LOAD-MANAGEMENT,   4, QUAL-SCH-FLAG,                                                        "", 14289, 32074, 0,  2, "Value of the flag in the Qualification Schedule: specifies when this Load Mgmt is active"
LOAD-MANAGEMENT,   4, CTRL-LOOP,                                                "Control Loop", 14292, 32074, 0,  0, "Name of Loop whose load is used to switch Equip Ctrl sequences that apply to another loop"
LOAD-MANAGEMENT,   4, LOADS-THRU-1,                                             "Loads Thru 1", 14297, 32074, 0,  2, "The maximum load that this range applies to (used if the Type is Loop Load)"
LOAD-MANAGEMENT,   4, LOADS-THRU-2,                                                         "", 14297, 32074, 0,  2, "The maximum load that this range applies to (used if the Type is Loop Load)"
LOAD-MANAGEMENT,   4, LOADS-THRU-3,                                                         "", 14297, 32074, 0,  2, "The maximum load that this range applies to (used if the Type is Loop Load)"
LOAD-MANAGEMENT,   4, LOADS-THRU-4,                                                         "", 14297, 32074, 0,  2, "The maximum load that this range applies to (used if the Type is Loop Load)"
LOAD-MANAGEMENT,   4, LOADS-THRU-5,                                                         "", 14297, 32074, 0,  2, "The maximum load that this range applies to (used if the Type is Loop Load)"
LOAD-MANAGEMENT,   4, CTRL-PRIORITY-1,                                                      "", 14366, 32074, 0,  2, "A number between 1 and 100 (1 indicates lowest priority, and 100 is the highest)"
LOAD-MANAGEMENT,   4, CTRL-PRIORITY-2,                                                      "", 14366, 32074, 0,  2, "A number between 1 and 100 (1 indicates lowest priority, and 100 is the highest)"
LOAD-MANAGEMENT,   4, CTRL-PRIORITY-3,                                                      "", 14366, 32074, 0,  2, "A number between 1 and 100 (1 indicates lowest priority, and 100 is the highest)"
LOAD-MANAGEMENT,   4, CTRL-PRIORITY-4,                                                      "", 14366, 32074, 0,  2, "A number between 1 and 100 (1 indicates lowest priority, and 100 is the highest)"
LOAD-MANAGEMENT,   4, CTRL-PRIORITY-5,                                                      "", 14366, 32074, 0,  2, "A number between 1 and 100 (1 indicates lowest priority, and 100 is the highest)"
LOAD-MANAGEMENT,   4, EQUIP-CTRLS-1,                                                        "",   699, 32074, 0,  0, "Names of Equip Ctrl sequences used when Equip Ctrl Flag or Temp Through condition is true"
LOAD-MANAGEMENT,   4, EQUIP-CTRLS-2,                                                        "",   699, 32074, 0,  0, "Names of Equip Ctrl sequences used when Equip Ctrl Flag or Temp Through condition is true"
LOAD-MANAGEMENT,   4, EQUIP-CTRLS-3,                                                        "",   699, 32074, 0,  0, "Names of Equip Ctrl sequences used when Equip Ctrl Flag or Temp Through condition is true"
LOAD-MANAGEMENT,   4, EQUIP-CTRLS-4,                                                        "",   699, 32074, 0,  0, "Names of Equip Ctrl sequences used when Equip Ctrl Flag or Temp Through condition is true"
LOAD-MANAGEMENT,   4, EQUIP-CTRLS-5,                                                        "",   699, 32074, 0,  0, "Names of Equip Ctrl sequences used when Equip Ctrl Flag or Temp Through condition is true"
ELEC-METER,        1, TYPE,                                              "Electric Meter Type", 14121, 32075, 0,  0, "Utility=main site meter;Building=attached to Utility Meter;Sub-Meter=Attached to Bldg Meter"
ELEC-METER,        1, UNIT-INDEX,                                                           "", 14137, 32075, 0,  2, "An integer from the units table that defines the billing unit, used to convert english/metric units"
ELEC-METER,        1, DEM-UNIT-INDEX,                                                       "", 14157, 32075, 0,  2, "An integer from the units table that defines the maximum demand billing unit"
ELEC-METER,        1, SOURCE-SITE-EFF,                                                      "", 14158, 32075, 0,  2, "Fraction of total energy used at the utility source that arrives at the site boundary"
ELEC-METER,        1, INTERIOR-POWER,                                                       "",   736, 32075, 0,  2, "Hourly energy consumption of misc. energy uses (typically use Loop Process Loads instead)"
ELEC-METER,        1, INTERIOR-SCH,                                   "Interior Load Schedule",   735, 32075, 0,  0, "A fractional schedule of multipliers applied to the Interior Direct Load each hour"
ELEC-METER,        1, EXTERIOR-POWER,                                                       "",   738, 32075, 0,  2, "Hourly energy consumption of misc. energy uses (typically use Loop Process Loads instead)"
ELEC-METER,        1, EXTERIOR-SCH,                                   "Exterior Load Schedule",   737, 32075, 0,  0, "A fractional schedule of multipliers applied to the Exterior Direct Load each hour"
ELEC-METER,        1, REFG-POWER,                                        "Refrigeration Power",     0, 32075, 0,  2, "Hourly energy consumption of refrigeration equipment (excluding equipment modeled by the simulation)"
ELEC-METER,        1, REFG-SCH,                                       "Refrigeration Schedule",     0, 32075, 0,  0, "A fractional schedule of multipliers applied to the Refrigeration Load each hour"
ELEC-METER,        1, METER-REPORT,                                                         "",     0, 32075, 0,  0, ""
ELEC-METER,        1, TRANSFORMER-SIZE,                                                     "", 14159, 32075, 0,  2, "Capacity of this meter's transformer"
ELEC-METER,        1, TRANSFORMER-LOSS,                                                     "", 14160, 32075, 0,  2, "Fraction of output power lost at full load (used only if Transformer Size is specified)"
ELEC-METER,        1, TRANS-LOSS-FPLR,                                                      "", 14171, 32075, 0,  0, "Quadratic Curve Fit: Multiplier on the Transformer Loss, as a function of the part load"
ELEC-METER,        1, EQUIP-CTRL,                                                           "",     0, 32075, 0,  0, ""
ELEC-METER,        1, COGEN-TRACK-MODE,                                                     "",     0, 32075, 0,  0, ""
ELEC-METER,        1, COGEN-TRACK-SCH,                                                      "",     0, 32075, 0,  0, ""
ELEC-METER,        1, BLDG/SUB-METERS,                                                      "",   739, 32075, 0,  0, "Names of Electric Meters (with Type = Building or Sub-Meter) this meter supplies power to"
ELEC-METER,        2, TYPE,                                              "Electric Meter Type", 14121, 32075, 0,  0, "Utility=main site meter;Building=attached to Utility Meter;Sub-Meter=Attached to Bldg Meter"
ELEC-METER,        2, UNIT-INDEX,                                                           "", 14137, 32075, 0,  2, "An integer from the units table that defines the billing unit, used to convert english/metric units"
ELEC-METER,        2, DEM-UNIT-INDEX,                                                       "", 14157, 32075, 0,  2, "An integer from the units table that defines the maximum demand billing unit"
ELEC-METER,        2, SOURCE-SITE-EFF,                                                      "", 14158, 32075, 0,  2, "Fraction of total energy used at the utility source that arrives at the site boundary"
ELEC-METER,        2, INTERIOR-POWER,                                                       "",   736, 32075, 0,  2, "Hourly energy consumption of misc. energy uses (typically use Loop Process Loads instead)"
ELEC-METER,        2, INTERIOR-SCH,                                   "Interior Load Schedule",   735, 32075, 0,  0, "A fractional schedule of multipliers applied to the Interior Direct Load each hour"
ELEC-METER,        2, EXTERIOR-POWER,                                                       "",   738, 32075, 0,  2, "Hourly energy consumption of misc. energy uses (typically use Loop Process Loads instead)"
ELEC-METER,        2, EXTERIOR-SCH,                                   "Exterior Load Schedule",   737, 32075, 0,  0, "A fractional schedule of multipliers applied to the Exterior Direct Load each hour"
ELEC-METER,        2, REFG-POWER,                                        "Refrigeration Power",     0, 32075, 0,  2, "Hourly energy consumption of refrigeration equipment (excluding equipment modeled by the simulation)"
ELEC-METER,        2, REFG-SCH,                                       "Refrigeration Schedule",     0, 32075, 0,  0, "A fractional schedule of multipliers applied to the Refrigeration Load each hour"
ELEC-METER,        2, METER-REPORT,                                                         "",     0, 32075, 0,  0, ""
ELEC-METER,        2, TRANSFORMER-SIZE,                                                     "", 14159, 32075, 0,  2, "Capacity of this meter's transformer"
ELEC-METER,        2, TRANSFORMER-LOSS,                                                     "", 14160, 32075, 0,  2, "Fraction of output power lost at full load (used only if Transformer Size is specified)"
ELEC-METER,        2, TRANS-LOSS-FPLR,                                                      "", 14171, 32075, 0,  0, "Quadratic Curve Fit: Multiplier on the Transformer Loss, as a function of the part load"
ELEC-METER,        2, SUB-METERS,                                                           "",   734, 32075, 0,  0, "Names of Electric Meters (with Type = Sub-Meter) this Building meter supplies power to"
ELEC-METER,        3, TYPE,                                              "Electric Meter Type", 14121, 32075, 0,  0, "Utility=main site meter;Building=attached to Utility Meter;Sub-Meter=Attached to Bldg Meter"
ELEC-METER,        3, UNIT-INDEX,                                                           "", 14137, 32075, 0,  2, "An integer from the units table that defines the billing unit, used to convert english/metric units"
ELEC-METER,        3, DEM-UNIT-INDEX,                                                       "", 14157, 32075, 0,  2, "An integer from the units table that defines the maximum demand billing unit"
ELEC-METER,        3, SOURCE-SITE-EFF,                                                      "", 14158, 32075, 0,  2, "Fraction of total energy used at the utility source that arrives at the site boundary"
ELEC-METER,        3, INTERIOR-POWER,                                                       "",   736, 32075, 0,  2, "Hourly energy consumption of misc. energy uses (typically use Loop Process Loads instead)"
ELEC-METER,        3, INTERIOR-SCH,                                   "Interior Load Schedule",   735, 32075, 0,  0, "A fractional schedule of multipliers applied to the Interior Direct Load each hour"
ELEC-METER,        3, EXTERIOR-POWER,                                                       "",   738, 32075, 0,  2, "Hourly energy consumption of misc. energy uses (typically use Loop Process Loads instead)"
ELEC-METER,        3, EXTERIOR-SCH,                                   "Exterior Load Schedule",   737, 32075, 0,  0, "A fractional schedule of multipliers applied to the Exterior Direct Load each hour"
ELEC-METER,        3, REFG-POWER,                                        "Refrigeration Power",     0, 32075, 0,  2, "Hourly energy consumption of refrigeration equipment (excluding equipment modeled by the simulation)"
ELEC-METER,        3, REFG-SCH,                                       "Refrigeration Schedule",     0, 32075, 0,  0, "A fractional schedule of multipliers applied to the Refrigeration Load each hour"
ELEC-METER,        3, METER-REPORT,                                                         "",     0, 32075, 0,  0, ""
ELEC-METER,        3, TRANSFORMER-SIZE,                                                     "", 14159, 32075, 0,  2, "Capacity of this meter's transformer"
ELEC-METER,        3, TRANSFORMER-LOSS,                                                     "", 14160, 32075, 0,  2, "Fraction of output power lost at full load (used only if Transformer Size is specified)"
ELEC-METER,        3, TRANS-LOSS-FPLR,                                                      "", 14171, 32075, 0,  0, "Quadratic Curve Fit: Multiplier on the Transformer Loss, as a function of the part load"
ELEC-METER,        4, TYPE,                                              "Electric Meter Type", 14121, 32075, 0,  0, "Utility=main site meter;Building=attached to Utility Meter;Sub-Meter=Attached to Bldg Meter"
ELEC-METER,        4, UNIT-INDEX,                                                           "", 14137, 32075, 0,  2, "An integer from the units table that defines the billing unit, used to convert english/metric units"
ELEC-METER,        4, DEM-UNIT-INDEX,                                                       "", 14157, 32075, 0,  2, "An integer from the units table that defines the maximum demand billing unit"
ELEC-METER,        4, SOURCE-SITE-EFF,                                                      "", 14158, 32075, 0,  2, "Fraction of total energy used at the utility source that arrives at the site boundary"
ELEC-METER,        4, TRANSFORMER-SIZE,                                                     "", 14159, 32075, 0,  2, "Capacity of this meter's transformer"
ELEC-METER,        4, TRANSFORMER-LOSS,                                                     "", 14160, 32075, 0,  2, "Fraction of output power lost at full load (used only if Transformer Size is specified)"
ELEC-METER,        4, TRANS-LOSS-FPLR,                                                      "", 14171, 32075, 0,  0, "Quadratic Curve Fit: Multiplier on the Transformer Loss, as a function of the part load"
ELEC-METER,        4, COGEN-TRACK-MODE,                                                     "",     0, 32075, 0,  0, ""
ELEC-METER,        4, COGEN-TRACK-SCH,                                                      "",     0, 32075, 0,  0, ""
FUEL-METER,        0, TYPE,                                                  "Fuel Meter Type", 14133, 32076, 0,  2, "Type of fuel consumed by equipment attached to this meter"
FUEL-METER,        0, ENERGY/UNIT,                                                          "", 14174, 32076, 0,  2, "Number of Btus per billing unit for this meter (e.g. 100,000 for therms)"
FUEL-METER,        0, UNIT-INDEX,                                                           "", 14175, 32076, 0,  2, "An integer from the units table that defines the billing unit, used to convert english/metric units"
FUEL-METER,        0, DEM-UNIT-INDEX,                                                       "", 14176, 32076, 0,  2, "An integer from the units table that defines the maximum demand billing"
FUEL-METER,        0, SOURCE-SITE-EFF,                                                      "", 14177, 32076, 0,  2, "Fraction of total energy used at the utility source that arrives at the site boundary"
FUEL-METER,        0, INTERIOR-POWER,                                                       "",   746, 32076, 0,  2, "Hourly energy consumption of misc. energy uses (typically use Loop Process Loads instead)"
FUEL-METER,        0, INTERIOR-SCH,                                   "Interior Load Schedule",   745, 32076, 0,  2, "A fractional schedule of multipliers applied to the Interior Direct Load each hour"
FUEL-METER,        0, EXTERIOR-POWER,                                                       "",   748, 32076, 0,  2, "Hourly energy consumption of misc. energy uses (typically use Loop Process Loads instead)"
FUEL-METER,        0, EXTERIOR-SCH,                                   "Exterior Load Schedule",   747, 32076, 0,  2, "A fractional schedule of multipliers applied to the Exterior Direct Load each hour"
FUEL-METER,        0, METER-REPORT,                                                         "",     0, 32076, 0,  2, ""
STEAM-METER,       0, CAPACITY,                                                             "", 14108, 32077, 0,  2, "Capacity of the meter, defaults to product of Loop Capacity & the meter's Capacity Ratio"
STEAM-METER,       0, CAPACITY-RATIO,                                                       "", 14109, 32077, 0,  2, "If the meter Capacity is undefined, it is set to the product of this and the loop capacity"
STEAM-METER,       0, ENERGY/UNIT,                                                          "", 14110, 32077, 0,  2, "Number of Btus per billing unit for this meter (e.g. 100,000 for therms)"
STEAM-METER,       0, UNIT-INDEX,                                                           "", 14124, 32077, 0,  2, "An integer from the units table that defines the billing unit, used to convert english/metric units"
STEAM-METER,       0, DEM-UNIT-INDEX,                                                       "", 14125, 32077, 0,  2, "An integer from the units table that defines the maximum demand billing unit"
STEAM-METER,       0, SOURCE-SITE-EFF,                                                      "", 14111, 32077, 0,  2, "Fraction of total energy used at the utility source that arrives at the site boundary"
STEAM-METER,       0, INTERIOR-POWER,                                                       "",   731, 32077, 0,  2, "Hourly energy consumption of misc. energy uses (typically use Loop Process Loads instead)"
STEAM-METER,       0, INTERIOR-SCH,                                   "Interior Load Schedule",   730, 32077, 0,  2, "A fractional schedule of multipliers applied to the Interior Direct Load each hour"
STEAM-METER,       0, EXTERIOR-POWER,                                                       "",   733, 32077, 0,  2, "Hourly energy consumption of misc. energy uses (typically use Loop Process Loads instead)"
STEAM-METER,       0, EXTERIOR-SCH,                                   "Exterior Load Schedule",   732, 32077, 0,  2, "A fractional schedule of multipliers applied to the Exterior Direct Load each hour"
STEAM-METER,       0, CIRCULATION-LOOP,                                     "Circulation Loop", 19076, 32078, 0,  2, "Name of the Loop this meter is attached to (Loop Type must be compatible)"
STEAM-METER,       0, HX-HEAD,                                                              "", 14112, 32078, 0,  2, "Pressure drop through the meter's heat exchanger (if one exists)"
STEAM-METER,       0, HX-STATIC-HEAD,                                                       "", 14113, 32078, 0,  2, "Static pressure drop through the meter's heat exchanger (zero for almost all systems)"
STEAM-METER,       0, METER-REPORT,                                                         "",     0, 32077, 0,  2, ""
CHW-METER,         0, CAPACITY,                                                             "", 14116, 32078, 0,  2, "Capacity of the meter, defaults to product of Loop Capacity & the meter's Capacity Ratio"
CHW-METER,         0, CAPACITY-RATIO,                                                       "", 14117, 32078, 0,  2, "If the meter Capacity is undefined, it is set to the product of this and the loop capacity"
CHW-METER,         0, ENERGY/UNIT,                                                          "", 14118, 32078, 0,  2, "Number of Btus per billing unit for this meter (e.g. 100,000 for therms)"
CHW-METER,         0, UNIT-INDEX,                                                           "", 14140, 32078, 0,  2, "An integer from the units table that defines the billing unit, used to convert english/metric units"
CHW-METER,         0, DEM-UNIT-INDEX,                                                       "", 14141, 32078, 0,  2, "An integer from the units table that defines the maximum demand billing unit"
CHW-METER,         0, SOURCE-SITE-EFF,                                                      "", 14119, 32078, 0,  2, "Fraction of total energy used at the utility source that arrives at the site boundary"
CHW-METER,         0, INTERIOR-POWER,                                                       "",   742, 32078, 0,  2, "Hourly energy consumption of misc. energy uses (typically use Loop Process Loads instead)"
CHW-METER,         0, INTERIOR-SCH,                                   "Interior Load Schedule",   741, 32078, 0,  2, "A fractional schedule of multipliers applied to the Interior Direct Load each hour"
CHW-METER,         0, EXTERIOR-POWER,                                                       "",   744, 32078, 0,  2, "Hourly energy consumption of misc. energy uses (typically use Loop Process Loads instead)"
CHW-METER,         0, EXTERIOR-SCH,                                   "Exterior Load Schedule",   743, 32078, 0,  2, "A fractional schedule of multipliers applied to the Exterior Direct Load each hour"
CHW-METER,         0, CIRCULATION-LOOP,                                     "Circulation Loop", 19136, 32078, 0,  2, "Name of the Loop this meter is attached to (Loop Type must be compatible)"
CHW-METER,         0, HX-HEAD,                                                              "", 14145, 32078, 0,  2, "Pressure drop through the meter's heat exchanger (if one exists)"
CHW-METER,         0, HX-STATIC-HEAD,                                                       "", 14146, 32078, 0,  2, "Static pressure drop through the meter's heat exchanger (zero for almost all systems)"
CHW-METER,         0, METER-REPORT,                                                         "",     0, 32078, 0,  2, ""
MASTER-METERS,     0, MSTR-ELEC-METER,                                 "Master Electric Meter", 63008, 32079, 0,  2, "The ultimate default electric meter: all unassigned electricity consumption appears here"
MASTER-METERS,     0, MSTR-FUEL-METER,                                     "Master Fuel Meter", 63027, 32079, 0,  2, "The ultimate default fuel meter: all unassigned fuel consumption appears here"
MASTER-METERS,     0, LIGHT-ELEC-METER,                              "Lighting Electric Meter", 63009, 32079, 0,  2, "All unassigned non-task-lighting electric consumption is assigned to this meter (if defined)"
MASTER-METERS,     0, TASK-ELEC-METER,                                "Task Lt Electric Meter", 63010, 32079, 0,  2, "All unassigned task-lighting electric consumption is assigned to this meter (if defined)"
MASTER-METERS,     0, EQUIP-ELEC-METER,                             "Equipment Electric Meter", 63011, 32079, 0,  2, "All unassigned equipment electric consumption is assigned to this meter (if defined)"
MASTER-METERS,     0, SOURCE-ELEC-METE,                                "Source Electric Meter", 63012, 32079, 0,  2, "All unassigned 'source' electric consumption is assigned to this meter (if defined)"
MASTER-METERS,     0, HEAT-ELEC-METER,                                "Heating Electric Meter", 63013, 32079, 0,  2, "All unassigned space heating electric consumption is assigned to this meter (if defined)"
MASTER-METERS,     0, COOL-ELEC-METER,                                "Cooling Electric Meter", 63014, 32079, 0,  2, "All unassigned space cooling electric consumption is assigned to this meter (if defined)"
MASTER-METERS,     0, HTREJ-ELEC-METER,                             "Heat Rej. Electric Meter", 63015, 32079, 0,  2, "All unassigned heat rejection electric consumption is assigned to this meter (if defined)"
MASTER-METERS,     0, AUX-ELEC-METER,                               "Auxiliary Electric Meter", 63016, 32079, 0,  2, "All unassigned auxiliary electric consumption is assigned to this meter (if defined)"
MASTER-METERS,     0, VENT-ELEC-METER,                            "Ventilation Electric Meter", 63017, 32079, 0,  2, "All unassigned fan electric consumption is assigned to this meter (if defined)"
MASTER-METERS,     0, REFG-ELEC-METER,                          "Refrigeration Electric Meter", 63018, 32079, 0,  2, "All unassigned case refrigeration electric consumption is assigned to this meter (if defined)"
MASTER-METERS,     0, SUPP-ELEC-METER,                           "Supplemental Electric Meter", 63019, 32079, 0,  2, "All unassigned supplemental electric space heating consumption is assigned to this meter"
MASTER-METERS,     0, DHW-ELEC-METER,                              "DHW Heater Electric Meter", 63020, 32079, 0,  2, "All unassigned DHW electric consumption is assigned to this meter"
MASTER-METERS,     0, SOURCE-FUEL-METE,                                    "Source Fuel Meter", 63028, 32079, 0,  2, "All unassigned 'source' fuel consumption is assigned to this meter (if defined)"
MASTER-METERS,     0, HEAT-FUEL-METER,                                    "Heating Fuel Meter", 63029, 32079, 0,  2, "All unassigned space heating fuel consumption is assigned to this meter (if defined)"
MASTER-METERS,     0, COOL-FUEL-METER,                                    "Cooling Fuel Meter", 63030, 32079, 0,  2, "All unassigned space cooling fuel consumption is assigned to this meter (if defined)"
MASTER-METERS,     0, SUPP-FUEL-METER,                               "Supplemental Fuel Meter", 63031, 32079, 0,  2, "All unassigned supplemental space heating fuel consumption is assigned to this meter"
MASTER-METERS,     0, DHW-FUEL-METER,                                  "DHW Heater Fuel Meter", 63032, 32079, 0,  2, "All unassigned DHW fuel consumption is assigned to this meter (if defined)"
MATERIALS-COST,    0, FIRST-COST,                                                           "", 14223, 32080, 0,  2, "First cost for one piece of equipment, not including installation costs"
MATERIALS-COST,    0, INSTALLATION,                                                         "", 14224, 32080, 0,  2, "A multiplier applied to First Cost to obtain the total installation cost per unit"
MATERIALS-COST,    0, CONSUMABLES,                                                          "", 14227, 32080, 0,  2, "Cost of materials consumed during operation, excluding primary fuel ($/unit/hour)"
MATERIALS-COST,    0, MAINTENANCE,                                                          "", 14232, 32080, 0,  2, "Number of hours per year of maintenance that each piece of equipment requires"
MATERIALS-COST,    0, EQUIPMENT-LIFE,                                                       "", 14228, 32080, 0,  2, "Number of operating hours after which the unit must be replaced"
MATERIALS-COST,    0, MINOR-OVHL-INT,                                                       "", 14230, 32080, 0,  2, "Expected operating hours between minor overhauls (must correspond to Minor Overhaul Cost)"
MATERIALS-COST,    0, MINOR-OVHL-COST,                                                      "", 14225, 32080, 0,  2, "Cost for a minor overhaul (must correspond to Minor Overhaul Interval)"
MATERIALS-COST,    0, MAJOR-OVHL-INT,                                                       "", 14231, 32080, 0,  2, "Expected operating hours between major overhauls (must correspond to Major Overhaul"
MATERIALS-COST,    0, MAJOR-OVHL-COST,                                                      "", 14226, 32080, 0,  2, "Cost for a major overhaul (must correspond to Major Overhaul Interval)"
MATERIALS-COST,    0, HOURS-USED,                                                           "", 14229, 32080, 0,  2, "Number of hours that existing equipment has already operated (before analysis)"
PLANT-REPORT,      0, VERIFICATION,                                                         "",     0, 32081, 0,  2, ""
PLANT-REPORT,      0, SUMMARY,                                                              "",     0, 32081, 0,  2, ""
PLANT-REPORT,      0, DUMP-OPTIONS,                                                         "",     0, 32081, 0,  2, ""
PLANT-REPORT,      0, REPORT-FREQUENCY,                                                     "",     0, 32081, 0,  2, ""
PLANT-REPORT,      0, HOURLY-DATA-SAVE,                                                     "",     0, 32081, 0,  2, ""
GROUND-LOOP-HX,    1, TYPE,                                                             "Type", 19150, 32082, 0,  0, "The type of ground-coupled heat-exchanger"
GROUND-LOOP-HX,    1, LOOP-TEMP-SCH,                                                        "", 14505, 32082, 0,  0, "The (hourly) supply temperature of the Ground Loop Heat Exchanger"
GROUND-LOOP-HX,    1, CAPACITY,                                                             "",   665, 32082, 0,  2, "Rated capacity of the Ground Loop Heat Exchanger"
GROUND-LOOP-HX,    1, CAPACITY-RATIO,                                                       "",   664, 32082, 0,  2, "Fraction of the design loop capacity that PowerDOE sizes this heat exchanger to meet"
GROUND-LOOP-HX,    1, CIRCULATION-LOOP,                                      "WLHP or CW Loop", 19149, 32082, 0,  0, "Name of the attached Loop (the Loop's Type must be either WLHP or Condenser Water)"
GROUND-LOOP-HX,    1, HX-PUMP,                                                              "", 14504, 32082, 0,  0, "Name of a Pump that circulates fluid through the ground loop"
GROUND-LOOP-HX,    1, HX-DT,                                           "Heat Exchange Delta T", 14420, 32082, 0,  2, "Design temperature change of the fluid circulating through the ground loop"
GROUND-LOOP-HX,    1, HX-HEAD,                                                              "", 14421, 32082, 0,  2, "The head loss through the ground loop piping at the design flow rate"
GROUND-LOOP-HX,    1, HX-STATIC-HEAD,                                                       "", 14422, 32082, 0,  2, "Static head loss of the ground loop"
GROUND-LOOP-HX,    1, HX-FLOW-CTRL,                                                         "", 14419, 32082, 0,  0, "Type of flow through the ground loop heat exchanger"
GROUND-LOOP-HX,    1, HX-MIN-FLOW,                                                          "", 14423, 32082, 0,  2, "Minimum allowable fraction of the design flow rate through the ground loop"
GROUND-LOOP-HX,    1, HX-MAX-FLOW,                                                          "", 14424, 32082, 0,  2, "Ratio of the maximum allowable flow rate to the design flow rate"
GROUND-LOOP-HX,    1, COST-DATA,                                                            "",     0, 32082, 0,  2, ""
GROUND-LOOP-HX,    1, EQUIPMENT-REPORTS,                                                    "",     0, 32082, 0,  2, ""
GROUND-LOOP-HX,    1, PICTURE,                                                              "",     0, 32082, 0,  2, ""
GROUND-LOOP-HX,    1, DRAWING,                                                              "",     0, 32082, 0,  2, ""
GROUND-LOOP-HX,    2, TYPE,                                                             "Type", 19150, 32082, 0,  0, "The type of ground-coupled heat-exchanger"
GROUND-LOOP-HX,    2, CONFIGURATION,                                           "Configuration", 14475, 32082, 0,  0, "Configuration options vary by Ground Loop Heat Exchanger Type"
GROUND-LOOP-HX,    2, CAPACITY,                                                             "",   665, 32082, 0,  2, "Rated capacity of the Ground Loop Heat Exchanger"
GROUND-LOOP-HX,    2, CAPACITY-RATIO,                                                       "",   664, 32082, 0,  2, "Fraction of the design loop capacity that PowerDOE sizes this heat exchanger to meet"
GROUND-LOOP-HX,    2, DEPTH,                                                           "Depth", 14476, 32082, 0,  2, "Distance between the ground surface and the bottom of the trench"
GROUND-LOOP-HX,    2, SPACING,                                                       "Spacing", 14388, 32082, 0,  2, "Distance between the centerlines of each trench"
GROUND-LOOP-HX,    2, PIPE-OUTSIDE-DIA,                                "Pipe Outside Diameter", 14325, 32082, 0,  2, "Outside diameter of the U-tube or pipe"
GROUND-LOOP-HX,    2, PIPE-INSIDE-DIA,                                  "Pipe Inside Diameter", 14471, 32082, 0,  2, "Inside diameter of the U-tube or pipe"
GROUND-LOOP-HX,    2, U-TUBE-LEG-SEP,                                  "U-Tube Leg Separation", 14390, 32082, 0,  2, "Distance between the outer surfaces of the tubes"
GROUND-LOOP-HX,    2, PIPE-COND,                                           "Pipe Conductivity", 14472, 32082, 0,  2, "Thermal conductivity of the pipe"
GROUND-LOOP-HX,    2, FIELD-MULTIPLIER,                                                     "", 14391, 32082, 0,  2, "Number of identical well fields"
GROUND-LOOP-HX,    2, REF-GRND-TEMP,                                                        "", 14447, 32082, 0,  2, "for horiz loop: undisturbed mean ground T;for vert wells: the undisturbed far-field ground T"
GROUND-LOOP-HX,    2, GRND-DIFFUSIVITY,                                                     "", 14448, 32082, 0,  2, "Thermal diffusivity of the ground"
GROUND-LOOP-HX,    2, GRND-COND,                                                            "", 14449, 32082, 0,  2, "Thermal conductivity of the ground"
GROUND-LOOP-HX,    2, NUM-OF-YEARS,                                                         "", 14499, 32082, 0,  2, "Number of years of previous operation (before the simulation time period)"
GROUND-LOOP-HX,    2, DESIGN-HEAT-DAY,                                                      "", 14451, 32082, 0,  2, "Julian heating design day (used for design calculations)"
GROUND-LOOP-HX,    2, DESIGN-COOL-DAY,                                                      "", 14452, 32082, 0,  2, "Julian cooling design day (used for design calculations)"
GROUND-LOOP-HX,    2, DESIGN-HEAT-LOAD,                                                     "", 14402, 32082, 0,  2, "Hourly heat flow rate into the ground on the heating design day"
GROUND-LOOP-HX,    2, DESIGN-COOL-LOAD,                                                     "", 14457, 32082, 0,  2, "Hourly heat flow rate into the ground on the cooling design day"
GROUND-LOOP-HX,    2, CIRCULATION-LOOP,                                            "WLHP Loop", 19149, 32082, 0,  0, "Name of the attached Loop (the Loop's Type must be WLHP)"
GROUND-LOOP-HX,    2, HX-PUMP,                                                              "", 14504, 32082, 0,  0, "Name of a Pump that circulates fluid through the ground loop"
GROUND-LOOP-HX,    2, HX-DT,                                           "Heat Exchange Delta T", 14420, 32082, 0,  2, "Design temperature change of the fluid circulating through the ground loop"
GROUND-LOOP-HX,    2, HX-HEAD,                                                              "", 14421, 32082, 0,  2, "The head loss through the ground loop piping at the design flow rate"
GROUND-LOOP-HX,    2, HX-STATIC-HEAD,                                                       "", 14422, 32082, 0,  2, "Static head loss of the ground loop"
GROUND-LOOP-HX,    2, HX-FLOW-CTRL,                                                         "", 14419, 32082, 0,  0, "Type of flow through the ground loop heat exchanger"
GROUND-LOOP-HX,    2, HX-MIN-FLOW,                                                          "", 14423, 32082, 0,  2, "Minimum allowable fraction of the design flow rate through the ground loop"
GROUND-LOOP-HX,    2, HX-MAX-FLOW,                                                          "", 14424, 32082, 0,  2, "Ratio of the maximum allowable flow rate to the design flow rate"
GROUND-LOOP-HX,    2, COST-DATA,                                                            "",     0, 32082, 0,  2, ""
GROUND-LOOP-HX,    2, EQUIPMENT-REPORTS,                                                    "",     0, 32082, 0,  2, ""
GROUND-LOOP-HX,    2, PICTURE,                                                              "",     0, 32082, 0,  2, ""
GROUND-LOOP-HX,    2, DRAWING,                                                              "",     0, 32082, 0,  2, ""
GROUND-LOOP-HX,    3, TYPE,                                                             "Type", 19150, 32082, 0,  0, "The type of ground-coupled heat-exchanger"
GROUND-LOOP-HX,    3, CONFIGURATION,                                           "Configuration", 14475, 32082, 0,  0, "Configuration options vary by Ground Loop Heat Exchanger Type"
GROUND-LOOP-HX,    3, CAPACITY,                                                             "",   665, 32082, 0,  2, "Rated capacity of the Ground Loop Heat Exchanger"
GROUND-LOOP-HX,    3, CAPACITY-RATIO,                                                       "",   664, 32082, 0,  2, "Fraction of the design loop capacity that PowerDOE sizes this heat exchanger to meet"
GROUND-LOOP-HX,    3, DEPTH,                                                           "Depth", 14476, 32082, 0,  2, "Distance between the ground surface and the bottom of the trench"
GROUND-LOOP-HX,    3, SPACING,                                                       "Spacing", 14388, 32082, 0,  2, "Distance between the centerlines of each trench"
GROUND-LOOP-HX,    3, TRENCH-LENGTH,                                           "Trench Length", 14478, 32082, 0,  2, "The length of each trench"
GROUND-LOOP-HX,    3, PIPE-OUTSIDE-DIA,                                "Pipe Outside Diameter", 14325, 32082, 0,  2, "Outside diameter of the U-tube or pipe"
GROUND-LOOP-HX,    3, PIPE-INSIDE-DIA,                                  "Pipe Inside Diameter", 14471, 32082, 0,  2, "Inside diameter of the U-tube or pipe"
GROUND-LOOP-HX,    3, PIPE-COND,                                           "Pipe Conductivity", 14472, 32082, 0,  2, "Thermal conductivity of the pipe"
GROUND-LOOP-HX,    3, TRENCH-NUMBER,                                                        "", 14479, 32082, 0,  2, "The number of identical trenches"        
GROUND-LOOP-HX,    3, REF-GRND-TEMP,                                                        "", 14447, 32082, 0,  2, "for horiz loop: undisturbed mean ground T;for vert wells: the undisturbed far-field ground T"
GROUND-LOOP-HX,    3, GRND-DIFFUSIVITY,                                                     "", 14448, 32082, 0,  2, "Thermal diffusivity of the ground"
GROUND-LOOP-HX,    3, GRND-COND,                                                            "", 14449, 32082, 0,  2, "Thermal conductivity of the ground"
GROUND-LOOP-HX,    3, NUM-OF-YEARS,                                                         "", 14499, 32082, 0,  2, "Number of years of previous operation (before the simulation time period)"
GROUND-LOOP-HX,    3, GRND-YEAR-SWING,                        "Annual Surface Soil Temp Swing", 14459, 32082, 0,  2, "The annual surface soil temperature swing"
GROUND-LOOP-HX,    3, GRND-PHASE-CONST,                                                     "", 14460, 32082, 0,  2, "The phase constant (days) in ground temperature swing"
GROUND-LOOP-HX,    3, PIPE-VERT-SEP,                                "Pipe Vertical Separation", 14480, 32082, 0,  2, "Vertical distance between centerlines of pipes (for pipes arranged vertically)"
GROUND-LOOP-HX,    3, PIPE-HORIZ-SEP,                             "Pipe Horizontal Separation", 14481, 32082, 0,  2, "Horizontal distance between centerlines of pipes (for pipes arranged horizontally)"
GROUND-LOOP-HX,    3, DESIGN-HEAT-DAY,                                                      "", 14451, 32082, 0,  2, "Julian heating design day (used for design calculations)"
GROUND-LOOP-HX,    3, DESIGN-COOL-DAY,                                                      "", 14452, 32082, 0,  2, "Julian cooling design day (used for design calculations)"
GROUND-LOOP-HX,    3, DESIGN-HEAT-LOAD,                                                     "", 14402, 32082, 0,  2, "Hourly heat flow rate into the ground on the heating design day"
GROUND-LOOP-HX,    3, DESIGN-COOL-LOAD,                                                     "", 14457, 32082, 0,  2, "Hourly heat flow rate into the ground on the cooling design day"
GROUND-LOOP-HX,    3, CIRCULATION-LOOP,                                            "WLHP Loop", 19149, 32082, 0,  0, "Name of the attached Loop (the Loop's Type must be WLHP)"
GROUND-LOOP-HX,    3, HX-PUMP,                                                              "", 14504, 32082, 0,  0, "Name of a Pump that circulates fluid through the ground loop"
GROUND-LOOP-HX,    3, HX-DT,                                           "Heat Exchange Delta T", 14420, 32082, 0,  2, "Design temperature change of the fluid circulating through the ground loop"
GROUND-LOOP-HX,    3, HX-HEAD,                                                              "", 14421, 32082, 0,  2, "The head loss through the ground loop piping at the design flow rate"
GROUND-LOOP-HX,    3, HX-STATIC-HEAD,                                                       "", 14422, 32082, 0,  2, "Static head loss of the ground loop"
GROUND-LOOP-HX,    3, HX-FLOW-CTRL,                                                         "", 14419, 32082, 0,  0, "Type of flow through the ground loop heat exchanger"
GROUND-LOOP-HX,    3, HX-MIN-FLOW,                                                          "", 14423, 32082, 0,  2, "Minimum allowable fraction of the design flow rate through the ground loop"
GROUND-LOOP-HX,    3, HX-MAX-FLOW,                                                          "", 14424, 32082, 0,  2, "Ratio of the maximum allowable flow rate to the design flow rate"
GROUND-LOOP-HX,    3, COST-DATA,                                                            "",     0, 32082, 0,  2, ""
GROUND-LOOP-HX,    3, EQUIPMENT-REPORTS,                                                    "",     0, 32082, 0,  2, ""
GROUND-LOOP-HX,    3, PICTURE,                                                              "",     0, 32082, 0,  2, ""
GROUND-LOOP-HX,    3, DRAWING,                                                              "",     0, 32082, 0,  2, ""
GROUND-LOOP-HX,    4, TYPE,                                                             "Type", 19150, 32082, 0,  0, "The type of ground-coupled heat-exchanger"
GROUND-LOOP-HX,    4, CONFIGURATION,                                           "Configuration", 14475, 32082, 0,  0, "Configuration options vary by Ground Loop Heat Exchanger Type"
GROUND-LOOP-HX,    4, CAPACITY,                                                             "",   665, 32082, 0,  2, "Rated capacity of the Ground Loop Heat Exchanger"
GROUND-LOOP-HX,    4, CAPACITY-RATIO,                                                       "",   664, 32082, 0,  2, "Fraction of the design loop capacity that PowerDOE sizes this heat exchanger to meet"
GROUND-LOOP-HX,    4, DEPTH,                                                           "Depth", 14476, 32082, 0,  2, "Distance between the ground surface and the bottom of the trench"
GROUND-LOOP-HX,    4, SPACING,                                                       "Spacing", 14388, 32082, 0,  2, "Distance between the centerlines of each trench"
GROUND-LOOP-HX,    4, TRENCH-LENGTH,                                           "Trench Length", 14478, 32082, 0,  2, "The length of each trench"
GROUND-LOOP-HX,    4, PIPE-OUTSIDE-DIA,                                "Pipe Outside Diameter", 14325, 32082, 0,  2, "Outside diameter of the U-tube or pipe"
GROUND-LOOP-HX,    4, PIPE-INSIDE-DIA,                                  "Pipe Inside Diameter", 14471, 32082, 0,  2, "Inside diameter of the U-tube or pipe"
GROUND-LOOP-HX,    4, PIPE-COND,                                           "Pipe Conductivity", 14472, 32082, 0,  2, "Thermal conductivity of the pipe"
GROUND-LOOP-HX,    4, TRENCH-NUMBER,                                                        "", 14479, 32082, 0,  2, "The number of identical trenches"
GROUND-LOOP-HX,    4, REF-GRND-TEMP,                                                        "", 14447, 32082, 0,  2, "for horiz loop: undisturbed mean ground T;for vert wells: the undisturbed far-field ground T"
GROUND-LOOP-HX,    4, GRND-DIFFUSIVITY,                                                     "", 14448, 32082, 0,  2, "Thermal diffusivity of the ground"
GROUND-LOOP-HX,    4, GRND-COND,                                                            "", 14449, 32082, 0,  2, "Thermal conductivity of the ground"
GROUND-LOOP-HX,    4, NUM-OF-YEARS,                                                         "", 14499, 32082, 0,  2, "Number of years of previous operation (before the simulation time period)"
GROUND-LOOP-HX,    4, GRND-YEAR-SWING,                        "Annual Surface Soil Temp Swing", 14459, 32082, 0,  2, "The annual surface soil temperature swing"
GROUND-LOOP-HX,    4, GRND-PHASE-CONST,                                                     "", 14460, 32082, 0,  2, "The phase constant (days) in ground temperature swing"
GROUND-LOOP-HX,    4, SLINKY-DIAMETER,                                     "'Slinky' Diameter", 14492, 32082, 0,  2, "The diameter of the slinky coil"
GROUND-LOOP-HX,    4, SLINKY-PITCH,                                           "'Slinky' Pitch", 14493, 32082, 0,  2, "The pitch of the slinky coil"
GROUND-LOOP-HX,    4, DESIGN-HEAT-DAY,                                                      "", 14451, 32082, 0,  2, "Julian heating design day (used for design calculations)"
GROUND-LOOP-HX,    4, DESIGN-COOL-DAY,                                                      "", 14452, 32082, 0,  2, "Julian cooling design day (used for design calculations)"
GROUND-LOOP-HX,    4, DESIGN-HEAT-LOAD,                                                     "", 14402, 32082, 0,  2, "Hourly heat flow rate into the ground on the heating design day"
GROUND-LOOP-HX,    4, DESIGN-COOL-LOAD,                                                     "", 14457, 32082, 0,  2, "Hourly heat flow rate into the ground on the cooling design day"
GROUND-LOOP-HX,    4, CIRCULATION-LOOP,                                            "WLHP Loop", 19149, 32082, 0,  0, "Name of the attached Loop (the Loop's Type must be WLHP)"
GROUND-LOOP-HX,    4, HX-PUMP,                                                              "", 14504, 32082, 0,  0, "Name of a Pump that circulates fluid through the ground loop"
GROUND-LOOP-HX,    4, HX-DT,                                           "Heat Exchange Delta T", 14420, 32082, 0,  2, "Design temperature change of the fluid circulating through the ground loop"
GROUND-LOOP-HX,    4, HX-HEAD,                                                              "", 14421, 32082, 0,  2, "The head loss through the ground loop piping at the design flow rate"
GROUND-LOOP-HX,    4, HX-STATIC-HEAD,                                                       "", 14422, 32082, 0,  2, "Static head loss of the ground loop"
GROUND-LOOP-HX,    4, HX-FLOW-CTRL,                                                         "", 14419, 32082, 0,  0, "Type of flow through the ground loop heat exchanger"
GROUND-LOOP-HX,    4, HX-MIN-FLOW,                                                          "", 14423, 32082, 0,  2, "Minimum allowable fraction of the design flow rate through the ground loop"
GROUND-LOOP-HX,    4, HX-MAX-FLOW,                                                          "", 14424, 32082, 0,  2, "Ratio of the maximum allowable flow rate to the design flow rate"
GROUND-LOOP-HX,    4, COST-DATA,                                                            "",     0, 32082, 0,  2, ""
GROUND-LOOP-HX,    4, EQUIPMENT-REPORTS,                                                    "",     0, 32082, 0,  2, ""
GROUND-LOOP-HX,    4, PICTURE,                                                              "",     0, 32082, 0,  2, ""
GROUND-LOOP-HX,    4, DRAWING,                                                              "",     0, 32082, 0,  2, ""
LUMINAIRE-TYPE,    0, DESCRIPTION,                                               "Description", 13538, 32083, 0, 64, "Description of the Type of Luminaire (the 'luminaire' includes all lamps and ballasts)"
LUMINAIRE-TYPE,    0, PICTURE,                                                              "",     0, 32083, 0,  2, ""
LUMINAIRE-TYPE,    0, DRAWING,                                                              "",     0, 32083, 0,  2, ""
LUMINAIRE-TYPE,    0, CU-RCR-1,                                          "Room Cavity Ratio 1", 13546, 32083, 0,  2, "Fraction of the lamp/luminaire light output that reaches the Workplane Height"
LUMINAIRE-TYPE,    0, CU-RCR-5,                                          "Room Cavity Ratio 5", 13555, 32083, 0,  2, "Fraction of the lamp/luminaire light output that reaches the Workplane Height"
LUMINAIRE-TYPE,    0, CU-RCR-10,                                        "Room Cavity Ratio 10", 13564, 32083, 0,  2, "Fraction of the lamp/luminaire light output that reaches the Workplane Height"
LUMINAIRE-TYPE,    0, NO-OF-LAMPS,                             "Number of Lamps per Luminaire", 13539, 32083, 0,  0, "Number of lamps in the luminaire (the 'luminaire' includes all lamps and ballasts)"
LUMINAIRE-TYPE,    0, ACCEPT-LAMP-SIZE,                                 "Acceptable Lamp Size", 13540, 32083, 0,  0, "Use to avoid inappropriate lamps in the luminaire (with inaccurate Coefficients Of Utilization)"
LUMINAIRE-TYPE,    0, ACCEPT-CONFIG,                                "Acceptable Configuration", 13541, 32083, 0,  0, "The Lighting subsystem can have any one of these three Luminaire Configurations"
LUMINAIRE-TYPE,    0, LUM-MAINT-CAT,                                    "Maintenance Category", 13542, 32083, 0,  0, "Used to calculate decrease in light output due to dirt accumulation"
LUMINAIRE-TYPE,    0, OPERATING-ATMOS,                                  "Operating Atmosphere", 13543, 32083, 0,  0, "Used to calculate decrease in light output due to dirt accumulation"
LUMINAIRE-TYPE,    0, CLEANING-CYCLE,                                   "Cleaning Cycle (yrs)", 13544, 32083, 0,  2, "Used to calculate decrease in light output due to dirt accumulation"
LIGHTING-SYSTEM,   0, DESCRIPTION,                                                          "", 14528, 32084, 0,  2, "A description of the Lighting System"
LIGHTING-SYSTEM,   0, PICTURE,                                                              "",     0, 32084, 0,  2, ""
LIGHTING-SYSTEM,   0, DRAWING,                                                              "",     0, 32084, 0,  2, ""
LIGHTING-SYSTEM,   0, LUMINAIRE-TYPE,                                         "Luminaire Type", 19039, 32084, 0,  0, "Name of luminaire in the llighting system; includes lamps and ballasts"
LIGHTING-SYSTEM,   0, LAMP-TYPE,                                                   "Lamp Type", 19042, 32084, 0,  0, "Name of the lamp type in the lighting system; form the library or custom built"
LIGHTING-SYSTEM,   0, LTG-CALC-METHOD,                  "Method of Lighting Power Calculation", 12308, 32084, 0,  0, "Whether you are using a Luminaire Type or gross power consumption for lighting calculations"
LIGHTING-SYSTEM,   0, BALLAST-TYPE,                                                         "", 19047, 32084, 0,  0, "Type of ballast"
LIGHTING-SYSTEM,   0, COEF-OF-UTIL,                               "Coefficient of Utilization", 12314, 32084, 0,  2, "Fraction of light output from lamp/luminaire combination that reaches the Workplane Height"
LIGHTING-SYSTEM,   0, RADIATIVE-FRAC,                                                       "",     0, 32084, 0,  2, ""
LIGHTING-SYSTEM,   0, TOT-LAMP-LUMENS,                                    "Total Light Output", 12316, 32084, 0,  2, "Total number of lumens produced by all lamps in the lighting subsystem (at 70% of lamp life)"
LIGHTING-SYSTEM,   0, TOT-POWER-INPUT,                                     "Total Power Input", 12311, 32084, 0,  2, "Total electrical input power for the Lighting System at full power (also called 'active power')"
LIGHTING-SYSTEM,   0, LUMINAIRE-CONFIG,                                                     "", 13583, 32084, 0,  0, "Used to calculate thermal effects that influence lamp input power and light output"
LAMP-TYPE,         0, DESCRIPTION,                                                          "", 14529, 32085, 0,  2, "Description of the lamp type"
LAMP-TYPE,         0, PICTURE,                                                              "",     0, 32085, 0,  2, ""
LAMP-TYPE,         0, DRAWING,                                                              "",     0, 32085, 0,  2, ""
LAMP-TYPE,         0, CATEGORY,                                                     "Category", 13182, 32085, 0,  0, "The type of Lamp"
LAMP-TYPE,         0, INIT-LUMEN-OUT,                                     "Rated Light Output", 12296, 32085, 0,  2, "Lamp light output; after seasoning the lamp for 100 hours"
LAMP-TYPE,         0, POWER-INPUT,                                               "Power Input",  1000, 32085, 0,  2, "Nominal lamp power consumption"
LAMP-TYPE,         0, LUMEN-DEPREC,                                             "Lumen Deprec",  1001, 32085, 0,  2, "Ratio of the lamp's light output at 70% of its rated life to its initial light output"
LAMP-TYPE,         0, SIZE,                                                             "Size", 13183, 32085, 0,  0, "Must match Luminaire's Accepts Lamp Size; forces compatible luminaire/lamp combinations"
COMPONENT-COST,    0, UNIT-NAME,                                                   "Unit Name", 14245, 32086, 0, 16, "Description of the type of building material that this set of component costs applies to"
COMPONENT-COST,    0, NUMBER-OF-UNITS,                                                      "", 14246, 32086, 0,  2, "A multiplier on all of the costs (for this set of component costs)"
COMPONENT-COST,    0, FIRST-COST,                                                           "", 14235, 32086, 0,  2, "Initial cost per unit (see Number of Units), excluding installation costs"
COMPONENT-COST,    0, INSTALL-COST,                                                         "", 14236, 32086, 0,  2, "Installation cost per unit, excluding the First Cost"
COMPONENT-COST,    0, ANNUAL-COST,                                                          "", 14239, 32086, 0,  2, "Annual maintenance (labor) and consumables (materials) cost per unit"
COMPONENT-COST,    0, COMPONENT-LIFE,                                                       "", 14240, 32086, 0,  2, "Expected life of the component: i.e., frequency that First- & Installation-Costs are incurred"
COMPONENT-COST,    0, MIN-OVHL-INT,                                                         "", 14242, 32086, 0,  2, "Expected time between minor overhauls, i.e frequency Minor Overhaul Costs are incurred"
COMPONENT-COST,    0, MIN-OVHL-COST,                                                        "", 14237, 32086, 0,  2, "Cost of a minor overhaul, per unit"
COMPONENT-COST,    0, MAJ-OVHL-INT,                                                         "", 14243, 32086, 0,  2, "Expected time between minor overhauls, i.e frequency Major Overhaul Costs are incurred"
COMPONENT-COST,    0, MAJ-OVHL-COST,                                                        "", 14238, 32086, 0,  2, "Cost of a major overhaul, per unit"
BASELINE,          0, FIRST-COST,                                                           "", 14147, 32087, 0,  2, "Total baseline initial costs, including installation (zero for existing, unmodified buildings)"
BASELINE,          0, REPLACE-COST,                                                         "", 14148, 32087, 0,  2, "Present value of the life-cycle baseline replacement costs"
BASELINE,          0, OPERATIONS-COST,                                                      "",   749, 32087, 0,  2, "Present Value of the baseline operations costs for each year of the project"
BASELINE,          0, ENERGY-COST,                                                          "",   750, 32087, 0,  2, "Present Value of the baseline energy cost for each year of the project"
BASELINE,          0, ENERGY-USE-SITE,                                                      "", 14149, 32087, 0,  2, "Baseline annual energy use at the site (i.e., at the building boundary)"
BASELINE,          0, ENERGY-USE-SRC,                                                       "", 14150, 32087, 0,  2, "Baseline source annual energy use: Site Energy use divided by (transmission) loss fraction"
BASELINE,          0, DISCOUNT-RATE,                                                        "", 14151, 32087, 0,  2, "The discount rate that PowerDOE uses in the life-cycle cost calculations"
BASELINE,          0, LABOR-INFLTN,                                                         "", 14152, 32087, 0,  2, "Annual % increase in labor costs (above the inflation rate), applies to maintenance labor only"
BASELINE,          0, MATERIALS-INFLTN,                                                     "", 14153, 32087, 0,  2, "Annual % increase in materials costs (above inflation), applies to non-maintenance labor also"
BASELINE,          0, PROJECT-LIFE,                                                         "", 14154, 32087, 0,  2, "Period of time over which PowerDOE calculates life-cycle costs"
BASELINE,          0, LABOR,                                                                "", 14155, 32087, 0,  2, "Cost of maintenance labor, in dollars per hour"
BASELINE,          0, SITE-FACTOR,                                                          "", 14156, 32087, 0,  2, "Multiplier on the Maintenance and Consumables costs (for different locations in a siting)"
ECONOMICS-REPORT,  0, VERIFICATION,                                                         "",     0, 32088, 0,  2, ""
ECONOMICS-REPORT,  0, SUMMARY,                                                              "",     0, 32088, 0,  2, ""
ECONOMICS-REPORT,  0, DUMP-OPTIONS,                                                         "",     0, 32088, 0,  2, ""
ECONOMICS-REPORT,  0, REPORT-FREQUENCY,                                                     "",     0, 32088, 0,  2, ""
ECONOMICS-REPORT,  0, HOURLY-DATA-SAVE,                                                     "",     0, 32088, 0,  2, ""
UTILITY-RATE,      0, TYPE,                                                "Utility Rate Type", 12300, 32089, 0,  0, "Determines which fuel or energy type is being valued"
UTILITY-RATE,      0, ELEC-METERS,                                                          "", 63097, 32089, 0,  2, "Meters assigned to this utility rate (must be of compatible Type)"
UTILITY-RATE,      0, FUEL-METERS,                                                          "", 63097, 32089, 0,  2, "Meters assigned to this utility rate (must be of compatible Type)"
UTILITY-RATE,      0, STEAM-METERS,                                                         "", 63097, 32089, 0,  2, "Meters assigned to this utility rate (must be of compatible Type)"
UTILITY-RATE,      0, CHW-METERS,                                                           "", 63097, 32089, 0,  2, "Meters assigned to this utility rate (must be of compatible Type)"
UTILITY-RATE,      0, BILLING-DAYS,                                                         "", 63103, 32089, 0,  2, "Last day of the utility billing period (for each of the twelve months of the year)"
UTILITY-RATE,      0, ENERGY-QUALS,                                                         "", 12304,  3079, 0,  2, "Minimum monthly energy usage that determines if this rate applies"
UTILITY-RATE,      0, DEMAND-QUALS,                                                         "", 12305,  3075, 0,  2, "Minimum demand that will be billed (used only if Use Minimum Rate Qualifiers = Yes)"
UTILITY-RATE,      0, QUAL-SCH,                                                             "", 12447,  3079, 0,  0, "Name of schedule that defines the period(s) during which this utility rate may be used"
UTILITY-RATE,      0, SCH-FLAG,                                          "Schedule Flag Value", 12448, 32089, 0,  2, "Flag value in the Qualification Schedule that activates this Utility Rate"
UTILITY-RATE,      0, USE-MIN-QUALS,                                                        "", 12412,  3079, 0,  0, "Whether there is a minimum charge calculation for either energy or demand"
UTILITY-RATE,      0, QUALIFY-RATE,                                                         "", 12446,  3079, 0,  0, "Defines how energy & demand qualifiers are used to determine if this rate qualifies for use"
UTILITY-RATE,      0, MONTH-CHGS,                                                           "", 11546, 32089, 0,  2, "A fixed monthly charge added to each billing cycle (for each month)"
UTILITY-RATE,      0, ENERGY-CHG,                                                           "", 12319, 32089, 0,  2, "an energy charge that is constant with time of use and fuel Type"
UTILITY-RATE,      0, ENERGY-CHG-SCH,                                                       "", 12320, 32089, 0,  0, "A schedule that defines Energy Cost Adjustment charges (on an hourly basis)"
UTILITY-RATE,      0, ENERGY-COST-ADJS,                                                     "", 11532, 32089, 0,  2, "Energy cost adjustment factor for each billing period: multiplied by total monthly energy use"
UTILITY-RATE,      0, ENERGY-ADJ-SCH,                                                       "", 11532, 32089, 0,  2, ""
UTILITY-RATE,      0, DEMAND-CHGS,                                                          "", 11528,  3075, 0,  2, "Dollars per peak unit:if less than 12 entries, the last one applies to all remaining billing periods"
UTILITY-RATE,      0, DEMAND-WINDOW,                                                        "", 12346, 32089, 0,  0, "Length of the time window in which peak demand is calculated"
UTILITY-RATE,      0, DEMAND-RATCHETS,                                                      "", 11530,  3075, 0,  2, "Names of ratchets that apply to this block charge"
UTILITY-RATE,      0, BLOCK-CHARGES,                                                        "", 12450,  3074, 0,  2, "You can assign up to 20 block charges to the current utility rate"
UTILITY-RATE,      0, POWER-FACTOR,                                                         "", 12439, 32089, 0,  2, "Fraction of peak kVA due to real power"
UTILITY-RATE,      0, EXCESS-KVAR-FRAC,                                                     "", 12440, 32089, 0,  2, "Fraction of real kW above which a charge is levied (I.e., Excess kVAR Charge applies)"
UTILITY-RATE,      0, EXCESS-KVAR-CHG,                                                      "", 12441, 32089, 0,  2, "Charge for excess reactive demand ($/kVAR)"
UTILITY-RATE,      0, ESCALATION,                                                           "", 12318, 32089, 0,  2, "Annual rate (%) of real price escalation (above inflation rate) for life-cycle cost calculations"
UTILITY-RATE,      0, MIN-MON-CHGS,                                                         "", 11531, 32089, 0,  2, "Minimum fixed charge for a billing period (for each month)"
UTILITY-RATE,      0, MIN-MON-DEM-CHGS,                                                     "", 63104, 32089, 0,  2, "Minimum charge, based on peak demand, for a billing period (for each month)"
UTILITY-RATE,      0, MIN-MON-RATCHETS,                                                     "", 63098,  3075, 0,  2, "Names of ratchets that modify demand for minimum monthly demand charges"
UTILITY-RATE,      0, RATE-LIMITATION,                                                      "", 12413, 32089, 0,  2, "Maximum effective charge ($ per unit) assessed on a utility or fuel for any month"
UTILITY-RATE,      0, PCT-TAX-BLOCKS,                                                       "", 11535,  3078, 0,  2, "Maximum size of the block of money upon which a tax will be levied (on a % basis)"
UTILITY-RATE,      0, PCT-TAXES,                                                 "Percent Tax", 63101,  3078, 0,  2, "The tax in % (up to 3 - corresponding to blocks in Percent Tax Data Block Size)"
UTILITY-RATE,      0, PCT-TAXES-APPLY,                                                      "", 12744,  3078, 0,  2, "The categories of charges upon which taxes are levied"
UTILITY-RATE,      0, UNIT-TAX-BLOCKS,                                                      "", 11536,  3078, 0,  2, "Maximum size of the block of energy upon which a tax is levied (per energy unit basis)"
UTILITY-RATE,      0, UNIT-TAXES,                                                   "Unit Tax", 63102,  3078, 0,  2, "Tax in $/energy unit  (up to 3 - corresponding to Unit Tax Data Block Size)"
UTILITY-RATE,      0, PCT-SRCHG-BLOCKS,                                                     "", 11533, 32089, 0,  2, "Maximum size of the block of money upon which a surcharge will be levied (on a % basis)"
UTILITY-RATE,      0, PCT-SRCHGS,                                          "Percent Surcharge", 63099, 32089, 0,  2, "Surcharge in % (up to 3 - corresponding to blocks in Percent Surcharge Data Block Size)"
UTILITY-RATE,      0, PCT-SRCHGS-APPLY,                                                     "", 12729, 32089, 0,  2, "The categories of charges upon which surcharges are levied"
UTILITY-RATE,      0, UNIT-SRCHG-BLOCK,                                                     "", 11534, 32089, 0,  2, "Maximum size of block of energy on which a surcharge is levied (per energy unit basis)"
UTILITY-RATE,      0, UNIT-SRCHGS,                                            "Unit Surcharge", 63102, 32089, 0,  2, "Surcharge in $/energy unit  (up to 3 - corresponding to Unit Surcharge Data Block Size)"
UTILITY-RATE,      0, DEMAND-INTERVAL,                                                      "", 14416, 32089, 0,  2, "Number of minutes used for demand calculation"
BLOCK-CHARGE,      0, BLOCK-SCH,                                                            "", 12452,  3074, 0,  0, "Name of schedule that defines the period over which energy or demand is accumulated"
BLOCK-CHARGE,      0, SCH-FLAG,                                          "Schedule Flag Value", 12453,  3074, 0,  2, "Flag value in the Block Schedule that indicates when this block charge is active"
BLOCK-CHARGE,      0, DEMAND-RATCHETS,                                                      "", 12500,  3074, 0,  2, "Names of up to 15 ratchets that modify the billing demands for all demand charges"
BLOCK-CHARGE,      0, TOU-SEASON-LINKS,                                                     "", 12454,  3074, 0,  0, "Name(s) of other block charge(s) that share the same billing period"
BLOCK-CHARGE,      0, BLOCKS-ARE,                                                           "", 12451,  3074, 0,  0, "Whether energy blocks are defined as cumulative or incremental"
BLOCK-CHARGE,      0, BLOCK1-TYPE,                                                          "", 12499,  3074, 0,  0, "Type of block calculation; specifies the basis of block charges for this block"
BLOCK-CHARGE,      0, BLOCKS-1,                                       "Size of Block 1, Step ", 11541, 11541, 0,  2, "The step size of the block (same units as the block Type); maximum of ten"
BLOCK-CHARGE,      0, COSTS-1,                                        "Cost of Block 1, Step ", 11540, 11540, 0,  2, "Cost per unit for the energy or demand falling within this block"
BLOCK-CHARGE,      0, LIMITS-1,                                                             "", 11539,  3074, 0,  0, "Maximum limit for this block (if Block Type is KWH/KW or KWH/KW-Limitsum); 0=no limit"
BLOCK-CHARGE,      0, BLOCK2-TYPE,                                                          "", 12499,  3074, 0,  0, "Maximum limit for this block (if Block Type is KWH/KW or KWH/KW-Limitsum); 0=no limit"
BLOCK-CHARGE,      0, BLOCKS-2,                                       "Size of Block 2, Step ", 11541,  3074, 0,  2, "The step size of the block (same units as the block Type); maximum of ten"
BLOCK-CHARGE,      0, COSTS-2,                                        "Cost of Block 2, Step ", 11540,  3074, 0,  2, "Cost per unit for the energy or demand falling within this block"
BLOCK-CHARGE,      0, LIMITS-2,                                                             "", 11539,  3074, 0,  0, "Maximum limit for this block (if Block Type is KWH/KW or KWH/KW-Limitsum); 0=no limit"
BLOCK-CHARGE,      0, BLOCK3-TYPE,                                                          "", 12499,  3074, 0,  0, "Type of block calculation; specifies the basis of block charges for this block"
BLOCK-CHARGE,      0, BLOCKS-3,                                       "Size of Block 3, Step ", 11541,  3074, 0,  2, "The step size of the block (same units as the block Type); maximum of ten"
BLOCK-CHARGE,      0, COSTS-3,                                        "Cost of Block 3, Step ", 11540,  3074, 0,  2, "Cost per unit for the energy or demand falling within this block"
BLOCK-CHARGE,      0, LIMITS-3,                                                             "", 11539,  3074, 0,  0, "Maximum limit for this block (if Block Type is KWH/KW or KWH/KW-Limitsum); 0=no limit"
BLOCK-CHARGE,      0, BLOCK4-TYPE,                                                          "", 12499,  3074, 0,  0, "Type of block calculation; specifies the basis of block charges for this block"
BLOCK-CHARGE,      0, BLOCKS-4,                                       "Size of Block 4, Step ", 11541,  3074, 0,  2, "The step size of the block (same units as the block Type); maximum of ten"
BLOCK-CHARGE,      0, COSTS-4,                                        "Cost of Block 4, Step ", 11540,  3074, 0,  2, "Cost per unit for the energy or demand falling within this block"
BLOCK-CHARGE,      0, LIMITS-4,                                                             "", 11539,  3074, 0,  0, "Maximum limit for this block (if Block Type is KWH/KW or KWH/KW-Limitsum); 0=no limit"
BLOCK-CHARGE,      0, BLOCK5-TYPE,                                                          "", 12499,  3074, 0,  0, "Type of block calculation; specifies the basis of block charges for this block"
BLOCK-CHARGE,      0, BLOCKS-5,                                       "Size of Block 5, Step ", 11541,  3074, 0,  2, "The step size of the block (same units as the block Type); maximum of ten"
BLOCK-CHARGE,      0, COSTS-5,                                        "Cost of Block 5, Step ", 11540,  3074, 0,  2, "Cost per unit for the energy or demand falling within this block"
BLOCK-CHARGE,      0, LIMITS-5,                                                             "", 11539,  3074, 0,  0, "Maximum limit for this block (if Block Type is KWH/KW or KWH/KW-Limitsum); 0=no limit"
RATCHET,           0, NUM-MONTHS,                                                           "", 12502,  3074, 0,  0, "Period over which current ratchet is calculated (1 = current month only)"
RATCHET,           0, RATCHET-SCH,                                                          "", 12727,  3074, 0,  0, "Name of a schedule that defines the period over which the ratchet is calculated"
RATCHET,           0, SCH-FLAG,                                          "Schedule Flag Value", 12728,  3074, 0,  2, "Flag value in the Ratchet Schedule that indicates when this ratchet is active"
RATCHET,           0, TYPE,                                                                 "", 12503,  3074, 0,  0, "Whether demand is based on the highest monthly peak or average monthly peak"
RATCHET,           0, OFFSET,                                                               "", 12265,  3074, 0, 32, "A number added to the demand (demand + Offest is not allowed to fall below zero)"
RATCHET,           0, FRACTION,                                                             "", 12587,  3074, 0, 32, "A number between 0 and 1 that is multiplied against the demand"
WINDOW-LAYER,      0, TYPE,                                                "Window Layer Type", 12322, 32092, 0,  0, "Glass=plastic/transparent mat'l;Gap=air,argon,etc;Blind=slatted shade (e.g. venetian blind)"
WINDOW-LAYER,      0, TRANS-SOL-BB,                                                         "", 12349, 32092, 0,  0, "Fraction of incident beam solar that is transmitted as beam radiation (at normal incidence)"
WINDOW-LAYER,      0, REFL-SOL-BB,                                                          "", 12350, 32092, 0,  0, "Fraction of beam solar incident on front that is reflected as beam (at normal incidence)"
WINDOW-LAYER,      0, BACKREFL-SOL-BB,                                                      "", 12351, 32092, 0,  0, "Fraction of beam solar, incident on back side, that is reflected as beam (at normal incidence)"
WINDOW-LAYER,      0, TRANS-SOL-BH,                                                         "", 12352, 32092, 0,  0, "Fraction of incident beam solar that is reflected as diffuse radiation (at normal incidence)"
WINDOW-LAYER,      0, REFL-SOL-BH,                                                          "", 12353, 32092, 0,  0, "Fraction of beam solar incident on front that is reflected as diffuse (at normal incidence)"
WINDOW-LAYER,      0, BACKREFL-SOL-BH,                                                      "", 12354, 32092, 0,  0, "Fraction of beam solar, incident on back side, that is reflected as diffuse (at normal incidence)"
WINDOW-LAYER,      0, TRANS-SOL-HH,                                                         "", 12355, 32092, 0,  0, "Fraction of incident diffuse solar that is reflected"
WINDOW-LAYER,      0, REFL-SOL-HH,                                                          "", 12356, 32092, 0,  0, "Fraction of diffuse solar incident on front that is reflected"
WINDOW-LAYER,      0, BACKREFL-SOL-HH,                                                      "", 12357, 32092, 0,  0, "Fraction of diffuse solar, incident on back side, that is reflected"
WINDOW-LAYER,      0, TRANS-VIS-BB,                                                         "", 12363, 32092, 0,  0, "Fraction of incident visible beam solar that is transmitted as beam (at normal incidence)"
WINDOW-LAYER,      0, REFL-VIS-BB,                                                          "", 12364, 32092, 0,  0, "Fraction of incident visible beam solar that is reflected as beam (at normal incidence)"
WINDOW-LAYER,      0, BACKREFL-VIS-BB,                                                      "", 12365, 32092, 0,  0, "Fraction of visible beam solar, incident on back side, that is reflected (at normal incidence)"
WINDOW-LAYER,      0, TRANS-VIS-BH,                                                         "", 12366, 32092, 0,  0, "Fraction of incident visible beam solar that is transmitted as diffuse (at normal incidence)"
WINDOW-LAYER,      0, REFL-VIS-BH,                                                          "", 12367, 32092, 0,  0, "Fraction of incident visible beam solar that is reflected as diffuse (at normal incidence)"
WINDOW-LAYER,      0, BACKREFL-VIS-BH,                                                      "", 12368, 32092, 0,  0, "Fraction of visible beam solar, incident on back side, reflected as diffuse (at normal incidence)"
WINDOW-LAYER,      0, TRANS-VIS-HH,                                                         "", 12372, 32092, 0,  0, "Fraction of incident visible diffuse solar that is reflected"
WINDOW-LAYER,      0, REFL-VIS-HH,                                                          "", 12370, 32092, 0,  0, "Fraction of incident visible diffuse solar that is reflected"
WINDOW-LAYER,      0, BACKREFL-VIS-HH,                                                      "", 12371, 32092, 0,  0, "Fraction of visible diffuse solar, incident on back side, that is reflected"
WINDOW-LAYER,      0, TRANS-IR,                                                             "", 12325, 32092, 0,  0, "Fraction of incident infrared radiation that the (glass or blind) layer transmits"
WINDOW-LAYER,      0, EMIS-IR,                                                              "", 12326, 32092, 0,  0, "Hemispherical infrared emissivity of the front (or outside) of a glass or blind layer"
WINDOW-LAYER,      0, BACKEMIS-IR,                                                          "", 12327, 32092, 0,  0, "Hemispherical infrared emissivity of the back (or inside) of a glass or blind layer"
WINDOW-LAYER,      0, SLAT-ORIENTATION,                                                     "", 12328, 32092, 0,  0, "Whether the blinds are oriented in the X or Y plane of the window"
WINDOW-LAYER,      0, SLAT-ANGLE-MIN,                                                       "", 12333, 32092, 0,  0, "Minimum slat angle (for angle-adjustable slats) - limitation of the blind construction or controls"
WINDOW-LAYER,      0, SLAT-ANGLE-MAX,                                                       "", 12334, 32092, 0,  0, "Maximum slat angle (for angle-adjustable slats) - limitation of the blind construction or controls"
WINDOW-LAYER,      0, BLIND-COVER-MIN,                                                      "", 12336, 32092, 0,  0, "Minimum fraction of (glazed) window area covered by movable blinds"
WINDOW-LAYER,      0, BLIND-COVER-MAX,                                                      "", 12337, 32092, 0,  0, "Maximum fraction of (glazed) window area covered by movable blinds"
WINDOW-LAYER,      0, SLAT-WIDTH,                                                           "", 12332, 32092, 0,  0, "Width of the slat (in feet)"
WINDOW-LAYER,      0, SLAT-SEPARATION,                                                      "", 12330, 32092, 0,  0, "Distance between slats (in feet)"
WINDOW-LAYER,      0, THICKNESS,                                                            "", 12323, 32092, 0,  0, "Thickness of the Layer"
WINDOW-LAYER,      0, CONDUCTIVITY,                                                         "", 12324, 32092, 0,  0, "Heat transfer rate through the layer, per degree"
WINDOW-LAYER,      0, D-CONDUCTIVITY,                                                       "", 12341, 32092, 0,  0, "The (constant) change in Conductivity per change in temperature"
WINDOW-LAYER,      0, VISCOSITY,                                                            "", 12342, 32092, 0,  0, "Viscosity of the gas in the gap"
WINDOW-LAYER,      0, D-VISCOSITY,                                                          "", 12343, 32092, 0,  0, "The (constant) change in gas Viscosity per change in temperature"
WINDOW-LAYER,      0, DENSITY,                                                              "", 12344, 32092, 0,  0, "Density of the gas in the gap"
WINDOW-LAYER,      0, D-DENSITY,                                                            "", 12345, 32092, 0,  0, "The (constant) change in gas Density per change in temperature"
WINDOW-LAYER,      0, PRANDTL-NUMB,                                                         "", 12348, 32092, 0,  0, "Prandtl number of the gas in the gap (default is for Argon)"
WINDOW-LAYER,      0, D-PRANDTL-NUMB,                                                       "", 12347, 32092, 0,  0, "The (constant) change in Prandtl Number per change in temperature"
WINDOW-LAYER,      0, SLAT-ANGLE,                                                           "", 12331, 32092, 0,  0, "Angle between slat and window's outward normal (e.g., horizontal slats in vertical window=0)"
WINDOW-LAYER,      0, BLIND-COVER,                                                          "", 12335, 32092, 0,  0, "Fraction of the window area covered by the blind"
END

